Monthly Summary of Monitoring for Surface Water

Treatment Regulations

System: System Number:

Treatment Plant Name: Month: Year:

| Date | Filtered H2O  Temp. (0C) | pH | Filtration Rate (gpm) | Cl2 leaving plant(mg/L) | Cl2 storage tank (mg/L) |
| --- | --- | --- | --- | --- | --- |
| 1 |  |  |  |  |  |
| 2 |  |  |  |  |  |
| 3 |  |  |  |  |  |
| 4 |  |  |  |  |  |
| 5 |  |  |  |  |  |
| 7 |  |  |  |  |  |
| 7 |  |  |  |  |  |
| 8 |  |  |  |  |  |
| 9 |  |  |  |  |  |
| 10 |  |  |  |  |  |
| 11 |  |  |  |  |  |
| 12 |  |  |  |  |  |
| 13 |  |  |  |  |  |
| 14 |  |  |  |  |  |
| 15 |  |  |  |  |  |
| 16 |  |  |  |  |  |
| 17 |  |  |  |  |  |
| 18 |  |  |  |  |  |
| 19 |  |  |  |  |  |
| 20 |  |  |  |  |  |
| 21 |  |  |  |  |  |
| 22 |  |  |  |  |  |
| 23 |  |  |  |  |  |
| 24 |  |  |  |  |  |
| 25 |  |  |  |  |  |
| 26 |  |  |  |  |  |
| 27 |  |  |  |  |  |
| 28 |  |  |  |  |  |
| 29 |  |  |  |  |  |
| 30 |  |  |  |  |  |
| 31 |  |  |  |  |  |

Note: Adequate disinfection will be achieved provided the temperature never drops below 0.5 oC, the pH never increases above 7.0, and flow through the plant never exceeds 100 gpm.

Was **Temperature** ever below 0.5 OC?

Yes

No

Did the **Flow** through the plant ever exceed 100 gpm?

Yes

No

Did pH ever get above 7.0?

Yes

No