# Draft 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 3 - Central Coast Region

Water Body Name: | Zayante Creek
Water Body ID: | CAR3041202220020124155410
Water Body Type: | River & Stream

DECISION ID | 10470
Pollutant: | Ammonia (Unionized)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Zero of 14 samples exceeded the General Objective as it applies to Aquatic Life Beneficial Uses, and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10470

LOE ID: | 9259
Pollutant: | Ammonia (Unionized)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 14 samples exceed the criterion for Ammonia as N, Unionized.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin General Objective, Chapter III, Section II.A.2 (General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries) states that the discharge of wastes shall not cause concentrations of unionized ammonia (NH3) to exceed 0.025 mg/l (as N) in receiving waters (page III-4) .
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/20/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10474
Pollutant: | Boron
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 26 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Zero of 15 samples exceeded the Agricultural Supply water quality objective and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10474

LOE ID: | 9272
Pollutant: | Boron
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Agricultural Supply
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 15 samples exceed the criterion for Boron, dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. In addition, waters used for irrigation and livestock watering shall not exceed concentrations for those chemicals listed in Table 3.4 (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). Table 3-4 (page III-9) lists the maximum concentration for boron for irrigation supply is 0.75 mg/L.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/20/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 12074
Pollutant: | Chlorophyll-a
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. None of the 15 samples exceed the Evaluation Guideline (North Carolina Administrative code, Title 15A) and the General Water Quality Objective set to protect aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 26 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of the 15 samples exceed the Evaluation Guideline (North Carolina Administrative code, Title 15A) and the General Water Quality Objective set to protect aquatic life beneficial uses and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12074

LOE ID: | 9273
Pollutant: | Chlorophyll-a
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 15 samples exceed the criterion for Chlorophyll a.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Evaluation Guideline: | North Carolina Administrative code (NCAC), Title 15A - Environmental and Natural Resources, Subchapter 2B-Surface water and wetland standards, Rule 0211-Fresh surface water quality standards for class C waters (Class C is defined as freshwaters protected for secondary recreation, fishing, aquatic life including propagation and survival, and wildlife). Section 3(a) of Rule 0211 applies to all fresh surface waters and states that chlorophyll a is not to exceed 40 ug/L.
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/20/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 15885
Pollutant: | Diazinon
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. Neither of the 2 samples exceed the Evaluation Guideline (Sipmann and Finlayson, 2000) applied to protect for aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither of the 2 samples exceed the Evaluation Guideline (Sipmann and Finlayson, 2000) applied to protect for aquatic life beneficial uses and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15885

LOE ID: | 16609
Pollutant: | Diazinon
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (04SW3001) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Diazinon.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | One hour average maximum concentration 0.16 ug/L as stated in Sipmann and Finlayson (2000).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/3/2006-5/30/2006. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10477
Pollutant: | Electrical Conductivity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective for Agricultural Supply. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of the 284 samples exceeded the water quality objective for Agricultural Supply, and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10477

LOE ID: | 10231
Pollutant: | Electrical Conductivity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 15 samples exceed the criterion for Conductivity(Us).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when conductivity exceeds 3.0 mS/cm in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/20/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 17424
Pollutant: | Electrical Conductivity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 5
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 5 samples exceed the criterion for Conductivity(Us).
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when conductivity exceeds 3.0 mS/cm in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 2 monitoring sites [ 304-ZAYAN-21 - Zayante Creek, 304-ZAYAN-22 - Zayante Creek at Quail Hollow Rd. Bridge]
Temporal Representation: | Data was collected over the time period 5/1/2004-5/6/2006. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 10268
Pollutant: | Electrical Conductivity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Conductivity(Us).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when conductivity exceeds 3.0 mS/cm in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 8/25/2005-8/26/2005. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 18568
Pollutant: | Electrical Conductivity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 262
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Cruz County Environmental Health Monitoring Program (R3_SCCEH) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 262 samples exceed the criterion for Conductivity(Us).
Data Reference: | Final Data File used for assessment: Santa Cruz County Environmental Health data 1971-1996
| Final Data File used for assessment: Santa Cruz County Environmental Health data 1997-2006
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when conductivity exceeds 3.0 mS/cm in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 3 monitoring sites [ 304ZAC_SCC - ZAYANTE CR. BELOW LOMPICO CR., 304ZAS_SCC - ZAYANTE CR. at SLR, 304ZAZ_SCC - ZAYANTE CR. at ZAYANTE]
Temporal Representation: | Data was collected over the time period 5/15/1990-7/13/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | This monitoring program has been underway for thirty years, with changes over time to protocols, level of QA, and documentation. In general, QA documentation included with the dataset is minimal. However, data quality appears to be reasonably good.
QAPP Information Reference(s):

DECISION ID | 10478
Pollutant: | Escherichia coli (E. Coli)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.3 of the Listing Policy. Under section 3.3 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Four of the 18 samples exceed the Evaluation Guideline (USEPA Ambient Water Quality Criteria for Bacteria, 1986) as it applies to the Water Contact Recreation beneficial use and none of the 18 samples exceed the water quality objective for Non-Contact Recreation. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Four of the 18 samples exceed the Evaluation Guideline (USEPA Ambient Water Quality Criteria for Bacteria, 1986) as it applies to the Water Contact Recreation beneficial use and none of the 18 samples exceed the water quality objective for Non-Contact Recreation. This does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10478

LOE ID: | 18427
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 3
Number of Exceedances: | 0
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 3 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | USEPA Ambient Water Quality Criteria for Bacteria -1986.
Objective/Criterion Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | Single sample maximum allowable density for E. coli in freshwater is 235 MPN/100mL (as stated in Table 4, page 15)
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 2 monitoring sites [ 304-ZAYAN-21 - Zayante Creek, 304-ZAYAN-22 - Zayante Creek at Quail Hollow Rd. Bridge]
Temporal Representation: | Data was collected over the time period 5/1/2004-5/7/2005. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 10232
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 15
Number of Exceedances: | 4
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 4 of 15 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | USEPA Ambient Water Quality Criteria for Bacteria -1986.
Objective/Criterion Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | Single sample maximum allowable density for E. coli in freshwater is 235 MPN/100mL (as stated in Table 4, page 15)
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/20/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 10233
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 15 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml. E. coli is a fecal coliform.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/20/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 18428
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 3
Number of Exceedances: | 0
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 3 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml. E. coli is a fecal coliform.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 2 monitoring sites [ 304-ZAYAN-21 - Zayante Creek, 304-ZAYAN-22 - Zayante Creek at Quail Hollow Rd. Bridge]
Temporal Representation: | Data was collected over the time period 5/1/2004-5/7/2005. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):

DECISION ID | 10483
Pollutant: | Low Dissolved Oxygen
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Three of the 280 samples exceed the Cold Freshwater Habitat water quality objective for Dissolved Oxygen. In addition, 4 of 84 samples exceed the General water quality objective for Oxygen Saturation as it applies to the Cold Freshwater Habitat Beneficial Use. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Three of the 280 samples exceed the Cold Freshwater Habitat water quality objective, and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10483

LOE ID: | 19812
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 258
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Cruz County Environmental Health Monitoring Program (R3_SCCEH) data for Zayante Creek to determine beneficial use support and results are as follows: 3 of 258 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: Santa Cruz County Environmental Health data 1971-1996
| Final Data File used for assessment: Santa Cruz County Environmental Health data 1997-2006
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 3 monitoring sites [ 304ZAC_SCC - ZAYANTE CR. BELOW LOMPICO CR., 304ZAS_SCC - ZAYANTE CR. at SLR, 304ZAZ_SCC - ZAYANTE CR. at ZAYANTE]
Temporal Representation: | Data was collected over the time period 5/15/1990-7/13/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | This monitoring program has been underway for thirty years, with changes over time to protocols, level of QA, and documentation. In general, QA documentation included with the dataset is minimal. However, data quality appears to be reasonably good.
QAPP Information Reference(s):
LOE ID: | 11996
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 8/25/2005-8/26/2005. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11995
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 8/25/2005-8/26/2005. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11976
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 15 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/20/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11975
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 15 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/20/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 18198
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 5
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 5 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 2 monitoring sites [ 304-ZAYAN-21 - Zayante Creek, 304-ZAYAN-22 - Zayante Creek at Quail Hollow Rd. Bridge]
Temporal Representation: | Data was collected over the time period 5/1/2004-5/6/2006. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 19873
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 67
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Cruz County Environmental Health Monitoring Program (R3_SCCEH) data for Zayante Creek to determine beneficial use support and results are as follows: 4 of 67 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: Santa Cruz County Environmental Health data 1971-1996
| Final Data File used for assessment: Santa Cruz County Environmental Health data 1997-2006
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 3 monitoring sites [ 304ZAC_SCC - ZAYANTE CR. BELOW LOMPICO CR., 304ZAS_SCC - ZAYANTE CR. at SLR, 304ZAZ_SCC - ZAYANTE CR. at ZAYANTE]
Temporal Representation: | Data was collected over the time period 1/6/1994-5/27/1998.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | This monitoring program has been underway for thirty years, with changes over time to protocols, level of QA, and documentation. In general, QA documentation included with the dataset is minimal. However, data quality appears to be reasonably good.
QAPP Information Reference(s):

DECISION ID | 10481
Pollutant: | Nitrate
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Six lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the Agricultural Supply or Municipal & Domestic Supply water quality objectives. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of the 282 samples exceed the Agricultural Supply or Municipal & Domestic Supply water quality objectives, and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10481

LOE ID: | 18226
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 3
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 3 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin Objective for municipal and domestic supply uses of inland surface waters (Section II.A.2) states the following: waters shall not contain concentrations of chemical constituents in excess of the limits specified in California Code of Regulations, Title 22, Article 4, Chapter 15, Section 64435, Tables 2 and 3 as listed in Table 3-2. The maximum contaminant level listed in Table 3-2 (inorganic and fluoride concentrations not to be exceeded in domestic or municipal supply) for nitrate is 10.0 mg/L (NO3 as N).
Objective/Criterion Reference: | Title 22, Division 4, Ch. 15, Article 4, Section 64431, Table 64431-A
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 2 monitoring sites [ 304-ZAYAN-21 - Zayante Creek, 304-ZAYAN-22 - Zayante Creek at Quail Hollow Rd. Bridge]
Temporal Representation: | Data was collected over the time period 5/1/2004-5/7/2005. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 18623
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 264
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Cruz County Environmental Health Monitoring Program (R3_SCCEH) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 264 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: Santa Cruz County Environmental Health data 1971-1996
| Final Data File used for assessment: Santa Cruz County Environmental Health data 1997-2006
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when nitrate exceeds 30 mg/L NO3 as N in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 3 monitoring sites [ 304ZAC_SCC - ZAYANTE CR. BELOW LOMPICO CR., 304ZAS_SCC - ZAYANTE CR. at SLR, 304ZAZ_SCC - ZAYANTE CR. at ZAYANTE]
Temporal Representation: | Data was collected over the time period 5/15/1990-7/13/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | This monitoring program has been underway for thirty years, with changes over time to protocols, level of QA, and documentation. In general, QA documentation included with the dataset is minimal. However, data quality appears to be reasonably good.
QAPP Information Reference(s):
LOE ID: | 9275
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 15 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin Objective for municipal and domestic supply uses of inland surface waters (Section II.A.2) states the following: waters shall not contain concentrations of chemical constituents in excess of the limits specified in California Code of Regulations, Title 22, Article 4, Chapter 15, Section 64435, Tables 2 and 3 as listed in Table 3-2. The maximum contaminant level listed in Table 3-2 (inorganic and fluoride concentrations not to be exceeded in domestic or municipal supply) for nitrate is 10.0 mg/L (NO3 as N).
Objective/Criterion Reference: | Title 22, Division 4, Ch. 15, Article 4, Section 64431, Table 64431-A
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/20/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 18225
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 3
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 3 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when nitrate exceeds 30 mg/L NO3 as N in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 2 monitoring sites [ 304-ZAYAN-21 - Zayante Creek, 304-ZAYAN-22 - Zayante Creek at Quail Hollow Rd. Bridge]
Temporal Representation: | Data was collected over the time period 5/1/2004-5/7/2005. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 9274
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 15 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when nitrate exceeds 30 mg/L NO3 as N in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/20/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 18624
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 264
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Cruz County Environmental Health Monitoring Program (R3_SCCEH) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 264 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: Santa Cruz County Environmental Health data 1971-1996
| Final Data File used for assessment: Santa Cruz County Environmental Health data 1997-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin Objective for municipal and domestic supply uses of inland surface waters (Section II.A.2) states the following: waters shall not contain concentrations of chemical constituents in excess of the limits specified in California Code of Regulations, Title 22, Article 4, Chapter 15, Section 64435, Tables 2 and 3 as listed in Table 3-2. The maximum contaminant level listed in Table 3-2 (inorganic and fluoride concentrations not to be exceeded in domestic or municipal supply) for nitrate is 10.0 mg/L (NO3 as N).
Objective/Criterion Reference: | Title 22, Division 4, Ch. 15, Article 4, Section 64431, Table 64431-A
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 3 monitoring sites [ 304ZAC_SCC - ZAYANTE CR. BELOW LOMPICO CR., 304ZAS_SCC - ZAYANTE CR. at SLR, 304ZAZ_SCC - ZAYANTE CR. at ZAYANTE]
Temporal Representation: | Data was collected over the time period 5/15/1990-7/13/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | This monitoring program has been underway for thirty years, with changes over time to protocols, level of QA, and documentation. In general, QA documentation included with the dataset is minimal. However, data quality appears to be reasonably good.
QAPP Information Reference(s):

DECISION ID | 10473
Pollutant: | Nitrogen, ammonia (Total Ammonia)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. One of the samples exceed the Evaluation Guideline (EPA's Lifetime Health advisory level (EPA 2006)) as it applies to the Municipal & Domestic Supply Beneficial Use. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. One of 16 samples exceeded the Evaluation Guideline (EPA's Lifetime Health advisory level (EPA 2006)) as it applies to the Municipal & Domestic Supply Beneficial Use, and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10473

LOE ID: | 9258
Pollutant: | Ammonia as Nitrogen
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 15 samples exceed the criterion for Ammonia as N, Total.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | USEPA Health Advisory 2006 Edition of the Drinking Water Standards and Health Advisories (EPA 822-R-06-013, 2006).
Objective/Criterion Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Evaluation Guideline: | EPA's Lifetime Health advisory level for total ammonia is 30.0 mg/L as stated on page 8 of the 2006 edition of the drinking water standards and health advisories. This Advisory Level is defined as "the concentration of a chemical in drinking water that is not expected to cause any adverse noncarcinogenic effects for up to ten days of exposure."
Guideline Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/20/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 18774
Pollutant: | Ammonia as Nitrogen
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 1
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Cruz County Environmental Health Monitoring Program (R3_SCCEH) data for Zayante Creek to determine beneficial use support and results are as follows: 1 of 1 samples exceed the criterion for Ammonia As N, Total.
Data Reference: | Final Data File used for assessment: Santa Cruz County Environmental Health data 1971-1996
| Final Data File used for assessment: Santa Cruz County Environmental Health data 1997-2006
Water Quality Objective/Criterion: | USEPA Health Advisory 2006 Edition of the Drinking Water Standards and Health Advisories (EPA 822-R-06-013, 2006).
Objective/Criterion Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Evaluation Guideline: | EPA's Lifetime Health advisory level for total ammonia is 30.0 mg/L as stated on page 8 of the 2006 edition of the drinking water standards and health advisories. This Advisory Level is defined as "the concentration of a chemical in drinking water that is not expected to cause any adverse noncarcinogenic effects for up to ten days of exposure."
Guideline Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAC_SCC - ZAYANTE CR. BELOW LOMPICO CR.]
Temporal Representation: | Data was collected on a single day 8/21/1996.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | This monitoring program has been underway for thirty years, with changes over time to protocols, level of QA, and documentation. In general, QA documentation included with the dataset is minimal. However, data quality appears to be reasonably good.
QAPP Information Reference(s):

DECISION ID | 10485
Pollutant: | Temperature, water
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. None of the 284 samples exceed the Evaluation Guideline (Moyle 1976) as it applies to the Cold Freshwater Habitat water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of the 284 samples exceed the Evaluation Guideline (Moyle 1976) as it applies to the Cold Freshwater Habitat water quality objective, and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10485

LOE ID: | 11993
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 15 samples exceed the criterion for Water Temperature.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Board that such alteration in temperature does not adversely affect beneficial uses (General Objective in Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Inland Fishes of California (Moyle 1976) states that for rainbow trout the optimum range for growth and completion of most life stages is 13-21 degrees C (page 129).
Guideline Reference: | Inland Fishes of California
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/20/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 12010
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Water Temperature.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Board that such alteration in temperature does not adversely affect beneficial uses (General Objective in Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Inland Fishes of California (Moyle 1976) states that for rainbow trout the optimum range for growth and completion of most life stages is 13-21 degrees C (page 129).
Guideline Reference: | Inland Fishes of California
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 8/25/2005-8/26/2005. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 18769
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 5
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 5 samples exceed the criterion for Water Temperature.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | Natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Board that such alteration in temperature does not adversely affect beneficial uses (General Objective in Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Inland Fishes of California (Moyle 1976) states that for rainbow trout the optimum range for growth and completion of most life stages is 13-21 degrees C (page 129).
Guideline Reference: | Inland Fishes of California
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 2 monitoring sites [ 304-ZAYAN-21 - Zayante Creek, 304-ZAYAN-22 - Zayante Creek at Quail Hollow Rd. Bridge]
Temporal Representation: | Data was collected over the time period 5/1/2004-5/6/2006. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 19878
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 262
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Cruz County Environmental Health Monitoring Program (R3_SCCEH) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 262 samples exceed the criterion for Water Temperature.
Data Reference: | Final Data File used for assessment: Santa Cruz County Environmental Health data 1971-1996
| Final Data File used for assessment: Santa Cruz County Environmental Health data 1997-2006
Water Quality Objective/Criterion: | Natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Board that such alteration in temperature does not adversely affect beneficial uses (General Objective in Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Inland Fishes of California (Moyle 1976) states that for rainbow trout the optimum range for growth and completion of most life stages is 13-21 degrees C (page 129).
Guideline Reference: | Inland Fishes of California
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 3 monitoring sites [ 304ZAC_SCC - ZAYANTE CR. BELOW LOMPICO CR., 304ZAS_SCC - ZAYANTE CR. at SLR, 304ZAZ_SCC - ZAYANTE CR. at ZAYANTE]
Temporal Representation: | Data was collected over the time period 3/11/1992-7/13/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | This monitoring program has been underway for thirty years, with changes over time to protocols, level of QA, and documentation. In general, QA documentation included with the dataset is minimal. However, data quality appears to be reasonably good.
QAPP Information Reference(s):

DECISION ID | 12075
Pollutant: | Turbidity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Three lines of evidence are available in the administrative record to assess this pollutant. Five out of 222 samples exceed the Evaluation Guideline (Sigler et al., 1984) applied to protect for aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Five out of 222 samples exceed the Evaluation Guideline (Sigler et al., 1984) applied to protect for aquatic life beneficial uses and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12075

LOE ID: | 11994
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 9
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 2 of 9 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 2/16/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 18724
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 4
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 4 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 2 monitoring sites [ 304-ZAYAN-21 - Zayante Creek, 304-ZAYAN-22 - Zayante Creek at Quail Hollow Rd. Bridge]
Temporal Representation: | Data was collected over the time period 5/7/2005-5/6/2006. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 19648
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 209
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Cruz County Environmental Health Monitoring Program (R3_SCCEH) data for Zayante Creek to determine beneficial use support and results are as follows: 3 of 209 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: Santa Cruz County Environmental Health data 1971-1996
| Final Data File used for assessment: Santa Cruz County Environmental Health data 1997-2006
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 3 monitoring sites [ 304ZAC_SCC - ZAYANTE CR. BELOW LOMPICO CR., 304ZAS_SCC - ZAYANTE CR. at SLR, 304ZAZ_SCC - ZAYANTE CR. at ZAYANTE]
Temporal Representation: | Data was collected over the time period 5/15/1990-7/13/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | This monitoring program has been underway for thirty years, with changes over time to protocols, level of QA, and documentation. In general, QA documentation included with the dataset is minimal. However, data quality appears to be reasonably good.
QAPP Information Reference(s):

DECISION ID | 12077
Pollutant: | Unknown Toxicity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 and section 3.6 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Three lines of evidence are available in the administrative record to assess this pollutant in water samples. None of the samples were toxic to test organisms (exhibited a significant increase in mortality or decrease in cell density compared to the laboratory control) and therefore did not exceed the General water quality objective for toxicity, set to protect for aquatic life beneficial uses. The following is a summary of the results from individual toxicity tests. Neither of the 2 samples (tested for toxicity to plants) exhibited significant reduction in cell density relative to the control. In addition, Neither of the 2 samples (tested for toxicity to vertebrate test organisms) exhibited a significant increase in mortality compared to the laboratory control. Lastly, Neither of the 2 samples, tested for toxicity to invertebrate test organisms exhibited a significant increase in mortality compared to the laboratory control. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of the toxicity tests exceed the General water quality objective for toxicity, set to protect aquatic life beneficial uses and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12077

LOE ID: | 24721
Pollutant: | Invertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (04SW3001) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Toxicity, Ceriodaphnia dubia Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/3/2006-5/30/2006. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 24726
Pollutant: | Vertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (04SW3001) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Toxicity, Pimephales promelas Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/3/2006-5/30/2006. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 24727
Pollutant: | Plant Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (04SW3001) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Toxicity, Selenastrum capricornutum Growth (Cell Density) 4 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction in cell count of test organism relative to the control (alpha < 0.05) and cell count <80% of control.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/3/2006-5/30/2006. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10486
Pollutant: | pH
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Twenty lines of evidence are available in the administrative record to assess this pollutant. Seven of 288 samples exceed the Agricultural Supply water quality objective, 8 of 288 samples exceed the Cold Freshwater Habitat water quality objective and 13 of 288 samples exceed the numeric objective for Municipal & Domestic Supply, Non-contact Recreation and Water Contact Recreation. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Seven of 288 samples exceed the Agricultural Supply water quality objective, 8 of 288 samples exceed the Cold Freshwater Habitat water quality objective and 13 of 288 samples exceed the numeric objective for Municipal & Domestic Supply, Non-contact Recreation and Water Contact Recreation. None of these exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10486

LOE ID: | 19163
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 5
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 5 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 2 monitoring sites [ 304-ZAYAN-21 - Zayante Creek, 304-ZAYAN-22 - Zayante Creek at Quail Hollow Rd. Bridge]
Temporal Representation: | Data was collected over the time period 5/1/2004-5/6/2006. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 19145
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 5
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Zayante Creek to determine beneficial use support and results are as follows: 1 of 5 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 2 monitoring sites [ 304-ZAYAN-21 - Zayante Creek, 304-ZAYAN-22 - Zayante Creek at Quail Hollow Rd. Bridge]
Temporal Representation: | Data was collected over the time period 5/1/2004-5/6/2006. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 19146
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 5
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 5 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin, Section II.A.2. Municipal and Domestic Supply Objectives, Section II.A.2.a states the following: The pH value shall neither be depressed below 6.5 or raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 2 monitoring sites [ 304-ZAYAN-21 - Zayante Creek, 304-ZAYAN-22 - Zayante Creek at Quail Hollow Rd. Bridge]
Temporal Representation: | Data was collected over the time period 5/1/2004-5/6/2006. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 19147
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 5
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 5 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 2 monitoring sites [ 304-ZAYAN-21 - Zayante Creek, 304-ZAYAN-22 - Zayante Creek at Quail Hollow Rd. Bridge]
Temporal Representation: | Data was collected over the time period 5/1/2004-5/6/2006. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 10271
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin, Section II.A.2. Municipal and Domestic Supply Objectives, Section II.A.2.a states the following: The pH value shall neither be depressed below 6.5 or raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 8/25/2005-8/26/2005. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 10272
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 8/25/2005-8/26/2005. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 19144
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 5
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 5 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when pH is greater than 8.4 or less than 6.5 in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 2 monitoring sites [ 304-ZAYAN-21 - Zayante Creek, 304-ZAYAN-22 - Zayante Creek at Quail Hollow Rd. Bridge]
Temporal Representation: | Data was collected over the time period 5/1/2004-5/6/2006. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 19678
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 267
Number of Exceedances: | 7
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Cruz County Environmental Health Monitoring Program (R3_SCCEH) data for Zayante Creek to determine beneficial use support and results are as follows: 7 of 267 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Santa Cruz County Environmental Health data 1971-1996
| Final Data File used for assessment: Santa Cruz County Environmental Health data 1997-2006
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 3 monitoring sites [ 304ZAC_SCC - ZAYANTE CR. BELOW LOMPICO CR., 304ZAS_SCC - ZAYANTE CR. at SLR, 304ZAZ_SCC - ZAYANTE CR. at ZAYANTE]
Temporal Representation: | Data was collected over the time period 5/15/1990-7/13/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | This monitoring program has been underway for thirty years, with changes over time to protocols, level of QA, and documentation. In general, QA documentation included with the dataset is minimal. However, data quality appears to be reasonably good.
QAPP Information Reference(s):
LOE ID: | 10250
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 14 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin, Section II.A.2. Municipal and Domestic Supply Objectives, Section II.A.2.a states the following: The pH value shall neither be depressed below 6.5 or raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/20/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 10251
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 14 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/20/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 10252
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 14 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/20/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 19677
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 267
Number of Exceedances: | 7
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Cruz County Environmental Health Monitoring Program (R3_SCCEH) data for Zayante Creek to determine beneficial use support and results are as follows: 7 of 267 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Santa Cruz County Environmental Health data 1971-1996
| Final Data File used for assessment: Santa Cruz County Environmental Health data 1997-2006
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when pH is greater than 8.4 or less than 6.5 in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 3 monitoring sites [ 304ZAC_SCC - ZAYANTE CR. BELOW LOMPICO CR., 304ZAS_SCC - ZAYANTE CR. at SLR, 304ZAZ_SCC - ZAYANTE CR. at ZAYANTE]
Temporal Representation: | Data was collected over the time period 5/15/1990-7/13/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | This monitoring program has been underway for thirty years, with changes over time to protocols, level of QA, and documentation. In general, QA documentation included with the dataset is minimal. However, data quality appears to be reasonably good.
QAPP Information Reference(s):
LOE ID: | 19681
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 267
Number of Exceedances: | 13
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Cruz County Environmental Health Monitoring Program (R3_SCCEH) data for Zayante Creek to determine beneficial use support and results are as follows: 13 of 267 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Santa Cruz County Environmental Health data 1971-1996
| Final Data File used for assessment: Santa Cruz County Environmental Health data 1997-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 3 monitoring sites [ 304ZAC_SCC - ZAYANTE CR. BELOW LOMPICO CR., 304ZAS_SCC - ZAYANTE CR. at SLR, 304ZAZ_SCC - ZAYANTE CR. at ZAYANTE]
Temporal Representation: | Data was collected over the time period 5/15/1990-7/13/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | This monitoring program has been underway for thirty years, with changes over time to protocols, level of QA, and documentation. In general, QA documentation included with the dataset is minimal. However, data quality appears to be reasonably good.
QAPP Information Reference(s):
LOE ID: | 19680
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 267
Number of Exceedances: | 13
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Cruz County Environmental Health Monitoring Program (R3_SCCEH) data for Zayante Creek to determine beneficial use support and results are as follows: 13 of 267 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Santa Cruz County Environmental Health data 1971-1996
| Final Data File used for assessment: Santa Cruz County Environmental Health data 1997-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 3 monitoring sites [ 304ZAC_SCC - ZAYANTE CR. BELOW LOMPICO CR., 304ZAS_SCC - ZAYANTE CR. at SLR, 304ZAZ_SCC - ZAYANTE CR. at ZAYANTE]
Temporal Representation: | Data was collected over the time period 5/15/1990-7/13/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | This monitoring program has been underway for thirty years, with changes over time to protocols, level of QA, and documentation. In general, QA documentation included with the dataset is minimal. However, data quality appears to be reasonably good.
QAPP Information Reference(s):
LOE ID: | 10248
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 14 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when pH is greater than 8.4 or less than 6.5 in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/20/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 10249
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 14 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/20/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 10270
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 8/25/2005-8/26/2005. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 10288
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 8/25/2005-8/26/2005. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 19679
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 267
Number of Exceedances: | 13
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Cruz County Environmental Health Monitoring Program (R3_SCCEH) data for Zayante Creek to determine beneficial use support and results are as follows: 13 of 267 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Santa Cruz County Environmental Health data 1971-1996
| Final Data File used for assessment: Santa Cruz County Environmental Health data 1997-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin, Section II.A.2. Municipal and Domestic Supply Objectives, Section II.A.2.a states the following: The pH value shall neither be depressed below 6.5 or raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 3 monitoring sites [ 304ZAC_SCC - ZAYANTE CR. BELOW LOMPICO CR., 304ZAS_SCC - ZAYANTE CR. at SLR, 304ZAZ_SCC - ZAYANTE CR. at ZAYANTE]
Temporal Representation: | Data was collected over the time period 5/15/1990-7/13/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | This monitoring program has been underway for thirty years, with changes over time to protocols, level of QA, and documentation. In general, QA documentation included with the dataset is minimal. However, data quality appears to be reasonably good.
QAPP Information Reference(s):
LOE ID: | 10269
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when pH is greater than 8.4 or less than 6.5 in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 8/25/2005-8/26/2005. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 15884
Pollutant: | Chlorpyrifos
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.1 of the Listing Policy. One line of evidence is available in the administrative record to assess this pollutant. Based on section 3.1 the site exceeded numeric objectives for toxic pollutants. Using the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.1. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Both of 2 samples exceeded the Evaluation Guideline (Sipmann and Finlayson, 2000) applied to protect for aquatic life beneficial uses and this exceeds the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15884

LOE ID: | 16175
Pollutant: | Chlorpyrifos
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (04SW3001) data for Zayante Creek to determine beneficial use support and results are as follows: 2 of 2 samples exceed the criterion for Chlorpyrifos.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
| Final Data File used for assessment: SWAMP Sediment Chemistry Data from Region 3 Harbors, 2004
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | One hour average maximum concentration 0.025 ug/L as stated in Sipmann and Finlayson (2000).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/3/2006-5/30/2006. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10479
Pollutant: | Fecal Coliform
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.3 of the Listing Policy. Two lines of evidence are available in the administrative record to assess this pollutant. Seven of 15 samples exceed the Water Contact Recreation water quality objective but none of the 15 samples exceed the Non-contact Recreation water quality objective. Based on section 3.3 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Seven of 15 samples exceed the Water Contact Recreation water quality objective and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10479

LOE ID: | 10230
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 0 of 15 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/20/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 10229
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 15
Number of Exceedances: | 7
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Zayante Creek to determine beneficial use support and results are as follows: 7 of 15 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 200 MPN/100 ml, nor shall more than ten percent of total samples during any 30-day period exceed 400 MPN/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Zayante Creek was collected at 1 monitoring site [ 304ZAY-Zayante Creek at Graham Hill Road]
Temporal Representation: | Data was collected over the time period 1/20/2005-3/8/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 6935
Pollutant: | Sedimentation/Siltation
Final Listing Decision: | List on 303(d) list (being addressed by USEPA approved TMDL)
Last Listing Cycle's Final Listing Decision: | List on 303(d) list (TMDL required list)(2006)
Revision Status | Original
Sources: | Agriculture | Disturbed Sites (Land Develop.) | Erosion/Siltation | Nonpoint Source | Road Construction | Silviculture
TMDL Name: | San Lorenzo River Sediment
TMDL Project Code: | 243
Date TMDL Approved by USEPA: | 02/19/2004
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | 303(d) listing decisions made prior to 2006 were not held in an assessment database. The Regional Boards will update this decision when new data and information become available and are assessed.
RWQCB Board Decision / Staff Recommendation: | No new data were assessed for 2008. The decision has not changed.
SWRCB Board Decision / Staff Recommendation: | N/A
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 6935

LOE ID: | 4022
Pollutant: | Sedimentation/Siltation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Not Recorded
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 0
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Unspecified--This LOE is a placeholder to support a 303(d) listing decision made prior to 2006.
Data Reference: | Placeholder reference pre-2006 303(d)
Water Quality Objective/Criterion: | Unspecified
Objective/Criterion Reference: | Placeholder reference pre-2006 303(d)
Evaluation Guideline: | Unspecified
Guideline Reference: | Placeholder reference pre-2006 303(d)
Spatial Representation: | Unspecified
Temporal Representation: | Unspecified
Environmental Conditions: | Unspecified
QAPP Information: | Unspecified
QAPP Information Reference(s):