# Draft 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 3 - Central Coast Region

Water Body Name: | Atascadero Creek (Santa Barbara county)
Water Body ID: | CAR3153101119990222145750
Water Body Type: | River & Stream

DECISION ID | 10818
Pollutant: | Ammonia (Unionized)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. None of the 72 samples exceed the water quality objective for Cold and Warm Freshwater Habitat. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of the 72 samples exceed the water quality objective for Cold and Warm Freshwater Habitat. This does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10818

LOE ID: | 9809
Pollutant: | Ammonia (Unionized)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 59
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 59 samples exceed the criterion for Ammonia as N, Unionized.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin General Objective, Chapter III, Section II.A.2 (General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries) states that the discharge of wastes shall not cause concentrations of unionized ammonia (NH3) to exceed 0.025 mg/l (as N) in receiving waters (page III-4) .
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 9854
Pollutant: | Ammonia (Unionized)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 13 samples exceed the criterion for Ammonia as N, Unionized.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin General Objective, Chapter III, Section II.A.2 (General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries) states that the discharge of wastes shall not cause concentrations of unionized ammonia (NH3) to exceed 0.025 mg/l (as N) in receiving waters (page III-4) .
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 9821
Pollutant: | Ammonia (Unionized)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 59
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 59 samples exceed the criterion for Ammonia as N, Unionized.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin General Objective, Chapter III, Section II.A.2 (General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries) states that the discharge of wastes shall not cause concentrations of unionized ammonia (NH3) to exceed 0.025 mg/l (as N) in receiving waters (page III-4) .
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 9855
Pollutant: | Ammonia (Unionized)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 13 samples exceed the criterion for Ammonia as N, Unionized.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin General Objective, Chapter III, Section II.A.2 (General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries) states that the discharge of wastes shall not cause concentrations of unionized ammonia (NH3) to exceed 0.025 mg/l (as N) in receiving waters (page III-4) .
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 15502
Pollutant: | Anthracene
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15502

LOE ID: | 15684
Pollutant: | Anthracene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Anthracene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for anthracene is 845 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14815
Pollutant: | Anthracene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Anthracene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for anthracene is 845 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15768
Pollutant: | Anthracene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Anthracene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for anthracene is 845 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15683
Pollutant: | Anthracene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Anthracene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for anthracene is 845 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10822
Pollutant: | Arsenic
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Neither of the two samples exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to Cold and Warm Freshwater Habitat objectives. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither of the two samples exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to Cold and Warm Freshwater Habitat objectives and therefore this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10822

LOE ID: | 15852
Pollutant: | Arsenic
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Arsenic.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for arsenic is 33 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15770
Pollutant: | Arsenic
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Arsenic.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for arsenic is 33 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15756
Pollutant: | Arsenic
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Arsenic.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for arsenic is 33 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15853
Pollutant: | Arsenic
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Arsenic.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for arsenic is 33 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 15503
Pollutant: | Benzo(a)pyrene (3,4-Benzopyrene -7-d)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15503

LOE ID: | 15451
Pollutant: | Benzo(a)pyrene (3,4-Benzopyrene -7-d)
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Benzo(a)pyrene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Benzo(a)Pyrene is 1450 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15438
Pollutant: | Benzo(a)pyrene (3,4-Benzopyrene -7-d)
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Benzo(a)pyrene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Benzo(a)Pyrene is 1450 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15534
Pollutant: | Benzo(a)pyrene (3,4-Benzopyrene -7-d)
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Benzo(a)pyrene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Benzo(a)Pyrene is 1450 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15533
Pollutant: | Benzo(a)pyrene (3,4-Benzopyrene -7-d)
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Benzo(a)pyrene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Benzo(a)Pyrene is 1450 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 15504
Pollutant: | Benzo[a]anthracene
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15504

LOE ID: | 15825
Pollutant: | Benzo[a]anthracene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Benzo(a)anthracene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Benzo(a)anthracene is 1050 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15664
Pollutant: | Benzo[a]anthracene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Benzo(a)anthracene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Benzo(a)anthracene is 1050 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15824
Pollutant: | Benzo[a]anthracene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Benzo(a)anthracene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Benzo(a)anthracene is 1050 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15665
Pollutant: | Benzo[a]anthracene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Benzo(a)anthracene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Benzo(a)anthracene is 1050 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10823
Pollutant: | Boron
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. Two of 68 samples exceed the water quality objective for Agricultural Supply. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Two of 68 samples exceed the water quality objective for Agricultural Supply. and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10823

LOE ID: | 9822
Pollutant: | Boron
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Agricultural Supply
Number of Samples: | 53
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 2 of 53 samples exceed the criterion for Boron, dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. In addition, waters used for irrigation and livestock watering shall not exceed concentrations for those chemicals listed in Table 3.4 (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). Table 3-4 (page III-9) lists the maximum concentration for boron for irrigation supply is 0.75 mg/L.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 9856
Pollutant: | Boron
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Agricultural Supply
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 15 samples exceed the criterion for Boron, dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. In addition, waters used for irrigation and livestock watering shall not exceed concentrations for those chemicals listed in Table 3.4 (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). Table 3-4 (page III-9) lists the maximum concentration for boron for irrigation supply is 0.75 mg/L.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/27/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10824
Pollutant: | Cadmium
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. Neither of the 2 samples exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither of the 2 samples exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life beneficial uses. The sample size is insufficient to determine with the power and confidence of the Listing Policy if water quality standards are being met. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10824

LOE ID: | 15552
Pollutant: | Cadmium
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Cadmium.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for cadmium is 4.98 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15395
Pollutant: | Cadmium
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Cadmium.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for cadmium is 4.98 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15551
Pollutant: | Cadmium
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Cadmium.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for cadmium is 4.98 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15382
Pollutant: | Cadmium
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Cadmium.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for cadmium is 4.98 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 15515
Pollutant: | Chlorophyll-a
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. None of the 71 samples exceed the Evaluation Guideline (North Carolina Administrative code, Title 15A) and the General Water Quality Objective set to protect aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of the 71 samples exceed the Evaluation Guideline (North Carolina Administrative code, Title 15A) and the General Water Quality Objective set to protect aquatic life beneficial uses and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15515

LOE ID: | 9621
Pollutant: | Chlorophyll-a
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 12
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 12 samples exceed the criterion for Chlorophyll a.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Evaluation Guideline: | North Carolina Administrative code (NCAC), Title 15A - Environmental and Natural Resources, Subchapter 2B-Surface water and wetland standards, Rule 0211-Fresh surface water quality standards for class C waters (Class C is defined as freshwaters protected for secondary recreation, fishing, aquatic life including propagation and survival, and wildlife). Section 3(a) of Rule 0211 applies to all fresh surface waters and states that chlorophyll a is not to exceed 40 ug/L.
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 9839
Pollutant: | Chlorophyll-a
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 59
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 59 samples exceed the criterion for Chlorophyll a.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Evaluation Guideline: | North Carolina Administrative code (NCAC), Title 15A - Environmental and Natural Resources, Subchapter 2B-Surface water and wetland standards, Rule 0211-Fresh surface water quality standards for class C waters (Class C is defined as freshwaters protected for secondary recreation, fishing, aquatic life including propagation and survival, and wildlife). Section 3(a) of Rule 0211 applies to all fresh surface waters and states that chlorophyll a is not to exceed 40 ug/L.
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 9838
Pollutant: | Chlorophyll-a
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 59
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 59 samples exceed the criterion for Chlorophyll a.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Evaluation Guideline: | North Carolina Administrative code (NCAC), Title 15A - Environmental and Natural Resources, Subchapter 2B-Surface water and wetland standards, Rule 0211-Fresh surface water quality standards for class C waters (Class C is defined as freshwaters protected for secondary recreation, fishing, aquatic life including propagation and survival, and wildlife). Section 3(a) of Rule 0211 applies to all fresh surface waters and states that chlorophyll a is not to exceed 40 ug/L.
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 9622
Pollutant: | Chlorophyll-a
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 12
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 12 samples exceed the criterion for Chlorophyll a.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Evaluation Guideline: | North Carolina Administrative code (NCAC), Title 15A - Environmental and Natural Resources, Subchapter 2B-Surface water and wetland standards, Rule 0211-Fresh surface water quality standards for class C waters (Class C is defined as freshwaters protected for secondary recreation, fishing, aquatic life including propagation and survival, and wildlife). Section 3(a) of Rule 0211 applies to all fresh surface waters and states that chlorophyll a is not to exceed 40 ug/L.
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 15517
Pollutant: | Chlorpyrifos
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. One of the 5 samples exceed the Evaluation Guideline (Sipmann and Finlayson, 2000) applied to protect for aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. One of the 5 samples exceed the Evaluation Guideline (Sipmann and Finlayson, 2000) applied to protect for aquatic life beneficial uses and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15517

LOE ID: | 16005
Pollutant: | Chlorpyrifos
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 1 of 1 samples exceed the criterion for Chlorpyrifos.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
| Final Data File used for assessment: SWAMP Sediment Chemistry Data from Region 3 Harbors, 2004
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | One hour average maximum concentration 0.025 ug/L as stated in Sipmann and Finlayson (2000).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16327
Pollutant: | Chlorpyrifos
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 4
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 4 samples exceed the criterion for Chlorpyrifos.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
| Final Data File used for assessment: SWAMP Sediment Chemistry Data from Region 3 Harbors, 2004
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | One hour average maximum concentration 0.025 ug/L as stated in Sipmann and Finlayson (2000).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 12/5/2001-3/27/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16326
Pollutant: | Chlorpyrifos
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 4
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 4 samples exceed the criterion for Chlorpyrifos.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
| Final Data File used for assessment: SWAMP Sediment Chemistry Data from Region 3 Harbors, 2004
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | One hour average maximum concentration 0.025 ug/L as stated in Sipmann and Finlayson (2000).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 12/5/2001-3/27/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16004
Pollutant: | Chlorpyrifos
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 1 of 1 samples exceed the criterion for Chlorpyrifos.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
| Final Data File used for assessment: SWAMP Sediment Chemistry Data from Region 3 Harbors, 2004
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | One hour average maximum concentration 0.025 ug/L as stated in Sipmann and Finlayson (2000).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10849
Pollutant: | Chromium (total)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence is available in the administrative record to assess this pollutant. Neither of the two samples exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither of the two samples exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life beneficial uses and therefore this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10849

LOE ID: | 15994
Pollutant: | Chromium (total)
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Chromium.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for chromium is 111 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16088
Pollutant: | Chromium (total)
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Chromium.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for chromium is 111 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16089
Pollutant: | Chromium (total)
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Chromium.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for chromium is 111 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15993
Pollutant: | Chromium (total)
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Chromium.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for chromium is 111 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 15505
Pollutant: | Chrysene (C1-C4)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15505

LOE ID: | 15922
Pollutant: | Chrysene (C1-C4)
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Chrysene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Chrysene is 1290 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16078
Pollutant: | Chrysene (C1-C4)
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Chrysene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Chrysene is 1290 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16079
Pollutant: | Chrysene (C1-C4)
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Chrysene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Chrysene is 1290 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15921
Pollutant: | Chrysene (C1-C4)
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Chrysene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Chrysene is 1290 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10851
Pollutant: | Copper
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence is available in the administrative record to assess this pollutant. Neither sample exceeded the Evaluation Guideline (MacDonald et al. 2000) as it applies to the General Objective. Based on the readily available data and information, the weight of evidence indicates that there is insufficient justification for placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. There are also an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither sample exceeds the Evaluation Guideline (MacDonald et al. 2000) as it applies to the General Objective, and did not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10851

LOE ID: | 16748
Pollutant: | Copper
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Copper.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for cooper is 149 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15908
Pollutant: | Copper
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Copper.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for cooper is 149 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16747
Pollutant: | Copper
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Copper.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for cooper is 149 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15895
Pollutant: | Copper
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Copper.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for cooper is 149 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 15518
Pollutant: | Diazinon
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. None of the 5 samples exceed the Evaluation Guideline (Sipmann and Finlayson, 2000) applied to protect for aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of the 5 samples exceed the Evaluation Guideline (Sipmann and Finlayson, 2000) applied to protect for aquatic life beneficial uses and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15518

LOE ID: | 16751
Pollutant: | Diazinon
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 4
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 4 samples exceed the criterion for Diazinon.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
| Final Data File used for assessment: SWAMP Sediment Chemistry Data from Region 3 Harbors, 2004
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | One hour average maximum concentration 0.16 ug/L as stated in Sipmann and Finlayson (2000).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 12/5/2001-3/27/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16750
Pollutant: | Diazinon
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 4
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 4 samples exceed the criterion for Diazinon.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
| Final Data File used for assessment: SWAMP Sediment Chemistry Data from Region 3 Harbors, 2004
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | One hour average maximum concentration 0.16 ug/L as stated in Sipmann and Finlayson (2000).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 12/5/2001-3/27/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16643
Pollutant: | Diazinon
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Diazinon.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
| Final Data File used for assessment: SWAMP Sediment Chemistry Data from Region 3 Harbors, 2004
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | One hour average maximum concentration 0.16 ug/L as stated in Sipmann and Finlayson (2000).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16644
Pollutant: | Diazinon
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Diazinon.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
| Final Data File used for assessment: SWAMP Sediment Chemistry Data from Region 3 Harbors, 2004
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | One hour average maximum concentration 0.16 ug/L as stated in Sipmann and Finlayson (2000).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 15506
Pollutant: | Dieldrin
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15506

LOE ID: | 16679
Pollutant: | Dieldrin
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Dieldrin.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for dieldrin is 61.8 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16680
Pollutant: | Dieldrin
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Dieldrin.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for dieldrin is 61.8 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16614
Pollutant: | Dieldrin
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Dieldrin.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for dieldrin is 61.8 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16615
Pollutant: | Dieldrin
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Dieldrin.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for dieldrin is 61.8 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10853
Pollutant: | Electrical Conductivity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Twenty-two out of 229 samples exceed the water quality objective for Agricultural Supply. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Twenty-two out of 229 samples exceed the water quality objective for Agricultural Supply and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10853

LOE ID: | 11532
Pollutant: | Electrical Conductivity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 12
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 12 samples exceed the criterion for Conductivity(Us).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when conductivity exceeds 3.0 mS/cm in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11511
Pollutant: | Electrical Conductivity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 6
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 1 of 6 samples exceed the criterion for Conductivity(Us).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when conductivity exceeds 3.0 mS/cm in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 7/16/2001-9/26/2001. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15067
Pollutant: | Electrical Conductivity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 152
Number of Exceedances: | 15
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 15 of 152 samples exceed the criterion for Conductivity(Us).
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when conductivity exceeds 3.0 mS/cm in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT1 - Atascadero Creek at Ward Drive, AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive]
Temporal Representation: | Data was collected over the time period 6/2/2002-1/7/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis
LOE ID: | 11477
Pollutant: | Electrical Conductivity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 59
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 6 of 59 samples exceed the criterion for Conductivity(Us).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when conductivity exceeds 3.0 mS/cm in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 15507
Pollutant: | Endrin
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15507

LOE ID: | 16436
Pollutant: | Endrin
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Endrin.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for endrin is 207 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16435
Pollutant: | Endrin
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Endrin.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for endrin is 207 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16842
Pollutant: | Endrin
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Endrin.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for endrin is 207 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16530
Pollutant: | Endrin
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Endrin.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for endrin is 207 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 15508
Pollutant: | Fluoranthene
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15508

LOE ID: | 16533
Pollutant: | Fluoranthene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Fluoranthene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Fluoranthene is 2,230 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16520
Pollutant: | Fluoranthene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Fluoranthene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Fluoranthene is 2,230 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16362
Pollutant: | Fluoranthene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Fluoranthene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Fluoranthene is 2,230 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16361
Pollutant: | Fluoranthene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Fluoranthene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Fluoranthene is 2,230 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 15509
Pollutant: | Fluorene
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15509

LOE ID: | 16478
Pollutant: | Fluorene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Fluorene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for fluorene is 536 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16477
Pollutant: | Fluorene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Fluorene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for fluorene is 536 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16398
Pollutant: | Fluorene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Fluorene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for fluorene is 536 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16397
Pollutant: | Fluorene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Fluorene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for fluorene is 536 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10857
Pollutant: | Lead
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Neither sample exceeds the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither sample exceeds the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life beneficial uses. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10857

LOE ID: | 17327
Pollutant: | Lead
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Lead.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for lead is 128 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 17328
Pollutant: | Lead
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Lead.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for lead is 128 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 17233
Pollutant: | Lead
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Lead.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for lead is 128 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 17232
Pollutant: | Lead
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Lead.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for lead is 128 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10858
Pollutant: | Mercury
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Neither of the two samples exceeded the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither of the two samples exceeded the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life beneficial uses, but this did not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10858

LOE ID: | 17129
Pollutant: | Mercury
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Mercury.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for mercury is 1.06 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16538
Pollutant: | Mercury
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Mercury.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for mercury is 1.06 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16537
Pollutant: | Mercury
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Mercury.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for mercury is 1.06 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 17142
Pollutant: | Mercury
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Mercury.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for mercury is 1.06 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 15510
Pollutant: | Naphthalene
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15510

LOE ID: | 17131
Pollutant: | Naphthalene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Naphthalene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for naphthalene is 561 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 17132
Pollutant: | Naphthalene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Naphthalene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for naphthalene is 561 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 17195
Pollutant: | Naphthalene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Naphthalene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for naphthalene is 561 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 17194
Pollutant: | Naphthalene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Naphthalene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for naphthalene is 561 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10859
Pollutant: | Nickel
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Neither sample exceeds the Evaluation Guideline (MacDonald et al. 2000) as it applies to Cold and Warm Freshwater Habitat beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither sample exceeded the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life beneficial uses. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10859

LOE ID: | 17047
Pollutant: | Nickel
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Nickel.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for nickel is 48.6 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16953
Pollutant: | Nickel
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Nickel.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for nickel is 48.6 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 17048
Pollutant: | Nickel
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Nickel.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for nickel is 48.6 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16952
Pollutant: | Nickel
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Nickel.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for nickel is 48.6 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10860
Pollutant: | Nitrate
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Six lines of evidence are available in the administrative record to assess this pollutant. Two of the 267 samples exceed the water quality objective for Municipal and Domestic Supply, and none of the 267 samples exceed the water quality objective for Agricultural Supply. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Two of the 267 samples exceed the water quality objective for Municipal and Domestic Supply and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10860

LOE ID: | 9636
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 15 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin Objective for municipal and domestic supply uses of inland surface waters (Section II.A.2) states the following: waters shall not contain concentrations of chemical constituents in excess of the limits specified in California Code of Regulations, Title 22, Article 4, Chapter 15, Section 64435, Tables 2 and 3 as listed in Table 3-2. The maximum contaminant level listed in Table 3-2 (inorganic and fluoride concentrations not to be exceeded in domestic or municipal supply) for nitrate is 10.0 mg/L (NO3 as N).
Objective/Criterion Reference: | Title 22, Division 4, Ch. 15, Article 4, Section 64431, Table 64431-A
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/27/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 9623
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 15 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when nitrate exceeds 30 mg/L NO3 as N in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/27/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14793
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 192
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 2 of 192 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin Objective for municipal and domestic supply uses of inland surface waters (Section II.A.2) states the following: waters shall not contain concentrations of chemical constituents in excess of the limits specified in California Code of Regulations, Title 22, Article 4, Chapter 15, Section 64435, Tables 2 and 3 as listed in Table 3-2. The maximum contaminant level listed in Table 3-2 (inorganic and fluoride concentrations not to be exceeded in domestic or municipal supply) for nitrate is 10.0 mg/L (NO3 as N).
Objective/Criterion Reference: | Title 22, Division 4, Ch. 15, Article 4, Section 64431, Table 64431-A
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive, AT7 - Atascadero Creek]
Temporal Representation: | Data was collected over the time period 10/23/2000-1/7/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis
LOE ID: | 9836
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 60
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 60 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin Objective for municipal and domestic supply uses of inland surface waters (Section II.A.2) states the following: waters shall not contain concentrations of chemical constituents in excess of the limits specified in California Code of Regulations, Title 22, Article 4, Chapter 15, Section 64435, Tables 2 and 3 as listed in Table 3-2. The maximum contaminant level listed in Table 3-2 (inorganic and fluoride concentrations not to be exceeded in domestic or municipal supply) for nitrate is 10.0 mg/L (NO3 as N).
Objective/Criterion Reference: | Title 22, Division 4, Ch. 15, Article 4, Section 64431, Table 64431-A
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14792
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 192
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 192 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when nitrate exceeds 30 mg/L NO3 as N in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive, AT7 - Atascadero Creek]
Temporal Representation: | Data was collected over the time period 10/23/2000-1/7/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis
LOE ID: | 9824
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 60
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 60 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when nitrate exceeds 30 mg/L NO3 as N in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10820
Pollutant: | Nitrogen, ammonia (Total Ammonia)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. None of the 75 samples exceed the water quality objective for Cold Freshwater Habitat. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of the 75 samples exceed the water quality objective for Cold Freshwater Habitat and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10820

LOE ID: | 9853
Pollutant: | Ammonia as Nitrogen
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 15 samples exceed the criterion for Ammonia as N, Total.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | USEPA Health Advisory 2006 Edition of the Drinking Water Standards and Health Advisories (EPA 822-R-06-013, 2006).
Objective/Criterion Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Evaluation Guideline: | EPA's Lifetime Health advisory level for total ammonia is 30.0 mg/L as stated on page 8 of the 2006 edition of the drinking water standards and health advisories. This Advisory Level is defined as "the concentration of a chemical in drinking water that is not expected to cause any adverse noncarcinogenic effects for up to ten days of exposure."
Guideline Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/27/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 9808
Pollutant: | Ammonia as Nitrogen
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 60
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 60 samples exceed the criterion for Ammonia as N, Total.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | USEPA Health Advisory 2006 Edition of the Drinking Water Standards and Health Advisories (EPA 822-R-06-013, 2006).
Objective/Criterion Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Evaluation Guideline: | EPA's Lifetime Health advisory level for total ammonia is 30.0 mg/L as stated on page 8 of the 2006 edition of the drinking water standards and health advisories. This Advisory Level is defined as "the concentration of a chemical in drinking water that is not expected to cause any adverse noncarcinogenic effects for up to ten days of exposure."
Guideline Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 15511
Pollutant: | Phenanthrene
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15511

LOE ID: | 16892
Pollutant: | Phenanthrene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Phenanthrene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Phenanthrene is 1170 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16893
Pollutant: | Phenanthrene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Phenanthrene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Phenanthrene is 1170 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 17052
Pollutant: | Phenanthrene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Phenanthrene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Phenanthrene is 1170 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 17051
Pollutant: | Phenanthrene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Phenanthrene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Phenanthrene is 1170 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 15512
Pollutant: | Pyrene
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither sample exceeds the exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15512

LOE ID: | 17825
Pollutant: | Pyrene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Pyrene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Pyrene is 1520 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 17826
Pollutant: | Pyrene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Pyrene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Pyrene is 1520 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16930
Pollutant: | Pyrene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Pyrene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Pyrene is 1520 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16916
Pollutant: | Pyrene
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Pyrene.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for Pyrene is 1520 ug/Kg dry weight (Macdonald et al. 2000)
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10869
Pollutant: | Salinity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Three lines of evidence is available in the administrative record to assess this pollutant. None of the 77 samples exceed the water quality objective for Agricultural Supply. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of the 77 samples exceed the water quality objective for Agricultural Supply and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10869

LOE ID: | 13303
Pollutant: | Salinity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 59
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 59 samples exceed the criterion for Salinity.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when salinity exceeds 3.0 ppt in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13052
Pollutant: | Salinity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 6
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 6 samples exceed the criterion for Salinity.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when salinity exceeds 3.0 ppt in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 7/16/2001-9/26/2001. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13074
Pollutant: | Salinity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 12
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 12 samples exceed the criterion for Salinity.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when salinity exceeds 3.0 ppt in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 16074
Pollutant: | Sediment Toxicity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.6 of the Listing Policy. Under section 3.6 a single line of evidence is necessary to assess listing status for toxicity. Two lines of evidence are available in the administrative record to assess this pollutant in sediment samples. The single sample was not toxic to invertebrate test organisms (exhibit a significant increase in mortality compared to the laboratory control) and therefore do not exceed the narrative General Objective for toxicity, set to protect for aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. single sample was not toxic to invertebrate test organisms. Therefore, this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded and the sample size is insufficient to determine with the power and confidence of the Listing Policy if water quality standards are met or exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16074

LOE ID: | 23614
Pollutant: | Invertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Toxicity, Hyalella azteca Survival (%) 10 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 23613
Pollutant: | Invertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Toxicity, Hyalella azteca Survival (%) 10 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 15513
Pollutant: | Turbidity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Eight lines of evidence are available in the administrative record to assess this pollutant. Seventeen of the 227 samples exceed the Evaluation Guideline (Sigler et al., 1984) applied to protect for aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Seventeen of the 227 samples exceed the Evaluation Guideline (Sigler et al., 1984) applied to protect for aquatic life beneficial uses and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15513

LOE ID: | 14971
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 158
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 6 of 158 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT1 - Atascadero Creek at Ward Drive, AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive]
Temporal Representation: | Data was collected over the time period 6/2/2002-1/7/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis
LOE ID: | 13304
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 50
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 6 of 50 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13088
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 5
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 5 of 13 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13089
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 5
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 5 of 13 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13305
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 50
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 6 of 50 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14987
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 158
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 6 of 158 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT1 - Atascadero Creek at Ward Drive, AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive]
Temporal Representation: | Data was collected over the time period 6/2/2002-1/7/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis
LOE ID: | 13053
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 6
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 6 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 7/16/2001-9/26/2001. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13054
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 6
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 6 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 7/16/2001-9/26/2001. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 16075
Pollutant: | Unknown Toxicity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 and section 3.6 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant in water samples. None of the samples were toxic to test organisms (exhibited a significant increase in mortality compared to the laboratory control) and therefore do not exceed the narrative General Objective for toxicity, set to protect for aquatic life beneficial uses. The following is a summary of the results from individual toxicity tests. None of the 2 samples (tested for toxicity to vertebrate test organisms) exhibited a significant increase in mortality compared to the laboratory control. In addition, none of the 2 samples, tested for toxicity to invertebrate test organisms exhibited a significant increase in mortality compared to the laboratory control. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of the 2 samples (tested for toxicity to vertebrate test organisms) exhibited a significant increase in mortality compared to the laboratory control. In addition, none of the 2 samples, tested for toxicity to invertebrate test organisms exhibited a significant increase in mortality compared to the laboratory control. Therefore, this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16075

LOE ID: | 23610
Pollutant: | Invertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 4
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 4 samples exceed the criterion for Toxicity, Ceriodaphnia dubia Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 12/5/2001-3/27/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 23618
Pollutant: | Vertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 4
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 4 samples exceed the criterion for Toxicity, Pimephales promelas Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATU-Atascadero Creek at Patterson Avenue, 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 12/5/2001-3/27/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 23609
Pollutant: | Invertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 4
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 4 samples exceed the criterion for Toxicity, Ceriodaphnia dubia Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 12/5/2001-3/27/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 23617
Pollutant: | Vertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 4
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 4 samples exceed the criterion for Toxicity, Pimephales promelas Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATU-Atascadero Creek at Patterson Avenue, 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 12/5/2001-3/27/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10889
Pollutant: | Zinc
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Neither of the two samples exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither of the two samples exceed the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life beneficial uses and therefore this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10889

LOE ID: | 17920
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Zinc.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for zinc is 459 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 17921
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (03SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Zinc.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for zinc is 459 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/31/2004. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 17813
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Zinc.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for zinc is 459 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 17828
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (00SW3001) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Zinc.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for zinc is 459 mg/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected on a single day 3/26/2002. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10846
Pollutant: | Chloride
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture | Confined Animal Feeding Operations (NPS) | Grazing-Related Sources | Urban Runoff/Storm Sewers
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.2 of the Listing Policy. One line of evidence is available in the administrative record to assess this pollutant. Based on section 3.2 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Fifty-five of 68 samples exceed the water quality objective for Agricultural Supply and this supports rejection of the nully hypothesis. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Fifty-five of 68 samples exceed the water quality objective for Agricultural Supply and this meets or exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10846

LOE ID: | 9620
Pollutant: | Chloride
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 15
Number of Exceedances: | 12
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 12 of 15 samples exceed the criterion for Chloride.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when chloride exceeds 106 mg/L in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/27/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 9823
Pollutant: | Chloride
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 53
Number of Exceedances: | 43
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 43 of 53 samples exceed the criterion for Chloride.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when chloride exceeds 106 mg/L in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10854
Pollutant: | Enterococcus
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture | Confined Animal Feeding Operations (NPS) | Grazing-Related Sources | Natural Sources | Urban Runoff/Storm Sewers
Expected TMDL Completion Date: | 2013
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.3 of the Listing Policy. Two lines of evidence are available in the administrative record to assess this pollutant. Based on section 3.3 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Eighty-six out of 157 samples exceed the Evaluation Guideline (USEPA Ambient Water Quality Criteria for Bacteria, 1986) as it applies to the Water Contact Recreation beneficial use and this supports rejection of the null hypotheses. Only 7 of 157 samples exceed the water quality objective for Non-Contact Recreation and therefore this beneficial use is fully supported. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Eighty-six out of 157 samples exceed the Evaluation Guideline (USEPA Ambient Water Quality Criteria for Bacteria, 1986) as it applies to the Water Contact Recreation beneficial use and this meets or exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10854

LOE ID: | 15104
Pollutant: | Enterococcus
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 157
Number of Exceedances: | 7
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 7 of 157 samples exceed the criterion for Enterococci.
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml. Enterococcus is a fecal coliform.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT1 - Atascadero Creek at Ward Drive, AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive]
Temporal Representation: | Data was collected over the time period 6/2/2002-2/4/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis
LOE ID: | 14985
Pollutant: | Enterococcus
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 157
Number of Exceedances: | 86
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 86 of 157 samples exceed the EPA criterion for Enterococci.
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | USEPA Ambient Water Quality Criteria for Bacteria -1986.
Objective/Criterion Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | Single sample maximum allowable density for Enterococci in freshwater is 61 MPN/100mL (as stated in Table 4, page 15).
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT1 - Atascadero Creek at Ward Drive, AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive]
Temporal Representation: | Data was collected over the time period 6/2/2002-2/4/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis

DECISION ID | 10855
Pollutant: | Escherichia coli (E. Coli)
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture | Confined Animal Feeding Operations (NPS) | Grazing-Related Sources | Natural Sources | Urban Runoff/Storm Sewers
Expected TMDL Completion Date: | 2013
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.3 of the Listing Policy. Four lines of evidence are available in the administrative record to assess this pollutant. Based on section 3.3 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Sixty of 181 samples exceed the Evaluation Guideline (USEPA Ambient Water Quality Criteria for Bacteria, 1986) as it applies to the Water Contact Recreation beneficial use and this supports rejection of the null hypothesis. Only 9 of 181 samples exceed the water quality objective for Non-Contact Recreation, and therefore this beneficial use is fully supported. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. If insufficient sample count add blurb here This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Sixty of 181 samples exceed the Evaluation Guideline (USEPA Ambient Water Quality Criteria for Bacteria, 1986) as it applies to the Water Contact Recreation beneficial use and this meets or exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10855

LOE ID: | 14943
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 156
Number of Exceedances: | 9
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 9 of 156 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml. E. coli is a fecal coliform.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT1 - Atascadero Creek at Ward Drive, AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive]
Temporal Representation: | Data was collected over the time period 6/2/2002-2/4/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis
LOE ID: | 14927
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 156
Number of Exceedances: | 51
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 51 of 156 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | USEPA Ambient Water Quality Criteria for Bacteria -1986.
Objective/Criterion Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | Single sample maximum allowable density for E. coli in freshwater is 235 MPN/100mL (as stated in Table 4, page 15)
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT1 - Atascadero Creek at Ward Drive, AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive]
Temporal Representation: | Data was collected over the time period 6/2/2002-2/4/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis
LOE ID: | 11515
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 25
Number of Exceedances: | 0
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 25 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml. E. coli is a fecal coliform.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 1/6/2005-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11514
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 25
Number of Exceedances: | 9
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 9 of 25 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | USEPA Ambient Water Quality Criteria for Bacteria -1986.
Objective/Criterion Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | Single sample maximum allowable density for E. coli in freshwater is 235 MPN/100mL (as stated in Table 4, page 15)
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 1/6/2005-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10856
Pollutant: | Fecal Coliform
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture | Confined Animal Feeding Operations (NPS) | Grazing-Related Sources | Natural Sources | Urban Runoff/Storm Sewers
Expected TMDL Completion Date: | 2013
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.3 of the Listing Policy. Four lines of evidence are available in the administrative record to assess this pollutant. Based on section 3.3 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Twenty-two of 75 samples exceeded the water quality objective for Water Contact Recreation and this supports rejection of the null hypothesis. Only 7 of the 75 samples exceeded the water quality objective for Non-Contact Recreation, and therefore this beneficial use is fully supported. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Twenty-two of 75 samples exceeded the water quality objective for Water Contact Recreation and this meets or exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10856

LOE ID: | 11476
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 61
Number of Exceedances: | 4
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 4 of 61 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11475
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 61
Number of Exceedances: | 15
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 15 of 61 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 200 MPN/100 ml, nor shall more than ten percent of total samples during any 30-day period exceed 400 MPN/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11530
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 14
Number of Exceedances: | 7
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 7 of 14 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 200 MPN/100 ml, nor shall more than ten percent of total samples during any 30-day period exceed 400 MPN/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11531
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 14
Number of Exceedances: | 3
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 3 of 14 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10862
Pollutant: | Low Dissolved Oxygen
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture | Confined Animal Feeding Operations (NPS) | Grazing-Related Sources | Urban Runoff/Storm Sewers
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.2 of the Listing Policy. Sixteen lines of evidence are available in the administrative record to assess this pollutant. Based on section 3.2 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Three water quality objectives are assessed: Fifty-one of 227 samples exceed the Dissolved Oxygen water quality objective for Cold Freshwater Habitat, and this supports rejection of the null hypothesis. However, only 16 of 227 samples exceed the Dissolved Oxygen water quality objectives for Warm Freshwater Habitat, and this beneficial use is fully supported In addition, 78 of 255 samples exceed the general water quality objective for oxygen saturation (when applied as a single sample maximum). However, the Basin Plan objective states that the median oxygen saturation value shall not fall below 85% and the median value did not exceed this criterion. Therefore, the use rating for oxygen saturation is set at insufficient information. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Fifty-one of 227 samples exceed the water quality objective for Cold Freshwater Habitat and this meets or exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10862

LOE ID: | 13286
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 59
Number of Exceedances: | 7
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 7 of 59 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, dissolved oxygen concentration shall not be reduced below 5.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13070
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 3 of 13 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13071
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 13 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, dissolved oxygen concentration shall not be reduced below 5.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13072
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 4 of 13 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13073
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 4 of 13 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13301
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 59
Number of Exceedances: | 23
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 23 of 59 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13302
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 59
Number of Exceedances: | 23
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 23 of 59 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13320
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 8
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 3 of 8 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 7/16/2001-8/13/2004. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13321
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 8
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 8 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, dissolved oxygen concentration shall not be reduced below 5.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 7/16/2001-8/13/2004. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13322
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 8
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 4 of 8 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 7/16/2001-8/13/2004. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13323
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 8
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 4 of 8 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 7/16/2001-8/13/2004. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13285
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 59
Number of Exceedances: | 14
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 14 of 59 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15145
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 145
Number of Exceedances: | 47
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 47 of 145 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT1 - Atascadero Creek at Ward Drive, AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive]
Temporal Representation: | Data was collected over the time period 6/2/2002-1/7/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis
LOE ID: | 15144
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 145
Number of Exceedances: | 47
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 47 of 145 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT1 - Atascadero Creek at Ward Drive, AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive]
Temporal Representation: | Data was collected over the time period 6/2/2002-1/7/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis
LOE ID: | 15103
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 147
Number of Exceedances: | 9
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 9 of 147 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, dissolved oxygen concentration shall not be reduced below 5.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT1 - Atascadero Creek at Ward Drive, AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive]
Temporal Representation: | Data was collected over the time period 6/2/2002-1/7/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis
LOE ID: | 15088
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 147
Number of Exceedances: | 31
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 31 of 147 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT1 - Atascadero Creek at Ward Drive, AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive]
Temporal Representation: | Data was collected over the time period 6/2/2002-1/7/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis

DECISION ID | 10874
Pollutant: | Sodium
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture | Confined Animal Feeding Operations (NPS) | Grazing-Related Sources | Urban Runoff/Storm Sewers
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.2 of the Listing Policy. Two lines of evidence are available in the administrative record to assess this pollutant. Based on section 3.2 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Sixty out of 68 samples exceed the water quality objective for Agricultural Supply and this supports rejection of the null hypothesis. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Sixty out of 68 samples exceed the water quality objective for Agricultural Supply and this meets or exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10874

LOE ID: | 9637
Pollutant: | Sodium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 15
Number of Exceedances: | 13
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 13 of 15 samples exceed the criterion for Sodium.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when sodium exceeds 69 mg/L in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/27/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 9837
Pollutant: | Sodium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 53
Number of Exceedances: | 47
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 47 of 53 samples exceed the criterion for Sodium.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when sodium exceeds 69 mg/L in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10879
Pollutant: | Temperature, water
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture | Confined Animal Feeding Operations (NPS) | Grazing-Related Sources | Urban Runoff/Storm Sewers
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.2 of the Listing Policy. Four lines of evidence are available in the administrative record to assess this pollutant. Based on section 3.2 the site exceeded evaluation guidelines for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Sixty-two out of 233 samples exceed the Evaluation Guideline set for Cold Freshwater Habitat. In addition, A recent publication (Steelhead/Rainbow Trout (Oncorhynchus mykiss) Resources South of the Golden Gate, California (Becker, G.S and I.J Reining, October 2008) identifies Atascadero Creek as having "Definite run or population". Therefore this Temperature Evaluation Guideline is relevant to the waterbody. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Sixty-two out of 233 samples exceed the Evaluation Guideline set for Cold Freshwater Habitat and this meets or exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10879

LOE ID: | 13055
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 8
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 2 of 8 samples exceed the criterion for Water Temperature.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Board that such alteration in temperature does not adversely affect beneficial uses (General Objective in Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Inland Fishes of California (Moyle 1976) states that for rainbow trout the optimum range for growth and completion of most life stages is 13-21 degrees C (page 129).
Guideline Reference: | Inland Fishes of California
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 7/16/2001-8/13/2004. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13090
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 5
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 5 of 13 samples exceed the criterion for Water Temperature.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Board that such alteration in temperature does not adversely affect beneficial uses (General Objective in Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Inland Fishes of California (Moyle 1976) states that for rainbow trout the optimum range for growth and completion of most life stages is 13-21 degrees C (page 129).
Guideline Reference: | Inland Fishes of California
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15027
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 153
Number of Exceedances: | 40
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 40 of 153 samples exceed the criterion for Water Temperature.
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | Natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Board that such alteration in temperature does not adversely affect beneficial uses (General Objective in Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Inland Fishes of California (Moyle 1976) states that for rainbow trout the optimum range for growth and completion of most life stages is 13-21 degrees C (page 129).
Guideline Reference: | Inland Fishes of California
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT1 - Atascadero Creek at Ward Drive, AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive]
Temporal Representation: | Data was collected over the time period 6/2/2002-1/7/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis
LOE ID: | 13319
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 59
Number of Exceedances: | 15
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 15 of 59 samples exceed the criterion for Water Temperature.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Board that such alteration in temperature does not adversely affect beneficial uses (General Objective in Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Inland Fishes of California (Moyle 1976) states that for rainbow trout the optimum range for growth and completion of most life stages is 13-21 degrees C (page 129).
Guideline Reference: | Inland Fishes of California
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10892
Pollutant: | pH
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture | Confined Animal Feeding Operations (NPS) | Grazing-Related Sources | Urban Runoff/Storm Sewers
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.2 of the Listing Policy. Twenty lines of evidence are available in the administrative record to assess this pollutant. Based on section 3.2 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Forty-eight of 238 samples exceeded the water quality objectives for Water Contact Recreation, Non-Contact Recreation, and Municipal and Domestic Supply, and this supports rejection of the null hypothesis. Twenty-seven of 238 samples exceeded the water quality objectives for Cold and Water Freshwater Habitat, and 39 of 238 samples exceeded the water quality objectives for Agricultural Supply. These other beneficial uses are fully supported. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. It should be noted that pH tends to be high in the Central Coast Region due to area geology, and exceedances may not be caused by anthropogenic activities. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Forty-eight of 238 samples exceeded the water quality objectives for Water Contact Recreation, Non-Contact Recreation, and Municipal and Domestic Supply, and this supports rejection of the null hypothesis and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10892

LOE ID: | 11512
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 6
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 6 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when pH is greater than 8.4 or less than 6.5 in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 7/16/2001-9/26/2001. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11550
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 13 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11549
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 13 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11548
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 13 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin, Section II.A.2. Municipal and Domestic Supply Objectives, Section II.A.2.a states the following: The pH value shall neither be depressed below 6.5 or raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11547
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 13 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11513
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 6
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 6 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 7/16/2001-9/26/2001. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11533
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 13 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when pH is greater than 8.4 or less than 6.5 in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15126
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 160
Number of Exceedances: | 37
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 37 of 160 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when pH is greater than 8.4 or less than 6.5 in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT1 - Atascadero Creek at Ward Drive, AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive]
Temporal Representation: | Data was collected over the time period 6/2/2002-1/7/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis
LOE ID: | 14869
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 160
Number of Exceedances: | 25
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 25 of 160 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT1 - Atascadero Creek at Ward Drive, AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive]
Temporal Representation: | Data was collected over the time period 6/2/2002-1/7/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis
LOE ID: | 14868
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 160
Number of Exceedances: | 46
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 46 of 160 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT1 - Atascadero Creek at Ward Drive, AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive]
Temporal Representation: | Data was collected over the time period 6/2/2002-1/7/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis
LOE ID: | 15162
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 160
Number of Exceedances: | 46
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 46 of 160 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT1 - Atascadero Creek at Ward Drive, AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive]
Temporal Representation: | Data was collected over the time period 6/2/2002-1/7/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis
LOE ID: | 15161
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 160
Number of Exceedances: | 46
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 46 of 160 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin, Section II.A.2. Municipal and Domestic Supply Objectives, Section II.A.2.a states the following: The pH value shall neither be depressed below 6.5 or raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT1 - Atascadero Creek at Ward Drive, AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive]
Temporal Representation: | Data was collected over the time period 6/2/2002-1/7/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis
LOE ID: | 15160
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 160
Number of Exceedances: | 25
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Santa Barbara Channelkeepers Citizen Monitoring Program (R3_SBKeepers) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 25 of 160 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Mutiple data sets, City of Santa Maria, Watsonville and Santa Barbara Channel Keeper Data
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 3 monitoring sites [ AT1 - Atascadero Creek at Ward Drive, AT2 - Atascadero Creek at Patterson Drive, AT3 - Atascadero Creek at Puente Drive]
Temporal Representation: | Data was collected over the time period 6/2/2002-1/7/2007. Santa Barbara Channelkeepers Citizen Monitoring is conducted monthly.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP, data entry completed by volunteers. Several errors were identified in data and were flagged or fixed by RB staff (in communication with SB Channel Keepers) prior to assessment of data.
QAPP Information Reference(s): | e-mail documenting QA procedures and analytical methods uses for sample analysis
LOE ID: | 11496
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 59
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 2 of 59 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11495
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 59
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 2 of 59 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11494
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 59
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 2 of 59 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11493
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 59
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 2 of 59 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin, Section II.A.2. Municipal and Domestic Supply Objectives, Section II.A.2.a states the following: The pH value shall neither be depressed below 6.5 or raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11345
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 6
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 6 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 7/16/2001-9/26/2001. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11344
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 6
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 6 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 7/16/2001-9/26/2001. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11478
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 59
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 2 of 59 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when pH is greater than 8.4 or less than 6.5 in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11492
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 59
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Coastal Confluences (CC) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 2 of 59 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATA-Atascadero Creek at Ward Drive ]
Temporal Representation: | Data was collected over the time period 3/7/2001-12/5/2006. CCAMP Coastal confluence monitoring is conducted monthly (with the exception of April 2003 - December 2003) and is ongoing.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11327
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 6
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 6 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin, Section II.A.2. Municipal and Domestic Supply Objectives, Section II.A.2.a states the following: The pH value shall neither be depressed below 6.5 or raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 7/16/2001-9/26/2001. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11551
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Barbara (SantaBarb) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 13 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 1 monitoring site [ 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 1/17/2001-3/7/2002. Santa Barbara Coast is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11343
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 6
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Atascadero Creek(315) to determine beneficial use support and results are as follows: 0 of 6 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Atascadero Creek(315) was collected at 2 monitoring sites [ 315ATA-Atascadero Creek at Ward Drive , 315ATU-Atascadero Creek at Patterson Avenue]
Temporal Representation: | Data was collected over the time period 7/16/2001-9/26/2001. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):