# Draft 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 3 - Central Coast Region

Water Body Name: | Struve Slough
Water Body ID: | CAR3051003020080603125227
Water Body Type: | River & Stream

DECISION ID | 11108
Pollutant: | Ammonia (Unionized)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. None of the 16 samples exceed the exceed the General water quality objective as it applies to the Warm Freshwater Habitat beneficial use. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of the 16 samples exceed the exceed the General water quality objective as it applies to the Warm Freshwater Habitat beneficial use, and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 11108

LOE ID: | 9365
Pollutant: | Ammonia (Unionized)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Struve Slough to determine beneficial use support and results are as follows: 0 of 14 samples exceed the criterion for Ammonia as N, Unionized.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin General Objective, Chapter III, Section II.A.2 (General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries) states that the discharge of wastes shall not cause concentrations of unionized ammonia (NH3) to exceed 0.025 mg/l (as N) in receiving waters (page III-4) .
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 1/24/2005-3/16/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13901
Pollutant: | Ammonia (Unionized)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Northern Area Ag-Waiver Monitoring (R3_CMPNorth) data for Struve Slough to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Ammonia as N, Unionized.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin General Objective, Chapter III, Section II.A.2 (General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries) states that the discharge of wastes shall not cause concentrations of unionized ammonia (NH3) to exceed 0.025 mg/l (as N) in receiving waters (page III-4) .
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 2/21/2006-3/28/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 12831
Pollutant: | Chlorophyll-a
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. Three of the 21 samples exceed the Evaluation Guideline (North Carolina Administrative code, Title 15A) and the General Water Quality Objective set to protect aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 26 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Three of the 21 samples exceed the Evaluation Guideline (North Carolina Administrative code, Title 15A) and the General Water Quality Objective set to protect aquatic life beneficial uses and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12831

LOE ID: | 9178
Pollutant: | Chlorophyll-a
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 16
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Struve Slough to determine beneficial use support and results are as follows: 3 of 16 samples exceed the criterion for Chlorophyll a.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Evaluation Guideline: | North Carolina Administrative code (NCAC), Title 15A - Environmental and Natural Resources, Subchapter 2B-Surface water and wetland standards, Rule 0211-Fresh surface water quality standards for class C waters (Class C is defined as freshwaters protected for secondary recreation, fishing, aquatic life including propagation and survival, and wildlife). Section 3(a) of Rule 0211 applies to all fresh surface waters and states that chlorophyll a is not to exceed 40 ug/L.
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 1/24/2005-3/16/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13902
Pollutant: | Chlorophyll-a
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 5
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Northern Area Ag-Waiver Monitoring (R3_CMPNorth) data for Struve Slough to determine beneficial use support and results are as follows: 0 of 5 samples exceed the criterion for Chlorophyll a.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Evaluation Guideline: | North Carolina Administrative code (NCAC), Title 15A - Environmental and Natural Resources, Subchapter 2B-Surface water and wetland standards, Rule 0211-Fresh surface water quality standards for class C waters (Class C is defined as freshwaters protected for secondary recreation, fishing, aquatic life including propagation and survival, and wildlife). Section 3(a) of Rule 0211 applies to all fresh surface waters and states that chlorophyll a is not to exceed 40 ug/L.
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 2/21/2006-9/26/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 12989
Pollutant: | Sediment Toxicity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 and section 3.6 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant in sediment samples. The single sample was not toxic to invertebrate test organisms (did not exhibit a significant increase in mortality compared to the laboratory control) and therefore do not exceed the narrative General Objective for toxicity, set to protect for aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting, only a single toxicity sample is assessed here. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. The single sample was not toxic to invertebrate test organisms (did not exhibit a significant increase in mortality compared to the laboratory control) and therefore did not exceed the narrative General Objective for toxicity, set to protect for aquatic life beneficial uses and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because it cannot be determined if applicable water quality standards are not being exceeded because sample size is insufficient.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12989

LOE ID: | 24774
Pollutant: | Invertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Northern Area Ag-Waiver Monitoring (R3_CMPnorth) data for Struve Slough to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Toxicity, Hyalella azteca Survival (%) 10 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected on a single day 5/23/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 11113
Pollutant: | Total Coliform
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.3 of the Listing Policy. However, on July 19, 2007 USEPA amended the water quality standards for Watsonville Slough and its tributaries (specifically including Struve Slough) by removing Shellfish Harvesting as a designated use. Concurrent with the submitted Pathogen TMDL, staff submitted a Use Attainability Analysis (UAA) to amend the beneficial use designations. The USEPA approved the UAA on March 28, 2007.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because teh beneficial use has been removed.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 11113

LOE ID: | 17422
Pollutant: | Total Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Shellfish Harvesting
Number of Samples: | 9
Number of Exceedances: | 9
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Struve Slough to determine beneficial use support and results are as follows: 9 of 9 samples exceed the criterion for Coliform, Total.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin Shellfish Harvesting objective (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries (page III-12)) states the following: At all areas where shellfish may be harvested for human consumption, the median total coliform concentration throughout the water column for any 30-day period shall not exceed 70 MPN/100mL, not shall more than ten percent of the samples collected during any 30-day period exceed 230 MPN/100mL for a five tube decimal dilution test.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 3 monitoring sites [ 305-WSTRU-21 - West Branch of Struve Slough at Harkins Slough Rd/Green Valley Road junction (DFG Site), 305-STRUV-21 - Struve Slough, 305-STRUV-22 - Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 5/17/2003-5/7/2005. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 17459
Pollutant: | Total Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Shellfish Harvesting
Number of Samples: | 4
Number of Exceedances: | 4
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Clean streams project) (R3_CLNStrm) data for Struve Slough to determine beneficial use support and results are as follows: 4 of 4 samples exceed the criterion for Coliform, Total.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin Shellfish Harvesting objective (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries (page III-12)) states the following: At all areas where shellfish may be harvested for human consumption, the median total coliform concentration throughout the water column for any 30-day period shall not exceed 70 MPN/100mL, not shall more than ten percent of the samples collected during any 30-day period exceed 230 MPN/100mL for a five tube decimal dilution test.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 2 monitoring sites [ 305-WSTRU-21 - West Branch of Struve Slough at Harkins Slough Rd/Green Valley Road junction (DFG Site), 305-STRUV-21 - Struve Slough]
Temporal Representation: | Data was collected over the time period 5/26/2004-7/6/2004.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Data entry completed by volunteers. Multiple errors were identified in data and were flagged by RB staff (in communication with Clean Streams Program staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 13814
Pollutant: | Total Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Shellfish Harvesting
Number of Samples: | 54
Number of Exceedances: | 49
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Central Coast Watershed Studies (R3_CCOWS) data for Struve Slough to determine beneficial use support and results are as follows: 49 of 54 samples exceed the criterion for Coliform, Total.
Data Reference: | Final Data File used for assessment: CCoWS (Central Coast Watershed Studies) Water Quality Data
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin Shellfish Harvesting objective (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries (page III-12)) states the following: At all areas where shellfish may be harvested for human consumption, the median total coliform concentration throughout the water column for any 30-day period shall not exceed 70 MPN/100mL, not shall more than ten percent of the samples collected during any 30-day period exceed 230 MPN/100mL for a five tube decimal dilution test.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 9 monitoring sites [ Lee Rd, near Cherry Blossom Drive, near Cherry Blossom Drive, near Cherry Blossom Drive, Cherry Blossom Dr; site coordinates done with spatial data editor in TNTmips because field GPS coordinates were not very accurate, Cherry Blossom Road, Cherry Blossom Drive; site coordinates done with spatial data editor in TNTmips because field GPS coordinates were not very accurate, Airport Boulevard, Harkins Slough Rd.]
Temporal Representation: | Data was collected over the time period 2/18/2003-12/9/2003.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Data quality is good and Standard Operating Procedures are well documented in QAPP. However, data documentation is poor and replicate samples and other quality assurance measurements are not consistently documented in this data set.
QAPP Information Reference(s):
LOE ID: | 11239
Pollutant: | Total Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Shellfish Harvesting
Number of Samples: | 28
Number of Exceedances: | 27
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Struve Slough to determine beneficial use support and results are as follows: 27 of 28 samples exceed the criterion for Coliform, Total.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin Shellfish Harvesting objective (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries (page III-12)) states the following: At all areas where shellfish may be harvested for human consumption, the median total coliform concentration throughout the water column for any 30-day period shall not exceed 70 MPN/100mL, not shall more than ten percent of the samples collected during any 30-day period exceed 230 MPN/100mL for a five tube decimal dilution test.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 1/24/2005-3/16/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 13002
Pollutant: | Turbidity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.2 of the Listing Policy. Four lines of evidence are available in the administrative record to assess this pollutant. Based on section 3.2 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Based on the readily available data and information, the weight of evidence indicates that there is insufficient justification for placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Eighteen of 60 samples exceeded the Evaluation Guideline (Sigler et al., 1984) applied to protect for aquatic life beneficial use and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. However, this Evaluation Guideline is not relevant to Struve Slough as it is not documented as steelhead habitat. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because this Evaluation Guideline is not relevant in this waterbody.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 13002

LOE ID: | 13718
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 35
Number of Exceedances: | 5
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Central Coast Watershed Studies (R3_CCOWS) data for Struve Slough to determine beneficial use support and results are as follows: 5 of 35 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: CCoWS (Central Coast Watershed Studies) Water Quality Data
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 3 monitoring sites [ Cherry Blossom Dr; site coordinates done with spatial data editor in TNTmips because field GPS coordinates were not very accurate, Lee Rd, Harkins Slough Rd.]
Temporal Representation: | Data was collected over the time period 2/18/2003-7/16/2003.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Data quality is good and Standard Operating Procedures are well documented in QAPP. However, data documentation is poor and replicate samples and other quality assurance measurements are not consistently documented in this data set.
QAPP Information Reference(s):
LOE ID: | 12054
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 8
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Struve Slough to determine beneficial use support and results are as follows: 1 of 8 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 7/21/2005-3/16/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16943
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 12
Number of Exceedances: | 9
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Monterey Area Research Consortium (R3_MARC) data for Struve Slough to determine beneficial use support and results are as follows: 9 of 12 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: Marc Los Huertos Water Quality Data, file A
| Final Data File used for assessment: Marc Los Huertos Water Quality Data, file B
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ SS-LEE - Struve Slough at Lee Rd]
Temporal Representation: | Data was collected over the time period 2/22/2006-1/24/2007.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 13651
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 5
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Northern Area Ag-Waiver Monitoring (R3_CMPNorth) data for Struve Slough to determine beneficial use support and results are as follows: 3 of 5 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 2/21/2006-9/26/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 12988
Pollutant: | Unknown Toxicity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 and section 3.6 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Three lines of evidence are available in the administrative record to assess this pollutant in water samples. None of the samples were toxic to test organisms (exhibited a significant increase in mortality or decrease in cell density compared to the laboratory control) and therefore do not exceed the narrative General Objective for toxicity, set to protect for aquatic life beneficial uses. The following is a summary of the results from individual toxicity tests. None of the 3 samples (tested for toxicity to plants) exhibited significant reduction in cell density relative to the control. In addition, None of the 3 samples (tested for toxicity to vertebrate test organisms) exhibited a significant increase in mortality compared to the laboratory control. Lastly, none of the 3 samples, tested for toxicity to invertebrate test organisms did not exhibit a significant increase in mortality compared to the laboratory control. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting, only 7 toxicity samples are assessed here. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of the samples were toxic to test organisms and therefore do not exceed the narrative General Objective for toxicity, set to protect for aquatic life beneficial uses and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12988

LOE ID: | 24785
Pollutant: | Vertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 3
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Northern Area Ag-Waiver Monitoring (R3_CMPnorth) data for Struve Slough to determine beneficial use support and results are as follows: 0 of 3 samples exceed the criterion for Toxicity, Pimephales promelas Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 2/21/2006-9/26/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 24786
Pollutant: | Plant Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 3
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Northern Area Ag-Waiver Monitoring (R3_CMPnorth) data for Struve Slough to determine beneficial use support and results are as follows: 0 of 3 samples exceed the criterion for Toxicity, Selenastrum capricornutum Growth (Cell Density) 4 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction in cell count of test organism relative to the control (alpha < 0.05) and cell count <80% of control.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 2/21/2006-9/26/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 24763
Pollutant: | Invertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 3
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Northern Area Ag-Waiver Monitoring (R3_CMPnorth) data for Struve Slough to determine beneficial use support and results are as follows: 0 of 3 samples exceed the criterion for Toxicity, Ceriodaphnia dubia Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected between 2/21/2006 and 9/26/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 11112
Pollutant: | Low Dissolved Oxygen
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture | Other Urban Runoff
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.2 of the Listing Policy. Five lines of evidence are available in the administrative record to assess this pollutant. Two water quality objectives are assessed: Fifty-three of 61 samples exceeded the Warm Freshwater Habitat water quality objective and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. In addition, 17 of 19 samples (and therefore the median value) exceeded the General water quality objective set to protect for Warm Freshwater Habitat (when applied as a single sample maximum). This also exceeds the Basin Plan objective which states that the median oxygen saturation value shall not fall below 85%. Based on section 3.2 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Fifty-three of 61 samples exceeded the Warm Freshwater Habitat water quality objective and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. In addition, 17 of 19 samples (and therefore the median value) exceeded the General water quality objective set to protect for Warm Freshwater Habitat and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 11112

LOE ID: | 18134
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 9
Number of Exceedances: | 9
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Struve Slough to determine beneficial use support and results are as follows: 9 of 9 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, dissolved oxygen concentration shall not be reduced below 5.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 3 monitoring sites [ 305-WSTRU-21 - West Branch of Struve Slough at Harkins Slough Rd/Green Valley Road junction (DFG Site), 305-STRUV-21 - Struve Slough, 305-STRUV-22 - Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 5/17/2003-5/6/2006. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 17873
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 12
Number of Exceedances: | 8
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Monterey Area Research Consortium (R3_MARC) data for Struve Slough to determine beneficial use support and results are as follows: 8 of 12 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: Marc Los Huertos Water Quality Data, file A
| Final Data File used for assessment: Marc Los Huertos Water Quality Data, file B
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, dissolved oxygen concentration shall not be reduced below 5.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ SS-LEE - Struve Slough at Lee Rd]
Temporal Representation: | Data was collected over the time period 2/22/2006-1/24/2007.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 12053
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 12
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Struve Slough to determine beneficial use support and results are as follows: 12 of 14 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 1/24/2005-3/16/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13631
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 5
Number of Exceedances: | 5
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Northern Area Ag-Waiver Monitoring (R3_CMPNorth) data for Struve Slough to determine beneficial use support and results are as follows: 5 of 5 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, dissolved oxygen concentration shall not be reduced below 5.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 2/21/2006-9/26/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 18075
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 21
Number of Exceedances: | 20
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Clean streams project) (R3_CLNStrm) data for Struve Slough to determine beneficial use support and results are as follows: 20 of 21 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, dissolved oxygen concentration shall not be reduced below 5.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 3 monitoring sites [ 305-STRUV-21 - Struve Slough, 305-WSTRU-21 - West Branch of Struve Slough at Harkins Slough Rd/Green Valley Road junction (DFG Site), 305-STRUV-22 - Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 5/13/2004-8/30/2004.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Data entry completed by volunteers. Multiple errors were identified in data and were flagged by RB staff (in communication with Clean Streams Program staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 11929
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 11
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Struve Slough to determine beneficial use support and results are as follows: 11 of 14 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, dissolved oxygen concentration shall not be reduced below 5.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 1/24/2005-3/16/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13632
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 5
Number of Exceedances: | 5
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Northern Area Ag-Waiver Monitoring (R3_CMPNorth) data for Struve Slough to determine beneficial use support and results are as follows: 5 of 5 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 2/21/2006-9/26/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 11114
Pollutant: | pH
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.2 of the Listing Policy. Eighteen lines of evidence are available in the administrative record to assess this pollutant. Based on section 3.2 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Twenty-seven of 99 samples exceeded the Warm Freshwater Habitat water quality objective and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 11114

LOE ID: | 17970
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 23
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Clean streams project) (R3_CLNStrm) data for Struve Slough to determine beneficial use support and results are as follows: 3 of 23 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 3 monitoring sites [ 305-STRUV-21 - Struve Slough, 305-WSTRU-21 - West Branch of Struve Slough at Harkins Slough Rd/Green Valley Road junction (DFG Site), 305-STRUV-22 - Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 5/13/2004-9/18/2004.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Data entry completed by volunteers. Multiple errors were identified in data and were flagged by RB staff (in communication with Clean Streams Program staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 17971
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 23
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Clean streams project) (R3_CLNStrm) data for Struve Slough to determine beneficial use support and results are as follows: 3 of 23 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 3 monitoring sites [ 305-STRUV-21 - Struve Slough, 305-WSTRU-21 - West Branch of Struve Slough at Harkins Slough Rd/Green Valley Road junction (DFG Site), 305-STRUV-22 - Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 5/13/2004-9/18/2004.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Data entry completed by volunteers. Multiple errors were identified in data and were flagged by RB staff (in communication with Clean Streams Program staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 17652
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 12
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Monterey Area Research Consortium (R3_MARC) data for Struve Slough to determine beneficial use support and results are as follows: 0 of 12 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Marc Los Huertos Water Quality Data, file A
| Final Data File used for assessment: Marc Los Huertos Water Quality Data, file B
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ SS-LEE - Struve Slough at Lee Rd]
Temporal Representation: | Data was collected over the time period 2/22/2006-1/24/2007.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 17653
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 12
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Monterey Area Research Consortium (R3_MARC) data for Struve Slough to determine beneficial use support and results are as follows: 0 of 12 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Marc Los Huertos Water Quality Data, file A
| Final Data File used for assessment: Marc Los Huertos Water Quality Data, file B
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ SS-LEE - Struve Slough at Lee Rd]
Temporal Representation: | Data was collected over the time period 2/22/2006-1/24/2007.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 19049
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 12
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Struve Slough to determine beneficial use support and results are as follows: 0 of 12 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 3 monitoring sites [ 305-WSTRU-21 - West Branch of Struve Slough at Harkins Slough Rd/Green Valley Road junction (DFG Site), 305-STRUV-21 - Struve Slough, 305-STRUV-22 - Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 5/17/2003-5/6/2006. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 19050
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 12
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Struve Slough to determine beneficial use support and results are as follows: 0 of 12 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 3 monitoring sites [ 305-WSTRU-21 - West Branch of Struve Slough at Harkins Slough Rd/Green Valley Road junction (DFG Site), 305-STRUV-21 - Struve Slough, 305-STRUV-22 - Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 5/17/2003-5/6/2006. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 19051
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 12
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Struve Slough to determine beneficial use support and results are as follows: 3 of 12 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 3 monitoring sites [ 305-WSTRU-21 - West Branch of Struve Slough at Harkins Slough Rd/Green Valley Road junction (DFG Site), 305-STRUV-21 - Struve Slough, 305-STRUV-22 - Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 5/17/2003-5/6/2006. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 17986
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 23
Number of Exceedances: | 8
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Clean streams project) (R3_CLNStrm) data for Struve Slough to determine beneficial use support and results are as follows: 8 of 23 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 3 monitoring sites [ 305-STRUV-21 - Struve Slough, 305-WSTRU-21 - West Branch of Struve Slough at Harkins Slough Rd/Green Valley Road junction (DFG Site), 305-STRUV-22 - Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 5/13/2004-9/18/2004.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Data entry completed by volunteers. Multiple errors were identified in data and were flagged by RB staff (in communication with Clean Streams Program staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 13663
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 33
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Central Coast Watershed Studies (R3_CCOWS) data for Struve Slough to determine beneficial use support and results are as follows: 1 of 33 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCoWS (Central Coast Watershed Studies) Water Quality Data
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 3 monitoring sites [ Cherry Blossom Dr; site coordinates done with spatial data editor in TNTmips because field GPS coordinates were not very accurate, Harkins Slough Rd., Lee Rd]
Temporal Representation: | Data was collected over the time period 2/18/2003-7/16/2003.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Data quality is good and Standard Operating Procedures are well documented in QAPP. However, data documentation is poor and replicate samples and other quality assurance measurements are not consistently documented in this data set.
QAPP Information Reference(s):
LOE ID: | 17667
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 12
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Monterey Area Research Consortium (R3_MARC) data for Struve Slough to determine beneficial use support and results are as follows: 4 of 12 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Marc Los Huertos Water Quality Data, file A
| Final Data File used for assessment: Marc Los Huertos Water Quality Data, file B
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ SS-LEE - Struve Slough at Lee Rd]
Temporal Representation: | Data was collected over the time period 2/22/2006-1/24/2007.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 13661
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 33
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Central Coast Watershed Studies (R3_CCOWS) data for Struve Slough to determine beneficial use support and results are as follows: 0 of 33 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCoWS (Central Coast Watershed Studies) Water Quality Data
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 3 monitoring sites [ Cherry Blossom Dr; site coordinates done with spatial data editor in TNTmips because field GPS coordinates were not very accurate, Harkins Slough Rd., Lee Rd]
Temporal Representation: | Data was collected over the time period 2/18/2003-7/16/2003.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Data quality is good and Standard Operating Procedures are well documented in QAPP. However, data documentation is poor and replicate samples and other quality assurance measurements are not consistently documented in this data set.
QAPP Information Reference(s):
LOE ID: | 13635
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 5
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Northern Area Ag-Waiver Monitoring (R3_CMPNorth) data for Struve Slough to determine beneficial use support and results are as follows: 2 of 5 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 2/21/2006-9/26/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13634
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 5
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Northern Area Ag-Waiver Monitoring (R3_CMPNorth) data for Struve Slough to determine beneficial use support and results are as follows: 0 of 5 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 2/21/2006-9/26/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13633
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 5
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Northern Area Ag-Waiver Monitoring (R3_CMPNorth) data for Struve Slough to determine beneficial use support and results are as follows: 0 of 5 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 2/21/2006-9/26/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11258
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 14
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Struve Slough to determine beneficial use support and results are as follows: 1 of 14 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 1/24/2005-3/16/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11257
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 14
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Struve Slough to determine beneficial use support and results are as follows: 1 of 14 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 1/24/2005-3/16/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11259
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 9
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Struve Slough to determine beneficial use support and results are as follows: 9 of 14 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 1/24/2005-3/16/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13662
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 33
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Central Coast Watershed Studies (R3_CCOWS) data for Struve Slough to determine beneficial use support and results are as follows: 0 of 33 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCoWS (Central Coast Watershed Studies) Water Quality Data
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 3 monitoring sites [ Cherry Blossom Dr; site coordinates done with spatial data editor in TNTmips because field GPS coordinates were not very accurate, Harkins Slough Rd., Lee Rd]
Temporal Representation: | Data was collected over the time period 2/18/2003-7/16/2003.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Data quality is good and Standard Operating Procedures are well documented in QAPP. However, data documentation is poor and replicate samples and other quality assurance measurements are not consistently documented in this data set.
QAPP Information Reference(s):

DECISION ID | 15878
Pollutant: | Pathogens
Final Listing Decision: | List on 303(d) list (being addressed by USEPA approved TMDL)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
TMDL Name: | Watsonville Slough Pathogen
TMDL Project Code: | 35
Date TMDL Approved by USEPA: | 07/19/2007
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | A TMDL has been approved by USEPA (July 19, 2007) for pathogens in Watsonville Slough and four of its tributaries (specifically, Struve Slough). Struve Slough was not specifically identified on the 2006 Section 303(d) list for this pollutant but was included in the TMDL because it is impaired and the source controls are overlapping. This pollutant is being considered for removal from the section 303(d) list under section 4.3 of the Listing Policy. Under this section a single line of evidence is necessary to assess listing status. Twelve lines of evidence are available in the administrative record to assess this pollutant. Thirty-nine of the 89 samples exceed the Evaluation Guideline (USEPA Ambient Water Quality Criteria for Bacteria, 1986) as it applies to the Water Contact Recreation beneficial use. In addition, 34 of the 71 Fecal Coliform samples exceed the water quality objective for Water Contact Recreation. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against removing this water segment-pollutant combination from the section 303(d) list. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Thirty-nine of the 89 samples exceed the Evaluation Guideline (USEPA Ambient Water Quality Criteria for Bacteria, 1986) as it applies to the Water Contact Recreation beneficial use. In addition, 34 of the 71 Fecal Coliform samples exceed the water quality objective for Water Contact Recreation. Each of these exceeds the allowable frequency calculated from the equation in Table 4.2 of the Listing Policy. 4. Pursuant to section 4.11 of the Listing Policy, no additional data and information are available indicating that standards are met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list (being addressed by USEPA approved TMDL) because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15878

LOE ID: | 18494
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 9
Number of Exceedances: | 1
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Struve Slough to determine beneficial use support and results are as follows: 1 of 9 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | USEPA Ambient Water Quality Criteria for Bacteria -1986.
Objective/Criterion Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | Single sample maximum allowable density for E. coli in freshwater is 235 MPN/100mL (as stated in Table 4, page 15)
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 3 monitoring sites [ 305-WSTRU-21 - West Branch of Struve Slough at Harkins Slough Rd/Green Valley Road junction (DFG Site), 305-STRUV-21 - Struve Slough, 305-STRUV-22 - Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 5/17/2003-5/7/2005. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 18509
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 9
Number of Exceedances: | 0
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Struve Slough to determine beneficial use support and results are as follows: 0 of 9 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml. E. coli is a fecal coliform.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 3 monitoring sites [ 305-WSTRU-21 - West Branch of Struve Slough at Harkins Slough Rd/Green Valley Road junction (DFG Site), 305-STRUV-21 - Struve Slough, 305-STRUV-22 - Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 5/17/2003-5/7/2005. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 13776
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 57
Number of Exceedances: | 14
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Central Coast Watershed Studies (R3_CCOWS) data for Struve Slough to determine beneficial use support and results are as follows: 14 of 57 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCoWS (Central Coast Watershed Studies) Water Quality Data
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 9 monitoring sites [ Lee Rd, near Cherry Blossom Drive, near Cherry Blossom Drive, near Cherry Blossom Drive, Cherry Blossom Dr; site coordinates done with spatial data editor in TNTmips because field GPS coordinates were not very accurate, Cherry Blossom Road, Cherry Blossom Drive; site coordinates done with spatial data editor in TNTmips because field GPS coordinates were not very accurate, Airport Boulevard, Harkins Slough Rd.]
Temporal Representation: | Data was collected over the time period 2/18/2003-12/9/2003.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Data quality is good and Standard Operating Procedures are well documented in QAPP. However, data documentation is poor and replicate samples and other quality assurance measurements are not consistently documented in this data set.
QAPP Information Reference(s):
LOE ID: | 18521
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 4
Number of Exceedances: | 3
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Clean streams project) (R3_CLNStrm) data for Struve Slough to determine beneficial use support and results are as follows: 3 of 4 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | USEPA Ambient Water Quality Criteria for Bacteria -1986.
Objective/Criterion Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | Single sample maximum allowable density for E. coli in freshwater is 235 MPN/100mL (as stated in Table 4, page 15)
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 2 monitoring sites [ 305-WSTRU-21 - West Branch of Struve Slough at Harkins Slough Rd/Green Valley Road junction (DFG Site), 305-STRUV-21 - Struve Slough]
Temporal Representation: | Data was collected over the time period 5/26/2004-7/6/2004.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Data entry completed by volunteers. Multiple errors were identified in data and were flagged by RB staff (in communication with Clean Streams Program staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 11238
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Struve Slough to determine beneficial use support and results are as follows: 0 of 14 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 1/24/2005-3/16/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11237
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 14
Number of Exceedances: | 2
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Struve Slough to determine beneficial use support and results are as follows: 2 of 14 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 200 MPN/100 ml, nor shall more than ten percent of total samples during any 30-day period exceed 400 MPN/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 1/24/2005-3/16/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11256
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Struve Slough to determine beneficial use support and results are as follows: 0 of 14 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml. E. coli is a fecal coliform.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 1/24/2005-3/16/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14058
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 57
Number of Exceedances: | 32
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Central Coast Watershed Studies (R3_CCOWS) data for Struve Slough to determine beneficial use support and results are as follows: 32 of 57 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCoWS (Central Coast Watershed Studies) Water Quality Data
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 200 MPN/100 ml, nor shall more than ten percent of total samples during any 30-day period exceed 400 MPN/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 9 monitoring sites [ Lee Rd, near Cherry Blossom Drive, near Cherry Blossom Drive, near Cherry Blossom Drive, Cherry Blossom Dr; site coordinates done with spatial data editor in TNTmips because field GPS coordinates were not very accurate, Cherry Blossom Road, Cherry Blossom Drive; site coordinates done with spatial data editor in TNTmips because field GPS coordinates were not very accurate, Airport Boulevard, Harkins Slough Rd.]
Temporal Representation: | Data was collected over the time period 2/18/2003-12/9/2003.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Data quality is good and Standard Operating Procedures are well documented in QAPP. However, data documentation is poor and replicate samples and other quality assurance measurements are not consistently documented in this data set.
QAPP Information Reference(s):
LOE ID: | 11255
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 14
Number of Exceedances: | 2
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Pajaro (Pajaro) data for Struve Slough to determine beneficial use support and results are as follows: 2 of 14 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | USEPA Ambient Water Quality Criteria for Bacteria -1986.
Objective/Criterion Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | Single sample maximum allowable density for E. coli in freshwater is 235 MPN/100mL (as stated in Table 4, page 15)
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 1 monitoring site [ 305STL-Struve Slough at Lee Road]
Temporal Representation: | Data was collected over the time period 1/24/2005-3/16/2006. Pajaro watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13656
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 62
Number of Exceedances: | 11
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Central Coast Watershed Studies (R3_CCOWS) data for Struve Slough to determine beneficial use support and results are as follows: 11 of 62 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: CCoWS (Central Coast Watershed Studies) Water Quality Data
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml. E. coli is a fecal coliform.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 9 monitoring sites [ Lee Rd, near Cherry Blossom Drive, near Cherry Blossom Drive, near Cherry Blossom Drive, Cherry Blossom Dr; site coordinates done with spatial data editor in TNTmips because field GPS coordinates were not very accurate, Cherry Blossom Road, Cherry Blossom Drive; site coordinates done with spatial data editor in TNTmips because field GPS coordinates were not very accurate, Airport Boulevard, Harkins Slough Rd.]
Temporal Representation: | Data was collected over the time period 2/18/2003-12/9/2003.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Data quality is good and Standard Operating Procedures are well documented in QAPP. However, data documentation is poor and replicate samples and other quality assurance measurements are not consistently documented in this data set.
QAPP Information Reference(s):
LOE ID: | 13655
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 62
Number of Exceedances: | 33
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Central Coast Watershed Studies (R3_CCOWS) data for Struve Slough to determine beneficial use support and results are as follows: 33 of 62 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: CCoWS (Central Coast Watershed Studies) Water Quality Data
Water Quality Objective/Criterion: | USEPA Ambient Water Quality Criteria for Bacteria -1986.
Objective/Criterion Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | Single sample maximum allowable density for E. coli in freshwater is 235 MPN/100mL (as stated in Table 4, page 15)
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 9 monitoring sites [ Lee Rd, near Cherry Blossom Drive, near Cherry Blossom Drive, near Cherry Blossom Drive, Cherry Blossom Dr; site coordinates done with spatial data editor in TNTmips because field GPS coordinates were not very accurate, Cherry Blossom Road, Cherry Blossom Drive; site coordinates done with spatial data editor in TNTmips because field GPS coordinates were not very accurate, Airport Boulevard, Harkins Slough Rd.]
Temporal Representation: | Data was collected over the time period 2/18/2003-12/9/2003.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Data quality is good and Standard Operating Procedures are well documented in QAPP. However, data documentation is poor and replicate samples and other quality assurance measurements are not consistently documented in this data set.
QAPP Information Reference(s):
LOE ID: | 18522
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 4
Number of Exceedances: | 0
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Clean streams project) (R3_CLNStrm) data for Struve Slough to determine beneficial use support and results are as follows: 0 of 4 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml. E. coli is a fecal coliform.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Struve Slough was collected at 2 monitoring sites [ 305-WSTRU-21 - West Branch of Struve Slough at Harkins Slough Rd/Green Valley Road junction (DFG Site), 305-STRUV-21 - Struve Slough]
Temporal Representation: | Data was collected over the time period 5/26/2004-7/6/2004.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Data entry completed by volunteers. Multiple errors were identified in data and were flagged by RB staff (in communication with Clean Streams Program staff) prior to assessment of data.
QAPP Information Reference(s):