# Draft 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 3 - Central Coast Region

Water Body Name: | Blosser Channel
Water Body ID: | CAR3121003020011121135941
Water Body Type: | River & Stream

DECISION ID | 16064
Pollutant: | Chlorophyll-a
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. None of the 11 samples exceed the Evaluation Guideline (North Carolina Administrative code, Title 15A) and the General Water Quality Objective set to protect aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 26 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of the 11 samples exceed the Evaluation Guideline (North Carolina Administrative code, Title 15A) and the General Water Quality Objective set to protect aquatic life beneficial uses and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16064

LOE ID: | 10101
Pollutant: | Chlorophyll-a
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 11
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 0 of 11 samples exceed the criterion for Chlorophyll a.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Evaluation Guideline: | North Carolina Administrative code (NCAC), Title 15A - Environmental and Natural Resources, Subchapter 2B-Surface water and wetland standards, Rule 0211-Fresh surface water quality standards for class C waters (Class C is defined as freshwaters protected for secondary recreation, fishing, aquatic life including propagation and survival, and wildlife). Section 3(a) of Rule 0211 applies to all fresh surface waters and states that chlorophyll a is not to exceed 40 ug/L.
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 10102
Pollutant: | Chlorophyll-a
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 11
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 0 of 11 samples exceed the criterion for Chlorophyll a.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Evaluation Guideline: | North Carolina Administrative code (NCAC), Title 15A - Environmental and Natural Resources, Subchapter 2B-Surface water and wetland standards, Rule 0211-Fresh surface water quality standards for class C waters (Class C is defined as freshwaters protected for secondary recreation, fishing, aquatic life including propagation and survival, and wildlife). Section 3(a) of Rule 0211 applies to all fresh surface waters and states that chlorophyll a is not to exceed 40 ug/L.
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 16066
Pollutant: | Chlorpyrifos
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. The single sample did exceed the Evaluation Guideline (Sipmann and Finlayson, 2000) applied to protect for aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. The single sample did exceed the Evaluation Guideline (Sipmann and Finlayson, 2000) applied to protect for aquatic life beneficial uses and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded and the sample size is insufficient to determine with the power and confidence of the Listing Policy if water quality standards are met or exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16066

LOE ID: | 16221
Pollutant: | Chlorpyrifos
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (04SW3001) data for Blosser Channel to determine beneficial use support and results are as follows: 1 of 1 samples exceed the criterion for Chlorpyrifos.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
| Final Data File used for assessment: SWAMP Sediment Chemistry Data from Region 3 Harbors, 2004
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | One hour average maximum concentration 0.025 ug/L as stated in Sipmann and Finlayson (2000).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected on a single day 2/27/2007. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16222
Pollutant: | Chlorpyrifos
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (04SW3001) data for Blosser Channel to determine beneficial use support and results are as follows: 1 of 1 samples exceed the criterion for Chlorpyrifos.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
| Final Data File used for assessment: SWAMP Sediment Chemistry Data from Region 3 Harbors, 2004
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | One hour average maximum concentration 0.025 ug/L as stated in Sipmann and Finlayson (2000).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected on a single day 2/27/2007. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 16067
Pollutant: | Diazinon
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. The single sample did exceed the Evaluation Guideline (Sipmann and Finlayson, 2000) applied to protect for aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. The single sample did exceed the Evaluation Guideline (Sipmann and Finlayson, 2000) applied to protect for aquatic life beneficial uses and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded and the sample size is insufficient to determine with the power and confidence of the Listing Policy if water quality standards are met or exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16067

LOE ID: | 16612
Pollutant: | Diazinon
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (04SW3001) data for Blosser Channel to determine beneficial use support and results are as follows: 1 of 1 samples exceed the criterion for Diazinon.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
| Final Data File used for assessment: SWAMP Sediment Chemistry Data from Region 3 Harbors, 2004
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | One hour average maximum concentration 0.16 ug/L as stated in Sipmann and Finlayson (2000).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected on a single day 2/27/2007. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 16625
Pollutant: | Diazinon
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (04SW3001) data for Blosser Channel to determine beneficial use support and results are as follows: 1 of 1 samples exceed the criterion for Diazinon.
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
| Final Data File used for assessment: SWAMP Sediment Chemistry Data from Region 3 Harbors, 2004
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | One hour average maximum concentration 0.16 ug/L as stated in Sipmann and Finlayson (2000).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected on a single day 2/27/2007. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 11042
Pollutant: | Low Dissolved Oxygen
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Three water quality objectives are assessed: Two of the 14 samples exceed the water quality objective for Cold Freshwater Habitat. One of the 14 samples exceed the water quality objective for Warm Freshwater Habitat. In addition, 4 of 14 samples exceed the general water quality objective for oxygen saturation (when applied as a single sample maximum). The range of dissolved oxygen measurements in the water segment was 1.60 mg/L to 18.3 mg/L. However, the Basin Plan objective states that the median oxygen saturation value shall not fall below 85% and the median value did not exceed this criterion. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 26 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Two of the 14 samples exceed the water quality objective for Cold Freshwater Habitat. One of the 14 samples exceed the water quality objective for Warm Freshwater Habitat and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. In addition, the median value did not exceed the General Objective. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 11042

LOE ID: | 13599
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 11
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 0 of 11 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, dissolved oxygen concentration shall not be reduced below 5.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13600
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 11
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 1 of 11 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13601
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 11
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 1 of 11 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13598
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 11
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 0 of 11 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13622
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 3
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Blosser Channel to determine beneficial use support and results are as follows: 3 of 3 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 6/27/2000-9/6/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13620
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 3
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Blosser Channel to determine beneficial use support and results are as follows: 2 of 3 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 6/27/2000-9/6/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13347
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 3
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Blosser Channel to determine beneficial use support and results are as follows: 3 of 3 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 6/27/2000-9/6/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13621
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 3
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Blosser Channel to determine beneficial use support and results are as follows: 1 of 3 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, dissolved oxygen concentration shall not be reduced below 5.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 6/27/2000-9/6/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 11039
Pollutant: | Nitrogen, ammonia (Total Ammonia)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. None of the 11 samples exceed the Evaluation Guideline set to protect for Municipal and Domestic Supply. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of the 11 samples exceed the Evaluation Guideline set to protect for Municipal and Domestic Supply and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 11039

LOE ID: | 10086
Pollutant: | Ammonia as Nitrogen
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 11
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 0 of 11 samples exceed the criterion for Ammonia as N, Total.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | USEPA Health Advisory 2006 Edition of the Drinking Water Standards and Health Advisories (EPA 822-R-06-013, 2006).
Objective/Criterion Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Evaluation Guideline: | EPA's Lifetime Health advisory level for total ammonia is 30.0 mg/L as stated on page 8 of the 2006 edition of the drinking water standards and health advisories. This Advisory Level is defined as "the concentration of a chemical in drinking water that is not expected to cause any adverse noncarcinogenic effects for up to ten days of exposure."
Guideline Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 11043
Pollutant: | Temperature, water
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. Three of the 14 samples exceed the Evaluation Guideline set to protect Cold Freshwater Habitat. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 26 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Three of the 14 samples exceed the Evaluation Guideline set to protect Cold Freshwater Habitat and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 11043

LOE ID: | 13619
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 11
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 3 of 11 samples exceed the criterion for Water Temperature.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Board that such alteration in temperature does not adversely affect beneficial uses (General Objective in Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Inland Fishes of California (Moyle 1976) states that for rainbow trout the optimum range for growth and completion of most life stages is 13-21 degrees C (page 129).
Guideline Reference: | Inland Fishes of California
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13350
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 3
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Blosser Channel to determine beneficial use support and results are as follows: 0 of 3 samples exceed the criterion for Water Temperature.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Board that such alteration in temperature does not adversely affect beneficial uses (General Objective in Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Inland Fishes of California (Moyle 1976) states that for rainbow trout the optimum range for growth and completion of most life stages is 13-21 degrees C (page 129).
Guideline Reference: | Inland Fishes of California
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 6/27/2000-9/6/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 16065
Pollutant: | Turbidity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Two of the 8 samples exceed the Evaluation Guideline (Sigler et al., 1984) applied to protect for aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 26 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Two of the 8 samples exceed the Evaluation Guideline (Sigler et al., 1984) applied to protect for aquatic life beneficial uses and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16065

LOE ID: | 13618
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 6
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 2 of 6 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 9/6/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13348
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Blosser Channel to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 6/27/2000-9/6/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13349
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Blosser Channel to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 6/27/2000-9/6/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13602
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 6
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 2 of 6 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 9/6/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 4719
Pollutant: | Ammonia (Unionized)
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)(2006)
Revision Status | Revised
Sources: | Agriculture | Groundwater Withdrawal | Intensive Animal Feeding Operations | Urban Runoff/Storm Sewers
Expected TMDL Completion Date: | 2013
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. In 2004, Regional Board staff recommended against placing this water segment-pollutant combination of the Section 303(d) list because at that time the channel was being modified and it was not known if the channel would be reconstructed to flow to the Santa Maria River again. Now reconstructed, Blosser Channel conveys water from a storm water channel that parallels Blosser Road and the by-pass channel along Canal Street to the Santa Maria River. This storm water channel is typically dry (between W. Fester Street and near Canal Street) unless there is storm water runoff or discharge from ground water pumping (near Donovan Street). Lower Blosser channel also receives discharge from a retention pond (located on Blosser Road) as well as year round flow from the bi-pass channel. The Blosser Channe/Bi-pass Channel confluence is just downstream of the intersection of Blosser Road and Canal Street. The CCAMP monitoring site is located on Blosser Channel, below Canal Street and therefore is representative of Blosser Channel discharge to Santa Maria River. Three lines of evidence are available in the administrative record to assess this pollutant. Two of these LOEs contain the same data (LOEs #1920 and #10088) and are functionally duplicates and are not double counted here. Three of 11 samples exceed the General water quality Objective set to protect for aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is insufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Three of 11 samples exceed the General water quality Objective set to protect for aquatic life beneficial uses and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 4719

LOE ID: | 1920
Pollutant: | Ammonia (Unionized)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 11
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Three of 11 data points exceed the water quality objective (CCAMP, 2004; SWAMP, 2004).
Data Reference: | Placeholder reference 2006 303(d)
Water Quality Objective/Criterion: | The discharge of wastes shall not cause concentrations of unionized ammonia (NH3) to exceed 0.025 mg/L (as N) in receiving waters (Region 3 Basin Plan, Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a. General Objectives, page III-4).
Objective/Criterion Reference: | Placeholder reference 2006 303(d)
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data were collected at site 312BCD on Blosser Channel, in Santa Barbara County. This data represents only the retention pond overflow as the upstream channel was dry most of the year.
Temporal Representation: | Samples were collected from May 2000 to February 2001. All 3 exceedances of the objective were during summer months when flows were primarily from the retention basin overflow. Since 2002 a new housing development is being built at the site location and the retention basin has been drained since 2004.
Environmental Conditions: | The waterbody is located in the Santa Maria hydrologic unit, Guadalupe hydrologic area, Guadalupe hydrologic subarea. The monitoring site is located at Blosser Channel downstream of groundwater recharge ponds (312BCD). In 2000 this site was downstream of a storm water channel and the discharge from groundwater recharge ponds. As of 2003 a housing development is underway and this site will be completely converted to storm water channel after the projects completion.
QAPP Information: | CCAMP and SWAMP QAPP.Samples were taken according to CCAMP protocols.
QAPP Information Reference(s):
LOE ID: | 10088
Pollutant: | Ammonia (Unionized)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 11
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 3 of 11 samples exceed the criterion for Ammonia as N, Unionized.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin General Objective, Chapter III, Section II.A.2 (General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries) states that the discharge of wastes shall not cause concentrations of unionized ammonia (NH3) to exceed 0.025 mg/l (as N) in receiving waters (page III-4) .
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 10087
Pollutant: | Ammonia (Unionized)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 11
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 3 of 11 samples exceed the criterion for Ammonia as N, Unionized.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin General Objective, Chapter III, Section II.A.2 (General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries) states that the discharge of wastes shall not cause concentrations of unionized ammonia (NH3) to exceed 0.025 mg/l (as N) in receiving waters (page III-4) .
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 4297
Pollutant: | Fecal Coliform
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | Delist from 303(d) list (TMDL required list)(2006)
Revision Status | Revised
Sources: | Agriculture | Groundwater Withdrawal | Intensive Animal Feeding Operations | Natural Sources | Urban Runoff/Storm Sewers
Expected TMDL Completion Date: | 2013
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.3 of the Listing Policy. Note that in 2006, this waterbody was removed from the Section 303(d) list of impaired waters because "... data represents only the retention pond overflow as the up stream channel was dry most of the year. The original listing was faulty. Data were not representative of ambient water quality. " However, staff now know that these data represent the combination of storm water discharges and the By-pass Channel between groundwater retention basins. The CCAMP monitoring site is located downstream of the confluence of the By-pass Channel and Blosser Channel and is representative of the water quality that is discharged to the Santa Maria River. Therefore, this data is representative of the conditions of lower Blosser Channel and should result in a new listing. Three lines of evidence are available in the administrative record to assess this pollutant. LOE #1921 is disregarded and replaced by LOE #11764 because all of the data in LOE #1921 is contained in LOE #11764 and LOE #11764 contains one additional data point. Based on section 3.3 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Six of 11 samples exceeded the water quality objective for Water Body Contact and this supports rejection of the null hypothesis. However, 2 of 11 samples exceeded the water quality objective for Non-Contact Recreation, so this beneficial use is not considered impaired. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Six of 11 samples exceeded the Water Contact Recreation water quality objective and this meets or exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: | After review of the available data and information, SWRCB staff concludes that the water body-pollutant combination should be removed from the section 303(d) list because the original listing was faulty.
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 4297

LOE ID: | 1921
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 10
Number of Exceedances: | 5
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Five of 10 samples exceed the water quality objectives (CCAMP, 2004).
Data Reference: | Placeholder reference 2006 303(d)
Water Quality Objective/Criterion: | Basin Plan: Fecal coliform concentration, based on minimum of not less than five samples or any 30-day period, shall not exceed a log mean of 200/100 ml, nor shall more than ten percent of the total samples during any 30-day period exceed 400/100 ml.
Objective/Criterion Reference: | Placeholder reference 2006 303(d)
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | There was one sampling site. This data represents only the retention pond overflow as the upstream channel was dry most of the year.
Temporal Representation: | There were monthly sampling events. All 3 exceedances of the objective were during summer months when flows were primarily from the retention basin overflow. Since 2002 a new housing development is being built at the site location and the retention basin has been drained (since 2004).
Environmental Conditions: |
QAPP Information: | CCAMP
QAPP Information Reference(s):
LOE ID: | 11764
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 11
Number of Exceedances: | 6
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 6 of 11 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 200 MPN/100 ml, nor shall more than ten percent of total samples during any 30-day period exceed 400 MPN/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11780
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 11
Number of Exceedances: | 2
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 2 of 11 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 11041
Pollutant: | Nitrate
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture | Groundwater Loadings | Urban Runoff/Storm Sewers
Expected TMDL Completion Date: | 2013
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Three lines of evidence are available in the administrative record to assess this pollutant. One of the 11 samples exceed the water quality objective for Municipal and Domestic Supply. There is not enough evidence to show that this beneficial use is impaired. However, 10 of the 11 samples exceeded the Evaluation Guideline for Nitrate established for aquatic life beneficial uses using the Numeric Nutrient Endpoint tool and this exceeds the allowable frequency as stated in table 3.1 of the Listing Policy. Nitrate concentrations in Blosser Channel ranged from non-detect (<0.02 mg/L) to 12.40 mg/L. The following, is additional supporting exidence of a biostimulatory problem in Blosser Channel: 1) Dissolved oxygen measurements ranged from 1.6 mg/L to 18.3 mg/L, exceeding both Warm and Cold water quality objectives. In addition, this waterbody exceeds the upper dissolved oxygen limit established for both Cold and Warm water Beneficial Uses is 13.0 mg/L (NNE Technical Report, 2009). 2) Using CCAMP data, the California Benthic Biomass Tool, v. 13 (Tetratech, 2007) predicted a benthic algal contribution to oxygen deficit for this water body of 2.72 mg/L DO exceeding the maximum benthic algal contribution to oxygen deficit established by Central Coast staff of 1.25 mg/L (NNE Technical Report, 2009). 3) The Biomass Tool (revised QUAL2K model, using CCAMP data) predicted algae biomass of 63 g/m2 ash-free dry weight (AFDW). This exceeds the Californias Nutrient Numeric Endpoints (Creager, et al., 2006) which established Cold and Warm water threshold values of 60 grams/m2 and 80 grams/m2, respectively. 4) The Biomass Tool also predicted benthic chlorophyll a concentration of 158 mg/m2. This exceeds the Cold water threshold value established in Californias Nutrient Numeric Endpoints (Creager, et al., 2006) of 150 mg/m2 but not the Warm water threshold values of 200 mg/m2. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification for placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Ten of the 11 samples exceeded the Evaluation Guideline for Nitrate established for aquatic life beneficial uses using the Numeric Nutrient Endpoint tool and this exceeds the allowable frequency as stated in table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 11041

LOE ID: | 10103
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 11
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 1 of 11 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin Objective for municipal and domestic supply uses of inland surface waters (Section II.A.2) states the following: waters shall not contain concentrations of chemical constituents in excess of the limits specified in California Code of Regulations, Title 22, Article 4, Chapter 15, Section 64435, Tables 2 and 3 as listed in Table 3-2. The maximum contaminant level listed in Table 3-2 (inorganic and fluoride concentrations not to be exceeded in domestic or municipal supply) for nitrate is 10.0 mg/L (NO3 as N).
Objective/Criterion Reference: | Title 22, Division 4, Ch. 15, Article 4, Section 64431, Table 64431-A
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 27853
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 11
Number of Exceedances: | 10
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Data for this assessment unit was collected by one monitoring project: CCAMP Santa Maria (SantaMaria)
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Technical approach to develop nutrient numeric endpoints for California, Tetra Tech, June 2006. The Central Coast Region numeric target for maximum nitrate concentration is based on the Tetra Tech NNE (Nutrient Numeric Endpoint) Model and CCAMP data for 193 sites, monitored monthly for at least 1 year between January 1998 and December 2006. The model numeric target for aquatic life habitats in the Central Coast Region is 1.0 mg/L Nitrate as N.
Guideline Reference: | Technical Approach to Develop Nutrient Numeric Endpoints for California
| Technical Paper - Interpreting Narrative Objectives for Biostimulatory Substances Using the Technical Approach for Developing California Nutrient Numeric Endpoints. Central Coast Region
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 27854
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 11
Number of Exceedances: | 10
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Data for this assessment unit was collected by one monitoring project: CCAMP Santa Maria (SantaMaria)
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Technical approach to develop nutrient numeric endpoints for California, Tetra Tech, June 2006. The Central Coast Region numeric target for maximum nitrate concentration is based on the Tetra Tech NNE (Nutrient Numeric Endpoint) Model and CCAMP data for 193 sites, monitored monthly for at least 1 year between January 1998 and December 2006. The model numeric target for aquatic life habitats in the Central Coast Region is 1.0 mg/L Nitrate as N.
Guideline Reference: | Technical Approach to Develop Nutrient Numeric Endpoints for California
| Technical Paper - Interpreting Narrative Objectives for Biostimulatory Substances Using the Technical Approach for Developing California Nutrient Numeric Endpoints. Central Coast Region
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 16068
Pollutant: | Unknown Toxicity
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture | Groundwater Withdrawal | Intensive Animal Feeding Operations | Urban Runoff/Storm Sewers
Expected TMDL Completion Date: | 2013
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 and section 3.6 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Six lines of evidence are available in the administrative record to assess this pollutant in water samples. Two of the 3 samples were toxic to test organisms (exhibited a significant increase in mortality or decrease in cell density compared to the laboratory control) and therefore exceed the narrative General Objective for toxicity, set to protect for aquatic life beneficial uses. The following is a summary of the results from individual toxicity tests. The single sample (tested for toxicity to plants) exhibited significant reduction in cell density relative to the control. In addition, the single sample tested for toxicity to invertebrate test organisms exhibited a significant increase in mortality compared to the laboratory control. However the single sample (tested for toxicity to vertebrate test organisms) did not exhibit a significant increase in mortality compared to the laboratory control. Two of the three samples were toxic to test organisms and therefore, based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Two of the three samples were toxic to test organisms. The single sample (tested for toxicity to plants) exhibited significant reduction in cell density relative to the control. In addition, the single sample tested for toxicity to invertebrate test organisms exhibited a significant increase in mortality compared to the laboratory control. Therefore, this exceeds the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16068

LOE ID: | 23657
Pollutant: | Plant Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 1
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (04SW3001) data for Blosser Channel to determine beneficial use support and results are as follows: 1 of 1 samples exceed the criterion for Toxicity, Selenastrum capricornutum Growth (Cell Density) 4 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction in cell count of test organism relative to the control (alpha < 0.05) and cell count <80% of control.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected on a single day 2/27/2007. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 23656
Pollutant: | Plant Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 1
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (04SW3001) data for Blosser Channel to determine beneficial use support and results are as follows: 1 of 1 samples exceed the criterion for Toxicity, Selenastrum capricornutum Growth (Cell Density) 4 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction in cell count of test organism relative to the control (alpha < 0.05) and cell count <80% of control.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds].
Temporal Representation: | Data was collected on a single day 2/27/2007. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 23655
Pollutant: | Vertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (04SW3001) data for Blosser Channel to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Toxicity, Pimephales promelas Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected on a single day 2/27/2007. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 23654
Pollutant: | Vertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (04SW3001) data for Blosser Channel to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Toxicity, Pimephales promelas Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected on a single day 2/27/2007. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 23651
Pollutant: | Invertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 1
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (04SW3001) data for Blosser Channel to determine beneficial use support and results are as follows: 1 of 1 samples exceed the criterion for Toxicity, Ceriodaphnia dubia Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected on a single day 2/27/2007. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 23629
Pollutant: | Invertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 1
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP_SWAMP Monitoring (04SW3001) data for Blosser Channel to determine beneficial use support and results are as follows: 1 of 1 samples exceed the criterion for Toxicity, Ceriodaphnia dubia Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: SWAMP Toxicity Data 2001-06
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected on a single day 2/27/2007. SWAMP toxicity monitoring includes both water samples (collected in both winter and summer) and sediment samples (collected in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 11044
Pollutant: | pH
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture | Groundwater Withdrawal | Urban Runoff/Storm Sewers
Expected TMDL Completion Date: | 2013
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Ten lines of evidence are available in the administrative record to assess this pollutant. Nine of 14 samples exceed the water quality objective for Cold and Warm Freshwater Habitat, Municipal & Domestic Supply, Non-Contact Recreation and Water Contact Recreation. The pH ranged between 7.51 - 9.17 in monthly monitoring at the CCAMP monitoring site. Super-saturated oxygen conditions and water temperature > 24 degrees co-occurred with the highest pH measurements. The conditions, along with elevated total ammonia concentrations directly contribute to the elevated unionized-ammonia levels in Blosser Channel. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Nine of 14 samples exceed the water quality objective for Cold and Warm Freshwater Habitat, Municipal & Domestic Supply, Non-Contact Recreation and Water Contact Recreation and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 11044

LOE ID: | 11781
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 11
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 6 of 11 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11782
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 11
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 6 of 11 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin, Section II.A.2. Municipal and Domestic Supply Objectives, Section II.A.2.a states the following: The pH value shall neither be depressed below 6.5 or raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11783
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 11
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 6 of 11 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11784
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 11
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 6 of 11 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11803
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 3
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Blosser Channel to determine beneficial use support and results are as follows: 3 of 3 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 6/27/2000-9/6/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11800
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 3
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Blosser Channel to determine beneficial use support and results are as follows: 3 of 3 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 6/27/2000-9/6/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11801
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 3
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Blosser Channel to determine beneficial use support and results are as follows: 3 of 3 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin, Section II.A.2. Municipal and Domestic Supply Objectives, Section II.A.2.a states the following: The pH value shall neither be depressed below 6.5 or raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 6/27/2000-9/6/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11802
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 3
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Blosser Channel to determine beneficial use support and results are as follows: 3 of 3 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 6/27/2000-9/6/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11818
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 3
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Blosser Channel to determine beneficial use support and results are as follows: 3 of 3 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 6/27/2000-9/6/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11799
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 11
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Blosser Channel to determine beneficial use support and results are as follows: 6 of 11 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Blosser Channel was collected at 1 monitoring site [ 312BCD-Blosser Channel d/s of groundwater recharge ponds]
Temporal Representation: | Data was collected over the time period 5/3/2000-2/28/2001. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):