# Draft 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 3 - Central Coast Region

Water Body Name: | Topo Creek
Water Body ID: | CAR3097007420080604164238
Water Body Type: | River & Stream

DECISION ID | 12781
Pollutant: | Chlorophyll-a
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. The single sample did not exceed the Evaluation Guideline (North Carolina Administrative code, Title 15A) and the General Water Quality Objective set to protect aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 26 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. The single sample did not exceed the Evaluation Guideline (North Carolina Administrative code, Title 15A) and the General Water Quality Objective set to protect aquatic life beneficial uses. The sample size is insufficient to determine with the power and confidence of the Listing Policy if water quality standards are being met. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because the sample size is insufficient to determine with the power and confidence of the Listing Policy if water quality standards are being met.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12781

LOE ID: | 10026
Pollutant: | Chlorophyll-a
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Topo Creek to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Chlorophyll a.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Evaluation Guideline: | North Carolina Administrative code (NCAC), Title 15A - Environmental and Natural Resources, Subchapter 2B-Surface water and wetland standards, Rule 0211-Fresh surface water quality standards for class C waters (Class C is defined as freshwaters protected for secondary recreation, fishing, aquatic life including propagation and survival, and wildlife). Section 3(a) of Rule 0211 applies to all fresh surface waters and states that chlorophyll a is not to exceed 40 ug/L.
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
Spatial Representation: | Data for this line of evidence for Topo Creek was collected at 1 monitoring site [ 309TOP-Topo Creek at Metz Road]
Temporal Representation: | Data was collected on a single day 2/2/1999. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 10025
Pollutant: | Chlorophyll-a
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Topo Creek to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Chlorophyll a.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Evaluation Guideline: | North Carolina Administrative code (NCAC), Title 15A - Environmental and Natural Resources, Subchapter 2B-Surface water and wetland standards, Rule 0211-Fresh surface water quality standards for class C waters (Class C is defined as freshwaters protected for secondary recreation, fishing, aquatic life including propagation and survival, and wildlife). Section 3(a) of Rule 0211 applies to all fresh surface waters and states that chlorophyll a is not to exceed 40 ug/L.
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
Spatial Representation: | Data for this line of evidence for Topo Creek was collected at 1 monitoring site [ 309TOP-Topo Creek at Metz Road]
Temporal Representation: | Data was collected on a single day 2/2/1999. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 11017
Pollutant: | Fecal Coliform
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. The single sample did not exceed the water quality objectives for Water Contact Recreation or Non-Contact Recreation. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. The single sample did not exceed the water quality objectives for Water Contact Recreation or Non-Contact Recreation, and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded and the sample size is insufficient to determine with the power and confidence of the Listing Policy if water quality standards are met or exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 11017

LOE ID: | 10842
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Topo Creek to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Topo Creek was collected at 1 monitoring site [ 309TOP-Topo Creek at Metz Road]
Temporal Representation: | Data was collected on a single day 2/2/1999. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 10841
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Topo Creek to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 200 MPN/100 ml, nor shall more than ten percent of total samples during any 30-day period exceed 400 MPN/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Topo Creek was collected at 1 monitoring site [ 309TOP-Topo Creek at Metz Road]
Temporal Representation: | Data was collected on a single day 2/2/1999. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 11019
Pollutant: | Nitrate
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. The single sample did not exceed the Municipal and Domestic Supply water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. The single sample did not exceed the Municipal and Domestic Supply water quality objective, and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded and the sample size is insufficient to determine with the power and confidence of the Listing Policy if water quality standards are met or exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 11019

LOE ID: | 10027
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Topo Creek to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin Objective for municipal and domestic supply uses of inland surface waters (Section II.A.2) states the following: waters shall not contain concentrations of chemical constituents in excess of the limits specified in California Code of Regulations, Title 22, Article 4, Chapter 15, Section 64435, Tables 2 and 3 as listed in Table 3-2. The maximum contaminant level listed in Table 3-2 (inorganic and fluoride concentrations not to be exceeded in domestic or municipal supply) for nitrate is 10.0 mg/L (NO3 as N).
Objective/Criterion Reference: | Title 22, Division 4, Ch. 15, Article 4, Section 64431, Table 64431-A
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Topo Creek was collected at 1 monitoring site [ 309TOP-Topo Creek at Metz Road]
Temporal Representation: | Data was collected on a single day 2/2/1999. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 11015
Pollutant: | Nitrogen, ammonia (Total Ammonia)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. The single sample did not exceed the exceed the Evaluation Guideline (EPA's Lifetime Health advisory level, 2006) applied to protect the Municipal & Domestic Supply beneficial use. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. The single sample did not exceed the exceed the Evaluation Guideline (EPA's Lifetime Health advisory level, 2006) applied to protect the Municipal & Domestic Supply beneficial use, and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded and the sample size is insufficient to determine with the power and confidence of the Listing Policy if water quality standards are met or exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 11015

LOE ID: | 10012
Pollutant: | Ammonia as Nitrogen
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Topo Creek to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Ammonia as N, Total.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | USEPA Health Advisory 2006 Edition of the Drinking Water Standards and Health Advisories (EPA 822-R-06-013, 2006).
Objective/Criterion Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Evaluation Guideline: | EPA's Lifetime Health advisory level for total ammonia is 30.0 mg/L as stated on page 8 of the 2006 edition of the drinking water standards and health advisories. This Advisory Level is defined as "the concentration of a chemical in drinking water that is not expected to cause any adverse noncarcinogenic effects for up to ten days of exposure."
Guideline Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Spatial Representation: | Data for this line of evidence for Topo Creek was collected at 1 monitoring site [ 309TOP-Topo Creek at Metz Road]
Temporal Representation: | Data was collected on a single day 2/2/1999. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):