# Draft 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 3 - Central Coast Region

Water Body Name: | Bradley Canyon Creek
Water Body ID: | CAR3121003020011121144840
Water Body Type: | River & Stream

DECISION ID | 4064
Pollutant: | Ammonia (Unionized)
Final Listing Decision: | Do Not Delist from 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | List on 303(d) list (TMDL required list)(2006)
Revision Status | Revised
Sources: | Agriculture
Expected TMDL Completion Date: | 2013
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for removal from the section 303(d) list under section 4.1 of the Listing Policy. Under this section a single line of evidence is necessary to assess listing status. Five lines of evidence are available in the administrative record to assess this pollutant. Eight of the 21 samples exceed the General water quality objective set to protect for aquatic life beneficial uses. Note that LOEs # 1922 and #9866 contains the same data and information. They are functionally duplicates and are not assessed twice. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against removing this water segment-pollutant combination from the section 303(d) list. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Eight of the 21 samples exceed the General water quality objective set to protect for aquatic life beneficial uses and this exceeds the allowable frequency calculated from the equation in Table 4.1 of the Listing Policy. 4. Pursuant to section 4.11 of the Listing Policy, no additional data and information are available indicating that standards are met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be removed from the section 303(d) list because applicable water quality standards for the pollutant are being exceeded.
SWRCB Board Decision / Staff Recommendation: | After review of the available data and information, SWRCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 4064

LOE ID: | 14563
Pollutant: | Ammonia (Unionized)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 5
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 5 of 14 samples exceed the criterion for Ammonia as N, Unionized.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin General Objective, Chapter III, Section II.A.2 (General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries) states that the discharge of wastes shall not cause concentrations of unionized ammonia (NH3) to exceed 0.025 mg/l (as N) in receiving waters (page III-4) .
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14564
Pollutant: | Ammonia (Unionized)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 5
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 5 of 14 samples exceed the criterion for Ammonia as N, Unionized.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin General Objective, Chapter III, Section II.A.2 (General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries) states that the discharge of wastes shall not cause concentrations of unionized ammonia (NH3) to exceed 0.025 mg/l (as N) in receiving waters (page III-4) .
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 1922
Pollutant: | Ammonia (Unionized)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 7
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Three out of seven samples exceeded the general water quality objective (CCAMP, 2004; SWAMP, 2004).
Data Reference: | Placeholder reference 2006 303(d)
Water Quality Objective/Criterion: | The discharge of wastes shall not cause concentrations of unionized ammonia (NH3) to exceed 0.025 mg/L (as N) in receiving waters (Region 3 Basin Plan, Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a. General Objectives, page III-4).
Objective/Criterion Reference: | Placeholder reference 2006 303(d)
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data were collected at site 312BCF on Bradley Canyon Creek, in Santa Barbara County.
Temporal Representation: | Samples were collected from April 2000 to December 2000.
Environmental Conditions: | Water body is located in the Santa Maria Hydrologic Unit. The site is identified as Bradley Canyon Diversion Channel at Foxen Canyon Road (312BCF).
QAPP Information: | CCAMP, SWAMP QAPP.Samples were taken according to CCAMP protocols.
QAPP Information Reference(s):
LOE ID: | 9866
Pollutant: | Ammonia (Unionized)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 7
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 3 of 7 samples exceed the criterion for Ammonia as N, Unionized.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin General Objective, Chapter III, Section II.A.2 (General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries) states that the discharge of wastes shall not cause concentrations of unionized ammonia (NH3) to exceed 0.025 mg/l (as N) in receiving waters (page III-4) .
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 4/12/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 9865
Pollutant: | Ammonia (Unionized)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 7
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 3 of 7 samples exceed the criterion for Ammonia as N, Unionized.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin General Objective, Chapter III, Section II.A.2 (General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries) states that the discharge of wastes shall not cause concentrations of unionized ammonia (NH3) to exceed 0.025 mg/l (as N) in receiving waters (page III-4) .
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 4/12/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 4298
Pollutant: | Fecal Coliform
Final Listing Decision: | Do Not Delist from 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | Do Not Delist from 303(d) list (TMDL required list)(2006)
Revision Status | Revised
Sources: | Agriculture | Natural Sources
Expected TMDL Completion Date: | 2013
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for removal from the section 303(d) list under section 4.3 of the Listing Policy. Under this section a single line of evidence is necessary to assess listing status. Three lines of evidence are available in the administrative record to assess this pollutant. LOE #11819 replaces LOE #1923. LOE #1923 erroneously showed 4 exceedances out of 7 samples. LOE #11819 correctly shows 5 exceedances out of the same 7 samples. These 5 samples exceed the water quality objective for Water Contact Recreation. Two of the 7 samples exceed the water quality objective for Non-Contact Recreation. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against removing this water segment-pollutant combination from the section 303(d) list. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Five of the 7 samples exceed the water quality objective for Water Contact Recreation. Two of the 7 samples exceed the water quality objective for Non-Contact Recreation.and this exceeds the allowable frequency calculated from the equation in Table 4.2 of the Listing Policy. 4. Pursuant to section 4.11 of the Listing Policy, no additional data and information are available indicating that standards are met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be removed from the section 303(d) list because applicable water quality standards for the pollutant are being exceeded.
SWRCB Board Decision / Staff Recommendation: | After review of the available data and information, SWRCB staff concludes that the water body-pollutant combination should not be removed from the section 303(d) list because it cannot be determined if applicable water quality standards are attained.
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 4298

LOE ID: | 11820
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 7
Number of Exceedances: | 2
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 2 of 7 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 4/12/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 1923
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 7
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | There were 7 samples collected at the Foxen Canyon Road site (CCAMP, 2004). Four of these samples exceeded the 400 MPN/100 ml criteria.
Data Reference: | Placeholder reference 2006 303(d)
Water Quality Objective/Criterion: | Basin Plan: Fecal coliform concentration, based on minimum of not less than five samples or any 30-day period, shall not exceed a log mean of 200/100 ml, nor shall more than ten percent of the total samples during any 30-day period exceed 400/100 ml.
Objective/Criterion Reference: | Placeholder reference 2006 303(d)
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Three stations were sampled.
Temporal Representation: | Sampling occurred monthly.
Environmental Conditions: |
QAPP Information: | CCAMP data.
QAPP Information Reference(s):
LOE ID: | 11819
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 7
Number of Exceedances: | 5
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 5 of 7 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 200 MPN/100 ml, nor shall more than ten percent of total samples during any 30-day period exceed 400 MPN/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 4/12/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 5501
Pollutant: | Nitrate
Final Listing Decision: | Do Not Delist from 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | List on 303(d) list (TMDL required list)(2006)
Revision Status | Revised
Sources: | Agriculture | Removal of Riparian Vegetation
Expected TMDL Completion Date: | 2013
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for removal from the section 303(d) list under section 4.1 of the Listing Policy. Under this section a single line of evidence is necessary to assess listing status. Eight lines of evidence are available in the administrative record to assess this pollutant. However, LOE #9881 replaces LOE #1924 because it contains the same data, with on exception. LOE #1924 erroneously stated that nine samples were available. Only 8 were available from this time period as shown in LOE #9881. Also, LOE #1924 expressed Nitrate as NO3. LOE #9881 expresses it as Nitrogen. Therefore LOE #1924 is not used in this assessment, to avoid double counting data. Three LOEs are used to assess the Municipal and Domestic Supply Beneficial Use. Six of the 15 samples exceed the water quality objective for Municipal and Domestic Supply. In addition, 5 of 8 samples exceed the Evaluation Guideline (OEHHA public Health Goal for Nitrate and Nitrogen in Drinking Water, December 1997) set to protect for Municipal and Domestic Supply. Each of these exceed that allowable frequency as stated in Table 4.1 of the Listing Policy. Four LOEs are used to assess the Cold and Warm Freshwater Habitat Beneficial Uses. Fourteen of the 15 samples exceeded the Evaluation Guideline for Nitrate established for aquatic life beneficial uses using the Numeric Nutrient Endpoint tool and this exceeds that allowable frequency as stated in Table 4.1 of the Listing Policy. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against removing this water segment-pollutant combination from the section 303(d) list. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Six of the 15 samples exceed the water quality objective for Municipal Domestic Supply and 5 of 8 samples exceed the Evaluation Guideline (OEHHA public Health Goal for Nitrate and Nitrogen in Drinking Water, December 1997) set to protect for Municipal and Domestic Supply. Each of these and this exceeds the allowable frequency calculated from the equation in Table 4.1 of the Listing Policy. 4. Fourteen of the 15 samples exceeded the Evaluation Guideline for Nitrate established for aquatic life beneficial uses using the Numeric Nutrient Endpoint tool and this exceeds that allowable frequency as stated in Table 4.1 of the Listing Policy. 5. Pursuant to section 4.11 of the Listing Policy, no additional data and information are available indicating that standards are met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be removed from the section 303(d) list because applicable water quality standards for the pollutant are being exceeded.
SWRCB Board Decision / Staff Recommendation: | After review of the available data and information, SWRCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 5501

LOE ID: | 14322
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 7
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 2 of 7 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin Objective for municipal and domestic supply uses of inland surface waters (Section II.A.2) states the following: waters shall not contain concentrations of chemical constituents in excess of the limits specified in California Code of Regulations, Title 22, Article 4, Chapter 15, Section 64435, Tables 2 and 3 as listed in Table 3-2. The maximum contaminant level listed in Table 3-2 (inorganic and fluoride concentrations not to be exceeded in domestic or municipal supply) for nitrate is 10.0 mg/L (NO3 as N).
Objective/Criterion Reference: | Title 22, Division 4, Ch. 15, Article 4, Section 64431, Table 64431-A
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/29/2005. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 15215
Pollutant: | Nitrate/Nitrite (Nitrite + Nitrate as N)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 8
Number of Exceedances: | 5
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 5 of 8 samples exceed the criterion for Nitrate/Nitrite as N.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | OEHHA public Health Goals for Nitrate and Nitrogen in Drinking Water (December 1997). Page 6.
Objective/Criterion Reference: | Public health goals for nitrate and nitrite in drinking water
Evaluation Guideline: | OEHHA Public Health Goal states that sum of the concentration of nitrate + nitrite shall not exceed 10 mg/L (NO3+NO2 expressed as N).
Guideline Reference: | Public health goals for nitrate and nitrite in drinking water
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 3/22/2005-11/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 9881
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 8
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 4 of 8 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin Objective for municipal and domestic supply uses of inland surface waters (Section II.A.2) states the following: waters shall not contain concentrations of chemical constituents in excess of the limits specified in California Code of Regulations, Title 22, Article 4, Chapter 15, Section 64435, Tables 2 and 3 as listed in Table 3-2. The maximum contaminant level listed in Table 3-2 (inorganic and fluoride concentrations not to be exceeded in domestic or municipal supply) for nitrate is 10.0 mg/L (NO3 as N).
Objective/Criterion Reference: | Title 22, Division 4, Ch. 15, Article 4, Section 64431, Table 64431-A
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 3/2/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 1924
Pollutant: | Nitrate as Nitrate (NO3)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 9
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Four out of nine samples exceeded the water quality objective for nitrate (as NO3) for municipal and domestic supply (CCAMP, 2004; SWAMP, 2004).
Data Reference: | Placeholder reference 2006 303(d)
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in excess of the limits specified in California Code of Regulations, Title 22, Article 4, Chapter 15, Section 64435, Tables 2 and 3 as listed in Table 3-2 (Region 3 Basin Plan, p III-3; In Table 3-2, the MCL for Nitrate (as NO3) in Domestic or Municipal Supply is 45 mg/L).
Objective/Criterion Reference: | Placeholder reference 2006 303(d)
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from 2 sites. All samples with exceedances were collected from one site (312BCF).
Temporal Representation: | Samples were collected from March 2000 to December 2000.
Environmental Conditions: | The water body is located in the Santa Maria hydrologic unit, Guadalupe hydrologic subarea. The site is located at Bradley Canyon Diversion Channel (312BCF) and Bradley Canyon Creek at Orcut-Garey Road (312BCG).
QAPP Information: | CCAMP, SWAMP QAPP.
QAPP Information Reference(s):
LOE ID: | 27859
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 8
Number of Exceedances: | 8
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Data for this assessment unit was collected by one monitoring project: CCAMP Santa Maria (SantaMaria)
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Technical approach to develop nutrient numeric endpoints for California, Tetra Tech, June 2006. The Central Coast Region numeric target for maximum nitrate concentration is based on the Tetra Tech NNE (Nutrient Numeric Endpoint) Model and CCAMP data for 193 sites, monitored monthly for at least 1 year between January 1998 and December 2006. The model numeric target for aquatic life habitats in the Central Coast Region is 1.0 mg/L Nitrate as N.
Guideline Reference: | Technical Approach to Develop Nutrient Numeric Endpoints for California
| Technical Paper - Interpreting Narrative Objectives for Biostimulatory Substances Using the Technical Approach for Developing California Nutrient Numeric Endpoints. Central Coast Region
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 3/2/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 27856
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 7
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Data for this assessment unit was collected by one monitoring project: CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth)
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Technical approach to develop nutrient numeric endpoints for California, Tetra Tech, June 2006. The Central Coast Region numeric target for maximum nitrate concentration is based on the Tetra Tech NNE (Nutrient Numeric Endpoint) Model and CCAMP data for 193 sites, monitored monthly for at least 1 year between January 1998 and December 2006. The model numeric target for aquatic life habitats in the Central Coast Region is 1.0 mg/L Nitrate as N.
Guideline Reference: | Technical Approach to Develop Nutrient Numeric Endpoints for California
| Technical Paper - Interpreting Narrative Objectives for Biostimulatory Substances Using the Technical Approach for Developing California Nutrient Numeric Endpoints. Central Coast Region
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/29/2005. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 27858
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 8
Number of Exceedances: | 8
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Data for this assessment unit was collected by one monitoring project: CCAMP Santa Maria (SantaMaria)
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Technical approach to develop nutrient numeric endpoints for California, Tetra Tech, June 2006. The Central Coast Region numeric target for maximum nitrate concentration is based on the Tetra Tech NNE (Nutrient Numeric Endpoint) Model and CCAMP data for 193 sites, monitored monthly for at least 1 year between January 1998 and December 2006. The model numeric target for aquatic life habitats in the Central Coast Region is 1.0 mg/L Nitrate as N.
Guideline Reference: | Technical Approach to Develop Nutrient Numeric Endpoints for California
| Technical Paper - Interpreting Narrative Objectives for Biostimulatory Substances Using the Technical Approach for Developing California Nutrient Numeric Endpoints. Central Coast Region
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 3/2/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 27857
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 7
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Data for this assessment unit was collected by one monitoring project: CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth)
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Technical approach to develop nutrient numeric endpoints for California, Tetra Tech, June 2006. The Central Coast Region numeric target for maximum nitrate concentration is based on the Tetra Tech NNE (Nutrient Numeric Endpoint) Model and CCAMP data for 193 sites, monitored monthly for at least 1 year between January 1998 and December 2006. The model numeric target for aquatic life habitats in the Central Coast Region is 1.0 mg/L Nitrate as N.
Guideline Reference: | Technical Approach to Develop Nutrient Numeric Endpoints for California
| Technical Paper - Interpreting Narrative Objectives for Biostimulatory Substances Using the Technical Approach for Developing California Nutrient Numeric Endpoints. Central Coast Region
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/29/2005. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 16057
Pollutant: | Chlorophyll-a
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. None of the 22 samples exceed the Evaluation Guideline (North Carolina Administrative code, Title 15A) and the General Water Quality Objective set to protect aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 26 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of the 22 samples exceed the Evaluation Guideline (North Carolina Administrative code, Title 15A) and the General Water Quality Objective set to protect aquatic life beneficial uses and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16057

LOE ID: | 14566
Pollutant: | Chlorophyll-a
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 0 of 14 samples exceed the criterion for Chlorophyll a.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Evaluation Guideline: | North Carolina Administrative code (NCAC), Title 15A - Environmental and Natural Resources, Subchapter 2B-Surface water and wetland standards, Rule 0211-Fresh surface water quality standards for class C waters (Class C is defined as freshwaters protected for secondary recreation, fishing, aquatic life including propagation and survival, and wildlife). Section 3(a) of Rule 0211 applies to all fresh surface waters and states that chlorophyll a is not to exceed 40 ug/L.
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14565
Pollutant: | Chlorophyll-a
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 0 of 14 samples exceed the criterion for Chlorophyll a.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Evaluation Guideline: | North Carolina Administrative code (NCAC), Title 15A - Environmental and Natural Resources, Subchapter 2B-Surface water and wetland standards, Rule 0211-Fresh surface water quality standards for class C waters (Class C is defined as freshwaters protected for secondary recreation, fishing, aquatic life including propagation and survival, and wildlife). Section 3(a) of Rule 0211 applies to all fresh surface waters and states that chlorophyll a is not to exceed 40 ug/L.
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 9867
Pollutant: | Chlorophyll-a
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 8
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 0 of 8 samples exceed the criterion for Chlorophyll a.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Evaluation Guideline: | North Carolina Administrative code (NCAC), Title 15A - Environmental and Natural Resources, Subchapter 2B-Surface water and wetland standards, Rule 0211-Fresh surface water quality standards for class C waters (Class C is defined as freshwaters protected for secondary recreation, fishing, aquatic life including propagation and survival, and wildlife). Section 3(a) of Rule 0211 applies to all fresh surface waters and states that chlorophyll a is not to exceed 40 ug/L.
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 3/2/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 9868
Pollutant: | Chlorophyll-a
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 8
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 0 of 8 samples exceed the criterion for Chlorophyll a.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Evaluation Guideline: | North Carolina Administrative code (NCAC), Title 15A - Environmental and Natural Resources, Subchapter 2B-Surface water and wetland standards, Rule 0211-Fresh surface water quality standards for class C waters (Class C is defined as freshwaters protected for secondary recreation, fishing, aquatic life including propagation and survival, and wildlife). Section 3(a) of Rule 0211 applies to all fresh surface waters and states that chlorophyll a is not to exceed 40 ug/L.
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 3/2/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 11210
Pollutant: | Nitrogen, ammonia (Total Ammonia)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. None of the 22 samples exceed the Evaluation Guideline set to protect for Municipal and Domestic Supply. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Zero of 22 samples exceeded the Evaluation Guideline (USEPA Health Advisory 2006 Edition of the Drinking Water Standards and Health Advisories (EPA 822-R-06-013, 2006)) as it applies to the Municipal and Domestic Supply Objective. This does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 11210

LOE ID: | 10104
Pollutant: | Ammonia as Nitrogen
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 8
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 0 of 8 samples exceed the criterion for Ammonia as N, Total.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | USEPA Health Advisory 2006 Edition of the Drinking Water Standards and Health Advisories (EPA 822-R-06-013, 2006).
Objective/Criterion Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Evaluation Guideline: | EPA's Lifetime Health advisory level for total ammonia is 30.0 mg/L as stated on page 8 of the 2006 edition of the drinking water standards and health advisories. This Advisory Level is defined as "the concentration of a chemical in drinking water that is not expected to cause any adverse noncarcinogenic effects for up to ten days of exposure."
Guideline Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 3/2/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14335
Pollutant: | Ammonia as Nitrogen
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 0 of 14 samples exceed the criterion for Ammonia As N, Total.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | USEPA Health Advisory 2006 Edition of the Drinking Water Standards and Health Advisories (EPA 822-R-06-013, 2006).
Objective/Criterion Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Evaluation Guideline: | EPA's Lifetime Health advisory level for total ammonia is 30.0 mg/L as stated on page 8 of the 2006 edition of the drinking water standards and health advisories. This Advisory Level is defined as "the concentration of a chemical in drinking water that is not expected to cause any adverse noncarcinogenic effects for up to ten days of exposure."
Guideline Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 16059
Pollutant: | Sediment Toxicity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.6 of the Listing Policy. Under section 3.6 a single line of evidence is necessary to assess listing status for toxicity. Four lines of evidence are available in the administrative record to assess this pollutant in sediment samples. One of the 2 samples were toxic to invertebrate test organisms (exhibit a significant increase in mortality compared to the laboratory control) and therefore do not exceed the narrative General Objective for toxicity, set to protect for aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. of the 2 samples were toxic to invertebrate test organisms. Therefore, this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16059

LOE ID: | 23666
Pollutant: | Invertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 1
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPsouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 1 of 1 samples exceed the criterion for Toxicity, Hyalella azteca Survival (%) 10 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected on a single day 5/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 23648
Pollutant: | Invertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPsouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Toxicity, Hyalella azteca Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected on a single day 4/20/2005. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 23667
Pollutant: | Invertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 1
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPsouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 1 of 1 samples exceed the criterion for Toxicity, Hyalella azteca Survival (%) 10 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected on a single day 5/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 23668
Pollutant: | Invertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPsouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Toxicity, Hyalella azteca Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected on a single day 4/20/2005. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 11228
Pollutant: | Temperature, water
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.2 of the Listing Policy. Three lines of evidence are available in the administrative record to assess this pollutant. Based on Section 3.2 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Seven of 24 samples exceeded the Evaluation Guideline (Moyle, 1976) set for protection of Cold Freshwater Habitat. However, although Bradley Canyon Creek flows to Santa Maria River which is identified as having a "definite run or population" of steelhead according to the recent publication (Steelhead/Rainbow Trout (Oncorhynchus mykiss) Resources South of the Golden Gate, California (Becker, G.S and I.J Reining, October 2008) this Evaluation is not relevant to this waterbody. The measurements which are in exceedance of the Temperature Evaluation Guideline are all from in summer months, when the Santa Maria River is dry at the confluence with Bradley Channel Creek. Therefore the warm water from Bradley Canyon Creek is not in exceedance of the General Objectives in the Central Coast Water Quality Control Plan. The General Objective states that natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Board that such alteration in temperature does not adversely affect beneficial uses. Because the Santa Maria Rive is dry in summer at the confluence, this discharge does not adversely affect beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Although Bradley Canyon Creek flows to Santa Maria River, in summer when temperatures are elevated the Santa Maria River is dry at the confluence. Therefore this Evaluation Guideline is not relevant for the Creek. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because the Evaluation Guideline is not relevant for the Creek.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 11228

LOE ID: | 13401
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Water Temperature.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Board that such alteration in temperature does not adversely affect beneficial uses (General Objective in Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Inland Fishes of California (Moyle 1976) states that for rainbow trout the optimum range for growth and completion of most life stages is 13-21 degrees C (page 129).
Guideline Reference: | Inland Fishes of California
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 6/30/2000-9/7/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13368
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 7
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 1 of 7 samples exceed the criterion for Water Temperature.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Board that such alteration in temperature does not adversely affect beneficial uses (General Objective in Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Inland Fishes of California (Moyle 1976) states that for rainbow trout the optimum range for growth and completion of most life stages is 13-21 degrees C (page 129).
Guideline Reference: | Inland Fishes of California
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 4/12/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14387
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 15
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 6 of 15 samples exceed the criterion for Water Temperature.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Board that such alteration in temperature does not adversely affect beneficial uses (General Objective in Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Inland Fishes of California (Moyle 1976) states that for rainbow trout the optimum range for growth and completion of most life stages is 13-21 degrees C (page 129).
Guideline Reference: | Inland Fishes of California
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 11226
Pollutant: | Low Dissolved Oxygen
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture | Removal of Riparian Vegetation
Expected TMDL Completion Date: | 2013
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.2 of the Listing Policy. Twelve lines of evidence are available in the administrative record to assess this pollutant. Based on section 3.2 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Six LOEs summarize Dissolved Oxygen data. Seven of 25 samples exceed the Cold Freshwater Habitat objective and 5 of 25 samples exceed the Warm Freshwater Habitat objective. Both of these rates of exceedance support rejection of the null hypothesis. Six LOEs summarize Oxygen Saturation data. Eleven of 25 samples exceed the general water quality objective for oxygen saturation (when applied as a single sample maximum). However, the Basin Plan objective states that the median oxygen saturation value shall not fall below 85% and the median value did not exceed this criterion. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Seven of 25 samples exceed the Cold Freshwater Habitat objective and 5 of 25 samples exceed the Warm Freshwater Habitat objective and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 11226

LOE ID: | 13351
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 8
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 2 of 8 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 3/2/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14617
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 15
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 6 of 15 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14616
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 15
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 2 of 15 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, dissolved oxygen concentration shall not be reduced below 5.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14615
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 15
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 4 of 15 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 12615
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 1 of 2 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 6/30/2000-9/7/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 12599
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 1 of 2 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 6/30/2000-9/7/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13383
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 1 of 2 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 6/30/2000-9/7/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13384
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 1 of 2 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, dissolved oxygen concentration shall not be reduced below 5.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 6/30/2000-9/7/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14618
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 15
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 6 of 15 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13367
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 8
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 4 of 8 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 3/2/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13365
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 8
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 2 of 8 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, dissolved oxygen concentration shall not be reduced below 5.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 3/2/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13366
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 8
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 4 of 8 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 3/2/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 16058
Pollutant: | Turbidity
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture
Expected TMDL Completion Date: | 2013
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.2 of the Listing Policy. Six lines of evidence are available in the administrative record to assess this pollutant. Based on section 3.2 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. This Evaluation Guideline is relevant for Bradley Canyon Creek as it is a tributary to Santa Maria River, and Turbidity levels in the Creek are elevated year round. A recent publication (Steelhead/Rainbow Trout (Oncorhynchus mykiss) Resources South of the Golden Gate, California (Becker, G.S and I.J Reining, October 2008) identifies Santa Maria River as having "Definite run or population". Therefore, discharge of turbid water from Bradley Canyon Creek is specifically prohibited by the General Objectives in the Central Coast Water Quality Control Plan which states that waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Fifteen of 19 samples exceeded the Evaluation Guideline (Sigler et al., 1984) applied to protect for aquatic life beneficial uses and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16058

LOE ID: | 13385
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 2 of 2 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 6/30/2000-9/7/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13382
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 3
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 3 of 3 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 4/12/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13381
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 3
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 3 of 3 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 4/12/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 13400
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 2 of 2 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 6/30/2000-9/7/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14386
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 10
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 10 of 14 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14385
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 10
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 10 of 14 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 16060
Pollutant: | Unknown Toxicity
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture
Expected TMDL Completion Date: | 2013
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 and section 3.6 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Six lines of evidence are available in the administrative record to assess this pollutant in water samples. Three of the samples were toxic to test organisms (exhibited a significant increase in mortality or decrease in cell density compared to the laboratory control) and therefore exceed the narrative General Objective for toxicity, set to protect for aquatic life beneficial uses. The following is a summary of the results from individual toxicity tests. None of the 4 samples (tested for toxicity to plants), exceed the narrative General Objective for toxicity and none of the 3 samples (tested for toxicity to vertebrate test organisms), exceed the narrative General Objective for toxicity. However, 3 of the 5 samples (tested for toxicity to invertebrate test organisms), exceed the narrative General Objective for toxicity and this exceeds the allowable frequency listed in Table 3.1 of the Listing Policy. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Three of the 5 samples (tested for toxicity to invertebrate test organisms), exceed the narrative General Objective for toxicity and this exceeds the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16060

LOE ID: | 23660
Pollutant: | Invertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 5
Number of Exceedances: | 3
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPsouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 3 of 5 samples exceed the criterion for Toxicity, Ceriodaphnia dubia Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 3/22/2005-7/26/2005. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 23661
Pollutant: | Invertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 5
Number of Exceedances: | 3
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPsouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 3 of 5 samples exceed the criterion for Toxicity, Ceriodaphnia dubia Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 3/22/2005-7/26/2005. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 23681
Pollutant: | Plant Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 4
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPsouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 0 of 4 samples exceed the criterion for Toxicity, Selenastrum capricornutum Growth (Cell Density) 4 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction in cell count of test organism relative to the control (alpha < 0.05) and cell count <80% of control.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-2/22/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 23680
Pollutant: | Plant Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 4
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPsouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 0 of 4 samples exceed the criterion for Toxicity, Selenastrum capricornutum Growth (Cell Density) 4 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction in cell count of test organism relative to the control (alpha < 0.05) and cell count <80% of control.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-2/22/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 23679
Pollutant: | Vertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 3
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPsouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 0 of 3 samples exceed the criterion for Toxicity, Pimephales promelas Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-2/22/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 23678
Pollutant: | Vertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 3
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPsouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 0 of 3 samples exceed the criterion for Toxicity, Pimephales promelas Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-2/22/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 11235
Pollutant: | pH
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture | Urban Runoff/Storm Sewers
Expected TMDL Completion Date: | 2013
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.2 of the Listing Policy. Fifteen lines of evidence are available in the administrative record to assess this pollutant. Based on section 3.2 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Ten of 25 samples exceed the numeric objective for Municipal & Domestic Supply, Non-Contact Recreation and Water Contact Recreation. Only 2 of 25 samples exceed the Cold and Warm Freshwater Habitat water quality objectives. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Ten of 25 samples exceed the numeric objective for Municipal & Domestic Supply, Non-Contact Recreation and Water Contact Recreation and this meets or exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 11235

LOE ID: | 11856
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 2
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 1 of 2 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 6/30/2000-9/7/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11857
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 2
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 1 of 2 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 6/30/2000-9/7/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11858
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 6/30/2000-9/7/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11839
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 8
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 2 of 8 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 3/2/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11840
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 8
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 0 of 8 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 3/2/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11821
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 8
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 0 of 8 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 3/2/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11822
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 8
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 2 of 8 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin, Section II.A.2. Municipal and Domestic Supply Objectives, Section II.A.2.a states the following: The pH value shall neither be depressed below 6.5 or raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 3/2/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11841
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 6/30/2000-9/7/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11842
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 1 of 2 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin, Section II.A.2. Municipal and Domestic Supply Objectives, Section II.A.2.a states the following: The pH value shall neither be depressed below 6.5 or raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 6/30/2000-9/7/2000. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 11838
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 8
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Santa Maria (SantaMaria) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 2 of 8 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCF-Bradley Canyon diversion channel at Foxen Canyon Road ]
Temporal Representation: | Data was collected over the time period 3/2/2000-12/7/2000. Santa Maria watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14368
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 15
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 2 of 15 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14369
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 15
Number of Exceedances: | 7
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 7 of 15 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin, Section II.A.2. Municipal and Domestic Supply Objectives, Section II.A.2.a states the following: The pH value shall neither be depressed below 6.5 or raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14370
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 15
Number of Exceedances: | 7
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 7 of 15 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14371
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 15
Number of Exceedances: | 7
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 7 of 15 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 14372
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 15
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCWQP Southern Area Ag-Waiver Monitoring (R3_CMPSouth) data for Bradley Canyon Creek to determine beneficial use support and results are as follows: 2 of 15 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Central Coast Water Quality Preservation Inc toxicity data
| Final Data File used for assessment: Central Coast Water Quality Preservation Inc water quality data
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Bradley Canyon Creek was collected at 1 monitoring site [ 312BCC - Bradley Canyon Creek at Culvert, up stream of Santa Maria River]
Temporal Representation: | Data was collected over the time period 2/21/2005-11/15/2006. Cooperative Monitoring Program (CMP) staff conduct monitoring for conventional pollutants at all Ag Waiver monitoring sites monthly. CMP staff also conduct water toxicity monitoring quarterly and sediment toxicity monitoring annually (in spring).
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the Cooperative Monitoring Program QAPP, (Clark and Ogle 2006). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):