# Draft 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 5 - Central Valley Region

Water Body Name: | Fitzhugh Creek, Lower (Modoc County)
Water Body ID: | CAR5265204220090113145748
Water Body Type: | River & Stream

DECISION ID | 10027
Pollutant: | Chloride
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. Table 3.1 of the listing policy recommends listing if a sample size of 2 has 2 or more samples that exceed the evaluation criteria.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10027

LOE ID: | 20602
Pollutant: | Chloride
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Chloride.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Chloride levels should not exceed 250 mg/L (USEPA Maximum Contaminant Level)
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Lower Fitzhugh Creek. Samples were collected at Upper Fitzhugh Creek.
Temporal Representation: | The samples were collected from Oct 16 2003 to Oct 17 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10028
Pollutant: | Copper
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the USEPA Primary MCL and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the California Toxics Rule and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10028

LOE ID: | 20649
Pollutant: | Copper
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Copper.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Copper levels should not exceed 1300 ug/L (Department of Public Health Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Lower Fitzhugh Creek. Samples were collected at Upper Fitzhugh Creek.
Temporal Representation: | The samples were collected from Oct 16 2003 to Oct 17 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 8790
Pollutant: | Copper
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Asses Water Quality: | Zero of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Copper.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Total Copper levels should not exceed the calculated limit based on the formula: Criteria Maximum Concentration (1-hour Average, total)=(EXP(0.9422*LN(hardness)-1.7)) (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals - 2007 for toxicity data
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Lower Fitzhugh Creek. Samples were collected at Upper Fitzhugh Creek.
Temporal Representation: | The samples were collected from Oct 16 2003 to Oct 17 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10371
Pollutant: | Escherichia coli (E. Coli)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.3 of the Listing Policy. Under section 3.3 a single line of evidence is necessary to assess listing status. Data is available from 3 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 14 available concentrations exceeded the USEPA E. coli Objective for Municipal Use and this does not exceed the allowable frequency using Table 3.2 of the Listing Policy. The recommendation is based on staff findings that 0 of 14 available concentrations exceeded the USEPA E. coli Objective for Non-Contact Recreation and this does not exceed the allowable frequency using Table 3.2 of the Listing Policy. The recommendation is based on staff findings that 0 of 14 available concentrations exceeded the USEPA E. coli Objective for Water Contact Recreation and this does not exceed the allowable frequency using Table 3.2 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10371

LOE ID: | 20506
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 14 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for E.Coli Bacteria.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | E.Coli Bacteria levels should not exceed 409 MPN/100 mL in any single sample (USEPA E.Coli Guideline)
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Samples were collected at Lower Fitzhugh Creek. Samples were collected at Upper Fitzhugh Creek.
Temporal Representation: | The samples were collected from Jun 14 2004 to Sep 19 2005
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 20505
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | PATHOGEN MONITORING
Data Used to Asses Water Quality: | 0 of the 14 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for E.Coli Bacteria.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | E.Coli Bacteria levels should not exceed 235 MPN/100 mL in any single sample (USEPA E.Coli Guideline)
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Samples were collected at Lower Fitzhugh Creek. Samples were collected at Upper Fitzhugh Creek.
Temporal Representation: | The samples were collected from Jun 14 2004 to Sep 19 2005
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 20504
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | PATHOGEN MONITORING
Data Used to Asses Water Quality: | 0 of the 14 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for E.Coli Bacteria.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | E.Coli Bacteria levels should not exceed 235 MPN/100 mL in any single sample (USEPA E.Coli objective)
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Lower Fitzhugh Creek. Samples were collected at Upper Fitzhugh Creek.
Temporal Representation: | The samples were collected from Jun 14 2004 to Sep 19 2005
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10030
Pollutant: | Specific Conductivity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 11 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.2 of the Listing Policy. Table 3.2 of the listing policy recommends listing if a sample size of 11 has 5 or more samples that exceed the evaluation criteria.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10030

LOE ID: | 20370
Pollutant: | Specific Conductivity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 11
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 11 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Specific Conductivity.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | The water quality objective used was the California Secondary MCL recommended level of 900 uS/cm. The Basin Plan includes chemical constituent water quality objectives that include (by reference) secondary maximum contaminant levels (MCLs) protective of MUN (CVRWQCB, 2007a).The secondary MCLs for electrical conductivity provide a range of values including a recommended level (900 uS/cm), upper level (1600 uS/cm) and a short-term level (2200 uS/cm). The recommended concentration was used as it is intended to be protective of all drinking water uses.
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Lower Fitzhugh Creek. Samples were collected at Upper Fitzhugh Creek.
Temporal Representation: | The samples were collected from Oct 16 2003 to Sep 15 2004
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10031
Pollutant: | Total Dissolved Solids
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. Table 3.1 of the listing policy recommends listing if a sample size of 2 has 2 or more samples that exceed the evaluation criteria.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10031

LOE ID: | 20728
Pollutant: | Total Dissolved Solids
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Total Dissolved Solids.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | The water quality objective used was the California Secondary MCL recommended level of 500 mg/L. The Basin Plan includes chemical constituent water quality objectives that include (by reference) secondary maximum contaminant levels (MCLs) protective of MUN (CVRWQCB, 2007a).The secondary MCLs for TDS provide a range of values including a recommended level (500 mg/L), upper level (1000 mg/L) and a short-term level (1500 mg/L). The recommended concentration was used as it is intended to be protective of all drinking water uses.
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Lower Fitzhugh Creek. Samples were collected at Upper Fitzhugh Creek.
Temporal Representation: | The samples were collected from Oct 16 2003 to Oct 17 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10032
Pollutant: | Zinc
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the USEPA Secondary MCL and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the USEPA National Ambient Water Quality Objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10032

LOE ID: | 20741
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Zinc.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Zinc levels should not exceed 5000 ug/L (Department of Public Health Secondary MCL)
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Lower Fitzhugh Creek. Samples were collected at Upper Fitzhugh Creek.
Temporal Representation: | The samples were collected from Oct 16 2003 to Oct 17 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 8791
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Asses Water Quality: | Zero of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Zinc.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Total Zinc levels should not exceed the calculated limit based on the formula: Criteria Maximum Concentration=EXP((0.8473*LN(hardness))+0.884)(CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals - 2007 for toxicity data
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Lower Fitzhugh Creek. Samples were collected at Upper Fitzhugh Creek.
Temporal Representation: | The samples were collected from Oct 16 2003 to Oct 17 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):