# Draft 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 5 - Central Valley Region

Water Body Name: | Pit River, North Fork
Water Body ID: | CAR5265201620080909193959
Water Body Type: | River & Stream

DECISION ID | 10243
Pollutant: | Specific Conductivity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 1 of 149 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using the BinomBal program provided by the SWRCB. The BinomBal program calculates a sample size of 149 having a listing requirement when 25 or more samples exceed the evaluation criteria. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10243

LOE ID: | 21036
Pollutant: | Specific Conductivity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 149
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 1 of the 149 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Specific Conductivity.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | The water quality objective used was the California Secondary MCL recommended level of 900 uS/cm. The Basin Plan includes chemical constituent water quality objectives that include (by reference) secondary maximum contaminant levels (MCLs) protective of MUN (CVRWQCB, 2007a).The secondary MCLs for electrical conductivity provide a range of values including a recommended level (900 uS/cm), upper level (1600 uS/cm) and a short-term level (2200 uS/cm). The recommended concentration was used as it is intended to be protective of all drinking water uses.
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at North Fork Pit in Alturas. Samples were collected at Pit @ North Fork (XL Ranch). Samples were collected at Pit @ USFS bridge near Likely.
Temporal Representation: | The samples were collected from Dec 30 1899 to Dec 30 1899
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 15954
Pollutant: | pH
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. One line of evidence are available in the administrative record to assess this pollutant. Seventy-two of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Seventy-two of 149 samples exceed the pH objective outlined in the Basin Plan and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15954

LOE ID: | 7913
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 149
Number of Exceedances: | 72
Data and Information Type: | Not Specified
Data Used to Asses Water Quality: | 72 of the 149 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for pH.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | pH levels should not be lower than 6.5 or higher than 8.5 (Basin Plan Objective)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| SWAMP data entered by SWRCB into BDAT database
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at North Fork Pit in Alturas. Samples were collected at Pit @ North Fork (XL Ranch). Samples were collected at Pit @ USFS bridge near Likely.
Temporal Representation: | The samples were collected from Apr 5 2001 to Sep 12 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):