# Draft 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 5 - Central Valley Region

Water Body Name: | Keswick Reservoir (portion downstream from Spring Creek)
Water Body ID: | CAL5244001220020730101915
Water Body Type: | Lake & Reservoir

DECISION ID | 6970
Pollutant: | Cadmium
Final Listing Decision: | Do Not Delist from 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | List on 303(d) list (TMDL required list)(2006)
Revision Status | Revised
Sources: | Resource Extraction
Expected TMDL Completion Date: | 2020
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for removal from the section 303(d) list under section 4.1 of the Listing Policy. Under this section a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess pollutant. None of samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against removing this water segment-pollutant combination from the section 303(d) list. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. The chemical analyses method detection limit were not low enough to determine whether or not the water bodys dissolved cadmium concentrations were below the WQOs for all 31 samples 4. Pursuant to section 4.11 of the Listing Policy, no additional data and information are available indicating that standards are met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be removed from the section 303(d) list because applicable water quality standards for the pollutant are being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 6970

LOE ID: | 22385
Pollutant: | Cadmium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 0
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Thirty-one samples were taken from the below Keswick Dam after the completion of the Slickrock Creek Dam. The chemical analyses method detection limit were not low enough to determine whether or not the water bodys dissolved cadmium concentrations were below the WQOs.
Data Reference: | Metals and hardness data for Sacramento River (below Keswick Dam and below Shasta Dam), 2004
Water Quality Objective/Criterion: | California Toxics Rule Criteria (USEPA, 2000) - Freshwater Aquatic Life ProtectionContinuous Concentration (4-day Average) calculated based on the following formula e(0.7852*ln(hardness)-2.715))x(1.101672-(ln(hardness)x0.041838)) which incorporates hardness.Basin Plan (CVRWQCB, 2007) - Maximum Contaminant Level Acute WQO based on the following formula e((1.160)x(ln(hardness) - 5.777)) which incorporates hardness.
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
| Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected in downstream of the Keswick Dam.
Temporal Representation: | Samples were only collected from June 2004 to December 2004.
Environmental Conditions: |
QAPP Information: | QA information not available
QAPP Information Reference(s):
LOE ID: | 4243
Pollutant: | Cadmium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Not Recorded
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 0
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Unspecified--This LOE is a placeholder to support a 303(d) listing decision made prior to 2006.
Data Reference: | Placeholder reference pre-2006 303(d)
Water Quality Objective/Criterion: | Unspecified
Objective/Criterion Reference: | Placeholder reference pre-2006 303(d)
Evaluation Guideline: | Unspecified
Guideline Reference: | Placeholder reference pre-2006 303(d)
Spatial Representation: | Unspecified
Temporal Representation: | Unspecified
Environmental Conditions: | Unspecified
QAPP Information: | Unspecified
QAPP Information Reference(s):

DECISION ID | 6971
Pollutant: | Copper
Final Listing Decision: | Do Not Delist from 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | List on 303(d) list (TMDL required list)(2006)
Revision Status | Revised
Sources: | Resource Extraction
Expected TMDL Completion Date: | 2020
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for removal from the section 303(d) list under section 4.1 of the Listing Policy. Under this section a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess pollutant. None of samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against removing this water segment-pollutant combination from the section 303(d) list. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 34 samples exceeded the acute California Toxics Rule criteria and this does not exceed the allowable frequency listed in Table 4.1 of the Listing Policy. However, the available data is not representative of all seasons. 4. Pursuant to section 4.11 of the Listing Policy, no additional data and information are available indicating that standards are met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be removed from the section 303(d) list because applicable water quality standards for the pollutant are being exceeded.
SWRCB Board Decision / Staff Recommendation: | N/A
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 6971

LOE ID: | 22384
Pollutant: | Copper
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 34
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Thirty-four samples were taken from the below Keswick Dam after the completion of the Slickrock Creek Dam. Zero exceedances of the acute or chronic WQO were observed.
Data Reference: | Metals and hardness data for Sacramento River (below Keswick Dam and below Shasta Dam), 2004
Water Quality Objective/Criterion: | California Toxics Rule Criteria (USEPA, 2000) - Freshwater Aquatic Life ProtectionContinuous Concentration (4-day Average) calculated based on the following formula e(0.8545*ln(hardness)-1.702))x(0.96) which incorporates hardness.Basin Plan (CVRWQCB, 2007) - Maximum Contaminant Level Acute WQO based on the following formula e((0.905)x(ln(hardness) - 1.612)) which incorporates hardness.
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
| Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected in downstream of the Keswick Dam.
Temporal Representation: | Samples were only collected from June 2004 to December 2004.
Environmental Conditions: |
QAPP Information: | QA information not available
QAPP Information Reference(s):
LOE ID: | 4244
Pollutant: | Copper
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Not Recorded
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 0
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Unspecified--This LOE is a placeholder to support a 303(d) listing decision made prior to 2006.
Data Reference: | Placeholder reference pre-2006 303(d)
Water Quality Objective/Criterion: | Unspecified
Objective/Criterion Reference: | Placeholder reference pre-2006 303(d)
Evaluation Guideline: | Unspecified
Guideline Reference: | Placeholder reference pre-2006 303(d)
Spatial Representation: | Unspecified
Temporal Representation: | Unspecified
Environmental Conditions: | Unspecified
QAPP Information: | Unspecified
QAPP Information Reference(s):

DECISION ID | 6972
Pollutant: | Zinc
Final Listing Decision: | Do Not Delist from 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | List on 303(d) list (TMDL required list)(2006)
Revision Status | Revised
Sources: | Resource Extraction
Expected TMDL Completion Date: | 2020
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for removal from the section 303(d) list under section 4.1 of the Listing Policy. Under this section a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess pollutant. None of samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against removing this water segment-pollutant combination from the section 303(d) list. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 31 samples exceeded the water quality objective and this exceeds the allowable frequency listed in Table 4.1 of the Listing Policy. However, the available data is not representative of all seasons. 4. Pursuant to section 4.11 of the Listing Policy, no additional data and information are available indicating that standards are met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be removed from the section 303(d) list because applicable water quality standards for the pollutant are being exceeded.
SWRCB Board Decision / Staff Recommendation: | N/A
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 6972

LOE ID: | 22386
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 31
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Thirty-one samples were taken from the below Keswick Dam after the completion of the Slickrock Creek Dam. Zero exceedances of the acute or chronic WQO were observed.
Data Reference: | Metals and hardness data for Sacramento River (below Keswick Dam and below Shasta Dam), 2004
Water Quality Objective/Criterion: | California Toxics Rule Criteria (USEPA, 2000) - Freshwater Aquatic Life ProtectionContinuous Concentration (4-day Average) calculated based on the following formula e(0.8473*ln(hardness)+0.884))x(0.986) which incorporates hardness.Basin Plan (CVRWQCB, 2007) - Maximum Contaminant Level Acute WQO based on the following formula e((0.830)x(ln(hardness) - 0.289)) which incorporates hardness.
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
| Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected in downstream of the Keswick Dam.
Temporal Representation: | Samples were only collected from June 2004 to December 2004.
Environmental Conditions: |
QAPP Information: | QA information not available
QAPP Information Reference(s):
LOE ID: | 4245
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Not Recorded
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 0
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Unspecified--This LOE is a placeholder to support a 303(d) listing decision made prior to 2006.
Data Reference: | Placeholder reference pre-2006 303(d)
Water Quality Objective/Criterion: | Unspecified
Objective/Criterion Reference: | Placeholder reference pre-2006 303(d)
Evaluation Guideline: | Unspecified
Guideline Reference: | Placeholder reference pre-2006 303(d)
Spatial Representation: | Unspecified
Temporal Representation: | Unspecified
Environmental Conditions: | Unspecified
QAPP Information: | Unspecified
QAPP Information Reference(s):