# Draft 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 5 - Central Valley Region

Water Body Name: | Calaveritas Creek (Calaveras County)
Water Body ID: | CAR5333004220080808173644
Water Body Type: | River & Stream

DECISION ID | 9846
Pollutant: | Arsenic
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 2 available concentrations exceeded the USEPA Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met. "
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9846

LOE ID: | 8350
Pollutant: | Arsenic
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Arsenic.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Arsenic levels should not exceed 340 ug/L maximum concentration for 1-hour average (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected from Jun 13 2002 to Jun 26 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 20542
Pollutant: | Arsenic
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Arsenic.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Arsenic levels should not exceed 10 ug/L (USEPA Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected from Jun 13 2002 to Jun 26 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 9847
Pollutant: | Cadmium
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 2 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9847

LOE ID: | 8352
Pollutant: | Cadmium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Cadmium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Cadmium levels should not exceed the calculated limit based on the formula: Criteria Maximum Concentration (1-hour Average dissolved)=(EXP(1.128*LN(hardness)-3.6867))*(1.136672-(LN(hardness)*0.041838)) (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected from Jun 13 2002 to Jun 26 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 20615
Pollutant: | Cadmium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Cadmium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Cadmium levels should not exceed 5 ug/L (Department of Public Health Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected from Jun 13 2002 to Jun 26 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 9848
Pollutant: | Chromium (total)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the Department of Public Health Primary MCL for Municipal and Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met. "
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9848

LOE ID: | 20576
Pollutant: | Chromium (total)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Chromium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Chromium levels should not exceed 50 ug/L (Department of Public Health Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected from Jun 13 2002 to Jun 26 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 9849
Pollutant: | Copper
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 2 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. In addition, 0 of 2 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9849

LOE ID: | 8355
Pollutant: | Copper
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Zero of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Copper.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | California Toxics Rule 4-day average criteria for dissolved Copper.
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected from Jun 13 2002 to Jun 26 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 20648
Pollutant: | Copper
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Copper.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Copper levels should not exceed 1300 ug/L (Department of Public Health Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected from Jun 13 2002 to Jun 26 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 14786
Pollutant: | Escherichia coli (E. Coli)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess this pollutant. One of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. One of 13 samples exceeded the E. Coli objective and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. According to table 3.2, a minimum sample size of 26 is required to designate a fully supporting use rating. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 14786

LOE ID: | 21762
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 13
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | The Central Valley Regional Water Quality Control Board Surface Water Ambient Monitoring Program collected 13 samples from March 2002 to December 2002. One of the 13 samples exceeded the evaluation objective.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. The objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | The USEPA E. Coli objective of 235/100 mL in any single sample (USEPA 1986).
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | Sampling occurred from March 2002 to December 2002.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)

DECISION ID | 9850
Pollutant: | Lead
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 2 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9850

LOE ID: | 20625
Pollutant: | Lead
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Lead.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Lead levels should not exceed 15 ug/L (Department of Public Health Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected from Jun 13 2002 to Jun 26 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 8359
Pollutant: | Lead
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Lead.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Lead levels should not exceed the calculated value based on the formula: Criteria Maximum Concentration (1-hour Average, dissolved)=(EXP(1.273*LN(hardness)-1.46))*(1.46203-(LN(hardness)*0.145712)) (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected from Jun 13 2002 to Jun 26 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 9852
Pollutant: | Nickel
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 2 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9852

LOE ID: | 20682
Pollutant: | Nickel
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Nickel.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Nickel levels should not exceed 100 ug/L (Department of Public Health Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected from Jun 13 2002 to Jun 26 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 8364
Pollutant: | Nickel
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Nickel.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Nickel levels should not exceed the calculated limit based on the formula: Criteria Maximum Concentration (1-hour Average, dissolved)=(EXP(0.846*LN(hardness)+2.255))*(0.998)(CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected from Jun 13 2002 to Jun 26 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 9853
Pollutant: | Nitrate as Nitrate (NO3)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the USEPA National Ambient Water Quality Objective for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 2 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met. "
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9853

LOE ID: | 20752
Pollutant: | Nitrate as Nitrate (NO3)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Nitrate-N.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Nitrate-N levels should not exceed 45 mg/L (Department of Public Health Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected from Jun 13 2002 to Jun 26 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 8366
Pollutant: | Nitrate as Nitrate (NO3)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation guideline for Nitrate-N.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Nitrate-N levels should not to exceed 100 mg/L (USEPA National Ambient Water Quality Objective)
Guideline Reference: | National Recommended Water Quality Criteria. United States Environmental Protection Agency. Office of Water. Office of Science and Technology. 4304T
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected from Jun 13 2002 to Jun 26 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 14785
Pollutant: | Oxygen, Dissolved
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess this pollutant. Two of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Two of 20 samples exceeded the fell below the minimum criterion water quality objective listed in the Sacramento/San Joaquin River Basin Plan and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 14785

LOE ID: | 21761
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 20
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Twenty samples were taken from Calaveritas Creek during 2002. Two of the twenty samples fell below the water quality objective for minimum dissolved oxygen content in surface water.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
Water Quality Objective/Criterion: | From the Sacramento/San Joaquin River Basin Plan the (COLD) Cold Freshwater Habitat criterion is a Minimum Dissolved Oxygen content of 7mg/L
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Calaveritas Creek in Calaveras County.
Temporal Representation: | Samples were collected between January and December 2002. Samples were collected at monthly intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 9854
Pollutant: | Selenium
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 one line(s) of evidence are necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 1 samples exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this sample size is insufficient to determine with the power and confidence of the Listing Policy if standards are not met. A minimum of 2 samples is needed for application of table 3.1. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because it cannot be determined if applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9854

LOE ID: | 8369
Pollutant: | Selenium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 1 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Selenium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Selenium levels should not to exceed 5 ug/L (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected from Oct 24 2002 to Oct 24 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 20260
Pollutant: | Selenium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 1 sample collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Selenium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Selenium levels should not exceed 50 ug/L (Department of Public Health Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | The sample was collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The sample was collected on Oct 24 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 9855
Pollutant: | Specific Conductivity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 20 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.2 of the Listing Policy. Table 3.2 of the listing policy recommends listing if a sample size of 20 has 5 or more samples that exceed the evaluation criteria. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9855

LOE ID: | 20803
Pollutant: | Specific Conductivity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 20
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 20 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Specific Conductivity.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | The water quality objective used was the California Secondary MCL recommended level of 900 uS/cm. The Basin Plan includes chemical constituent water quality objectives that include (by reference) secondary maximum contaminant levels (MCLs) protective of MUN (CVRWQCB, 2007a).The secondary MCLs for electrical conductivity provide a range of values including a recommended level (900 uS/cm), upper level (1600 uS/cm) and a short-term level (2200 uS/cm). The recommended concentration was used as it is intended to be protective of all drinking water uses.
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected from Jan 9 2002 to Dec 23 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 11175
Pollutant: | Unknown Toxicity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that only 1 sample for unknown toxicity Pimephales promelas is available and a minimum of 2 samples is needed for evaluation under section 3.1. The recommendation is also based on staff findings that only 1 sample is available for unknown toxicity Ceriodaphia dubia and a minimum of 2 samples is needed for evaluation under section 3.1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because it cannot be determined if applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 11175

LOE ID: | 25044
Pollutant: | Unknown Toxicity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 1 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation guideline for Unknown Toxicity-Ceriodaphia dubia.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a Fishers Exact analysis with 48-hour acute-style toxicity tests.
Guideline Reference: | Methods for Measuring the Acute Toxicity of Effluents and Receiving Waters to Freshwater and Marine Organisms, Fifth Edition. EPA-821-R-02-012
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected Sep 5 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 25043
Pollutant: | Unknown Toxicity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 1 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation guideline for Unknown Toxicity-Pimephales promelas.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a Fishers Exact analysis with 96-hour acute-style toxicity tests.
Guideline Reference: | Methods for Measuring the Acute Toxicity of Effluents and Receiving Waters to Freshwater and Marine Organisms, Fifth Edition. U.S. Environmental Protection Agency Office of Water, Washington, DC EPA-821-R-02-012
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected Sep 5 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 9856
Pollutant: | Zinc
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 2 available concentrations exceeded the Department of Public Health Secondary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9856

LOE ID: | 20737
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Zinc.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Zinc levels should not exceed 5000 ug/L (Department of Public Health Secondary MCL)
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected from Jun 13 2002 to Jun 26 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 8372
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Zinc.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Zinc levels should not exceed the calculated limit based on the formula: Criteria Maximum Concentration=EXP((0.8473*LN(hardness))+0.884)*(0.978) (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected from Jun 13 2002 to Jun 26 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 9078
Pollutant: | pH
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 20 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.2 of the Listing Policy. Table 3.2 of the listing policy recommends listing if a sample size of 20 has 5 or more samples that exceed the evaluation criteria. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9078

LOE ID: | 8367
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 20
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 20 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for pH.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | pH levels should not be lower than 6.5 or higher than 8.5 (Basin Plan Objective)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Calaveritas Creek at Highway 49.
Temporal Representation: | The samples were collected from Jan 9 2002 to Dec 23 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):