# Draft 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 5 - Central Valley Region

Water Body Name: | Mud Slough, North (upstream of San Luis Drain)
Water Body ID: | CAR5412000020080820163230
Water Body Type: | River & Stream

DECISION ID | 13341
Pollutant: | Electrical Conductivity
Final Listing Decision: | Do Not Delist from 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
Expected TMDL Completion Date: | 2019
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for removal from the section 303(d) list under section 4.2 of the Listing Policy. Under this section a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against removing this water segment-pollutant combination from the section 303(d) list. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Pursuant to section 4.11 of the Listing Policy, no additional data and information are available indicating that standards are met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be removed from the section 303(d) list because applicable water quality standards for the pollutant are being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 13341

LOE ID: | 7241
Pollutant: | Electrical Conductivity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Not Recorded
Beneficial Use: | Agricultural Supply
Number of Samples: | 0
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Unspecified--This LOE is a placeholder to support a 303(d) listing decision made prior to 2006.
Data Reference: | Placeholder reference pre-2006 303(d)
Water Quality Objective/Criterion: |
Objective/Criterion Reference:
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Unspecified
Temporal Representation: | Unspecified
Environmental Conditions: | Unspecified
QAPP Information: | Unspecified
QAPP Information Reference(s):

DECISION ID | 8362
Pollutant: | Ammonia
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 1 of 1016 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. Using BinomBal listing is recommended if a sample size of 1016 has 169 or more samples that exceed the evaluation criteria. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 8362

LOE ID: | 7314
Pollutant: | Ammonia
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 1016
Number of Exceedances: | 1
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | One of the 1016 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation guideline for Ammonia. The exceeded results are as follows: 4/1/1994 - a sample taken at Mud Slough Upstream of SLD Terminus had a result of 0.7mg/L.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Ammonia levels should not to exceed the calculated limit. Freshwater Aquatic Life Protection (Salmonid present) Criteria Maximum Concentration (CMC) (1-hour Average (mg N/L)) calculated based on the following formula: CMC = (0.275/(1 + 107.204-pH)) + (39.0/(1 + 10pH-7.204)) which incorporates pH (US EPA, 2005: Appendix C)
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Mud Slough Upstream of SLD Terminus.
Temporal Representation: | The samples were collected from Apr 1 1994 to Jun 21 2007
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 8364
Pollutant: | Cadmium
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 16 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 8364

LOE ID: | 7318
Pollutant: | Cadmium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 16
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 16 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Cadmium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Cadmium levels should not exceed the calculated limit based on the formula: Criteria Maximum Concentration (1-hour Average dissolved)=(EXP(1.128*LN(hardness)-3.6867))*(1.136672-(LN(hardness)*0.041838)) (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Mud Slough Upstream of SLD Terminus.
Temporal Representation: | The samples were collected from Jun 7 2001 to Nov 21 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 8365
Pollutant: | Copper
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 24 samples exceed the California Toxics Rule 4-day average criteria for dissolved Copper and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 8365

LOE ID: | 7320
Pollutant: | Copper
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 24
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Zero of the 24 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for dissolved Copper.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | California Toxics Rule 4-day average criteria for dissolved Copper.
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Mud Slough Upstream of SLD Terminus.
Temporal Representation: | The samples were collected from October 2000 to November 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 8366
Pollutant: | Lead
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 24 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 8366

LOE ID: | 7322
Pollutant: | Lead
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 24
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Zero of the 24 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Lead.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Lead levels should not exceed the calculated value based on the formula: Criteria Maximum Concentration (1-hour Average, dissolved)=(EXP(1.273*LN(hardness)-1.46))*(1.46203-(LN(hardness)*0.145712)) (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Mud Slough Upstream of SLD Terminus.
Temporal Representation: | The samples were collected from Oct 26 2000 to Nov 21 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 13682
Pollutant: | Malathion
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 31 available 4-day average concentrations exceeded criterion continuous concentration (CCC) and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. In addition, 0 of 31 available 1-hour average concentrations exceeded 1-hour criterion concentration and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 13682

LOE ID: | 23165
Pollutant: | Malathion
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 31
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 31 water samples were collected from Mud Slough from July 2004 through October 2006, representing 31 4-day average concentrations and 31 1-hour average concentrations.0 of 31 available 4-day average concentrations exceeded the 4-day maximum concentration guideline of 0.1 ug/L.0 of 31 available 1-hour average concentrations exceeded the maximum 1-hour concentration of 0.43 ug/L.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Quality Criteria for Water. USEPA Office of Water and Hazardous Materials. Washington, D.C
Evaluation Guideline: | US EPA recommended criterion continuous concentration (CCC) of 0.1 ug/L (US EPA, 1976). California Department of Fish and Game Hazard Assessment Criterion is 0.43 ug/L for criterion maximum concentration (CMC) (CDFG, 1998)
Guideline Reference: | Hazard Assessment of the Insecticide Malathion to Aquatic Life in the Sacramento-San Joaquin River System. California Department of Fish and Game. Office of Spill Prevention and Response Administrative Report 98-2
Spatial Representation: | Samples were collected from Mud Slough at the Upstream of the San Luis Drain.
Temporal Representation: | Samples were collected from July 2004 through October 2006 at monthly interval.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):

DECISION ID | 8368
Pollutant: | Molybdenum
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 117 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. Table 3.1 of the listing policy recommends listing if a sample size of 117 has 10 or more samples that exceed the evaluation criteria. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 8368

LOE ID: | 7328
Pollutant: | Molybdenum
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 117
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 117 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Molybdenum.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Molybdenum levels should not to exceed 50 ug/L (Basin Plan Objective)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Mud Slough Upstream of SLD Terminus.
Temporal Representation: | The samples were collected from Oct 29 1996 to Nov 16 2006
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 8369
Pollutant: | Nickel
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 24 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 8369

LOE ID: | 7330
Pollutant: | Nickel
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 24
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 24 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Nickel.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Nickel levels should not exceed the calculated limit based on the formula: Criteria Maximum Concentration (1-hour Average, dissolved)=(EXP(0.846*LN(hardness)+2.255))*(0.998)(CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Mud Slough Upstream of SLD Terminus.
Temporal Representation: | The samples were collected from Oct 26 2000 to Nov 21 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 8370
Pollutant: | Nitrate as Nitrate (NO3)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 1063 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. Using BinomBal listing is recommended if a sample size of 1063 has 177 or more samples that exceed the evaluation criteria. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 8370

LOE ID: | 7331
Pollutant: | Nitrate as Nitrate (NO3)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 1063
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 1063 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation guideline for Nitrate-N.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Nitrate-N levels should not to exceed 100 mg/L (USEPA National Ambient Water Quality Objective)
Guideline Reference: | National Recommended Water Quality Criteria. United States Environmental Protection Agency. Office of Water. Office of Science and Technology. 4304T
Spatial Representation: | Samples were collected at Mud Slough Upstream of SLD Terminus.
Temporal Representation: | The samples were collected from Jun 29 2000 to Jun 21 2007
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 8371
Pollutant: | Selenium
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 1 of 1561 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. Using BinomBal listing is recommended if a sample size of 1561 has 259 or more samples that exceed the evaluation criteria. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 8371

LOE ID: | 7332
Pollutant: | Selenium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 1561
Number of Exceedances: | 1
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | One of the 1561 samples collected by the Surface Water Ambient Monitoring Program exceeded the CTR for Selenium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | The CTR value for selenium is 5 ug/L.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Mud Slough Upstream of SLD Terminus.
Temporal Representation: | The samples were collected from Aug 20 1993 to Sep 27 2007
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 8372
Pollutant: | Zinc
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 23 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 8372

LOE ID: | 7334
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 23
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 23 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Zinc.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Zinc levels should not exceed the calculated limit based on the formula: Criteria Maximum Concentration=EXP((0.8473*LN(hardness))+0.884)*(0.978) (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Mud Slough Upstream of SLD Terminus.
Temporal Representation: | The samples were collected from Oct 26 2000 to Nov 21 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 13685
Pollutant: | pH
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. Nineteen of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Nineteen of 541 samples exceeded the pH objective and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 13685

LOE ID: | 23052
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 495
Number of Exceedances: | 17
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | The Central Valley Regional Water Quality Control Board Surface Water Ambient Monitoring Program collected 495 samples from October 1995 to June 2006. Seventeen out of 495 samples were outside the acceptable range; ten samples were higher than the acceptable range and seven samples were lower than the acceptable range.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | The pH of water shall not be depressed below 6.5,raised above 8.5, or changed at any time more than 0.5 units from normal ambient pH.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Measurement of pH within the range of 6.5 and 8.5
Guideline Reference:
Spatial Representation: | Samples were collected from Mud slough upstream San Luis Drain.
Temporal Representation: | Sampling occurred from October 1995 to June 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
LOE ID: | 23051
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 45
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | The Westside San Joaquin Water Quality Coalition collected 46 samples from July 2004 to October 2006. Two out of 45 samples were outside the acceptable range; both samples were lower than the acceptable range.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | The pH of water shall not be depressed below 6.5,raised above 8.5, or changed at any time more than 0.5 units from normal ambient pH.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Measurement of pH within the range of 6.5 and 8.5
Guideline Reference:
Spatial Representation: | Samples were collected from Mud Slough upstream San Luis Drain.
Temporal Representation: | Sampling occurred from July 2004 to October 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):

DECISION ID | 13686
Pollutant: | Escherichia coli (E. Coli)
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. Twenty-six of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Twenty-six of 74 samples exceed the E. Coli objective and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 13686

LOE ID: | 26019
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 45
Number of Exceedances: | 15
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | The Central Valley Regional Water Quality Control Board Surface Water Ambient Monitoring Program collected 89 samples from August 2002 to June 2006. Fifteen out of 45 samples exceeded the evaluation objective.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. The objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | The USEPA E. Coli objective of 235/100 mL in any single sample (USEPA 1986).
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Samples were collected at Mud Slough upstream of San Luis Drain.
Temporal Representation: | Sampling occurred from August 2002 to June 2006.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Boards Quality Assurance Program Plan for the State of Californias Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 23090
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 29
Number of Exceedances: | 11
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | The Westside San Joaquin River Water Quality Coalition collected 29 samples from August 2004 to October 2006. Eleven out of the 29 samples collected exceeded the evaluation objective.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. The objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | The USEPA E. Coli objective of 235/100 mL in any single sample (USEPA 1986).
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Samples were collected at Mud Slough upstream of San Luis Drain.
Temporal Representation: | Sampling occurred August 2004 to October 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):

DECISION ID | 12604
Pollutant: | Unknown Toxicity
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Six lines of evidence are available in the administrative record to assess this pollutant. Thirty-seven of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Twenty-four of 124 samples tested with fathead minnow exceed the narrative toxicity objective and this exceeds the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12604

LOE ID: | 23050
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 116
Number of Exceedances: | 10
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Ten of 116 samples tested with Selenastrum capricornutum were toxic and violated the narrative toxicity objective. Ten samples collected at Mud Slough Upstream San Luis Drain exhibited a statistically significant decrease in growth compared to the control. The sample dates and percent of control (in parentheses) are as follows:01 February 1997 (28)01 April 1997 (45)01 May 1997 (48)01 March 1999 (69)01 April 1999 (73)01 June 2001 (59)02 march 2002 (80)03 June 2003 (50)04 September 2004 (83)06 May 2006 (74)
Data Reference: | San Joaquin River SWAMP Monitoring Data - Grassland Bypass
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference was determined with ambient control (water from Delta Mendota Canal) for 4-day chronic-style toxicity tests. Data was evaluated using the TOXIS statistical package, which includes USEPA flow through chart. Statistics may include Fisher's exact test, Probit, Spearman-Karber, Dunnett's Procedure, Steel's Many-one Rank and the t-test. Depending on data input, TOXIS selects the most appropriate statistics
Guideline Reference: | Short-term Methods for Estimating the Chronic Toxicity of Effluents and Receiving Waters to Freshwater and Marine Organisms, Fourth Edition. U.S. Environmental Protection Agency Office of Water, Washington, DC EPA-821-R-02-013
Spatial Representation: | Samples were collected from Mud Slough Upstream San Luis Drain.
Temporal Representation: | Samples were collected from October 1996 to February 2007.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. This data meets all the requirments of the Grasslands Bypass Project QAPP.
QAPP Information Reference(s):
LOE ID: | 23036
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 28
Number of Exceedances: | 1
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | One of 28 samples tested with Selenastrum capricornutum was toxic and violated the narrative toxicity objective. One sample collected at Sand Dam exhibited a statistically significant decrease in growth compared to the control. The sample date and percent of control (in parentheses) are as follows:13 July 2004 (61)
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 4-day chronic-style toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from Mud Slough Upstream San Luis Drain.
Temporal Representation: | Samples were collected from July 2004 to October 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 22884
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 29
Number of Exceedances: | 1
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | One of the 29 samples tested with Ceriodaphnia dubia was toxic and violated the narrative toxicity objective. One sample collected at Mud Slough Upstream San Luis Drain exhibited a statistically significant decrease in growth compared to the control. The sample date and percent of control (in parentheses) are as follows:12 October 2004 (63)
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 4-day acute-style toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from Mud Slough Upstream San Luis Drain.
Temporal Representation: | Samples were collected from July 2004 to October 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 23034
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 30
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | None of the 30 samples tested with Pimephales promelas were toxic and violated the narrative toxicity objective.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 4-day acute-style toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from Mud Slough Upstream San Luis Drain
Temporal Representation: | Samples were collected from July 2004 to October 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 22885
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 124
Number of Exceedances: | 1
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | 1 of the 124 samples tested with Daphnia magna was toxic and violated the narrative toxicity objective. One sample collected at Mud Slough Upstream San Luis Drain exhibited a statistically significant decrease in survival compared to the control. The sample date and percent of control (in parentheses) are as follows:01 January 2001 (78)
Data Reference: | San Joaquin River SWAMP Monitoring Data - Grassland Bypass
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference was determined with ambient control (water from Delta Mendota Canal) for 7-day chronic-style toxicity tests. Data was evaluated using the TOXIS statistical package, which includes USEPA flow through chart. Statistics may include Fisher's exact test, Probit, Spearman-Karber, Dunnett's Procedure, Steel's Many-one Rank and the t-test. Depending on data input, TOXIS selects the most appropriate statistics
Guideline Reference:
Spatial Representation: | Samples were collected from Mud Slough Upstream San Luis Drain.
Temporal Representation: | Samples were collected from October 1996 to February 2007.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. This data meets all the requirments of the Grasslands Bypass Project QAPP.
QAPP Information Reference(s):
LOE ID: | 23035
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 124
Number of Exceedances: | 24
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Twenty-four of the 124 samples tested with Pimephales promelas were toxic and violated the narrative toxicity objective. Twenty-four samples collected at Mud Slough Upstream San Luis Drain exhibited a statistically significant decrease in growth compared to the control. The sample dates and percent of control (in parentheses) are as follows:01 December 1996 (51)01 February 1997 (90)01 November 1997 (77)01 December 1997 (57)01 January 1998 (44)01 February 1998 (46)01 March 1998 (63)01 October 1998 (55)01 November 1998 (61)01 December 1998 (73)01 November 1999 (44)01 December 1999 (73)01 January 2000 (40)01 October 2000 (75)01 November 2000 (16)01 December 2000 (72)01 December 2001 (56)02 November 2002 (55)03 January 2003 (74)03 March 2003 (85)03 December 2003 (45)04 January 2004 (59)04 December 2004 (69)05 December 2005 (29)
Data Reference: | San Joaquin River SWAMP Monitoring Data - Grassland Bypass
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference was determined with ambient control (water from Delta Mendota Canal) for 7-day chronic-style toxicity tests. Data was evaluated using the TOXIS statistical package, which includes USEPA flow through chart. Statistics may include Fisher's exact test, Probit, Spearman-Karber, Dunnett's Procedure, Steel's Many-one Rank and the t-test. Depending on data input, TOXIS selects the most appropriate statistics
Guideline Reference:
Spatial Representation: | Samples were collected from Mud Slough Upstream San Luis Drain.
Temporal Representation: | Samples were collected from October 1996 to February 2007.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. This data meets all the requirments of the Grasslands Bypass Project QAPP.
QAPP Information Reference(s):

DECISION ID | 13331
Pollutant: | Boron
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Original
Sources: | Source Unknown
Expected TMDL Completion Date: | 2019
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for removal from the section 303(d) list under section 4.1 of the Listing Policy. Under this section a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess pollutant. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against removing this water segment-pollutant combination from the section 303(d) list. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Pursuant to section 4.11 of the Listing Policy, no additional data and information are available indicating that standards are met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be removed from the section 303(d) list because applicable water quality standards for the pollutant are being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 13331

LOE ID: | 7238
Pollutant: | Boron
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Not Recorded
Beneficial Use: | Agricultural Supply
Number of Samples: | 0
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Unspecified--This LOE is a placeholder to support a 303(d) listing decision made prior to 2006.
Data Reference: | Placeholder reference pre-2006 303(d)
Water Quality Objective/Criterion: |
Objective/Criterion Reference:
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Unspecified
Temporal Representation: | Unspecified
Environmental Conditions: | Unspecified
QAPP Information: | Unspecified
QAPP Information Reference(s):

DECISION ID | 16117
Pollutant: | Pesticides
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Original
Sources: | Agriculture
Expected TMDL Completion Date: | 2019
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | 303(d) listing decisions made prior to 2006 were not held in an assessment database. This is a placeholder decision for a 303(d) listing made in a previous assessment cycle. The Regional Boards will update this decision when new data and information become available and are assessed.
RWQCB Board Decision / Staff Recommendation: | No new data were assessed for 2008. The Regional Board will update this decision when new data and information become available and are assessed.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16117

LOE ID: | 7246
Pollutant: | Pesticides
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Not Recorded
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 0
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Unspecified--This LOE is a placeholder to support a 303(d) listing decision made prior to 2006.
Data Reference: | Placeholder reference pre-2006 303(d)
Water Quality Objective/Criterion: |
Objective/Criterion Reference:
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Unspecified
Temporal Representation: | Unspecified
Environmental Conditions: | Unspecified
QAPP Information: | Unspecified
QAPP Information Reference(s):