# Draft 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 5 - Central Valley Region

Water Body Name: | Calaveras River, Lower (from New Hogan Reservoir to Bellota Weir)
Water Body ID: | CAR5313000020090428173756
Water Body Type: | Coastal & Bay Shoreline

DECISION ID | 16736
Pollutant: | Arsenic
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 2 samples exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. In addition, 0 of 2 samples exceeded the USEPA Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16736

LOE ID: | 28969
Pollutant: | Arsenic
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Arsenic.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Arsenic levels should not exceed 340 ug/L maximum concentration for 1-hour average (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Calaveras River at Monte Vista Trailhead.
Temporal Representation: | The samples were collected June 10, 2002 and June 24, 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 28972
Pollutant: | Arsenic
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Arsenic.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Arsenic levels should not exceed 10 ug/L (USEPA Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Calaveras River at Monte Vista Trailhead.
Temporal Representation: | The samples were collected June10, 2002 and June 24, 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 16751
Pollutant: | Cadmium
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. The recommendation is based on staff findings that 0 of 1 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. In addition, the recommendation is also based on staff findings that 0 of 2 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16751

LOE ID: | 29043
Pollutant: | Cadmium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 1 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Cadmium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Cadmium levels should not exceed the calculated limit based on the formula: Criteria Maximum Concentration (1-hour Average dissolved)=(EXP(1.128*LN(hardness)-3.6867))*(1.136672-(LN(hardness)*0.041838)) (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Sample was collected at Calaveras River at Monte Vista Trailhead.
Temporal Representation: | The sample was collected on June 10, 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 29045
Pollutant: | Cadmium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Cadmium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Cadmium levels should not exceed 5 ug/L (Department of Public Health Primary MCL).
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Calaveras River at Monte Vista Trailhead.
Temporal Representation: | The samples were collected on June 10, 2002 to June 24, 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 16753
Pollutant: | Chromium (total)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the Department of Public Health Primary MCL for Municipal and Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16753

LOE ID: | 29047
Pollutant: | Chromium (total)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Chromium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Chromium levels should not exceed 50 ug/L (Department of Public Health Primary MCL).
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Calaveras River at Monte Vista Trailhead.
Temporal Representation: | The samples were collected on June 10, 2002 and June 24, 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 16754
Pollutant: | Copper
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 1 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. In addition, 0 of 2 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16754

LOE ID: | 29051
Pollutant: | Copper
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Copper.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Copper levels should not exceed 1300 ug/L (Department of Public Health Primary MCL).
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Calaveras River at Monte Vista Trailhead.
Temporal Representation: | The samples were collected on June 10 2002 and June 24, 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 29049
Pollutant: | Copper
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 1 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for dissolved Copper.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | California Toxics Rule 4-day average criteria for dissolved Copper.
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Sample was collected at Calaveras River at Monte Vista Trailhead.
Temporal Representation: | The sample was collected on June 10, 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 16768
Pollutant: | Escherichia coli (E. Coli)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.3 of the Listing Policy. Under section 3.3 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 18 samples exceeded the US EPA E. Coli guideline and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16768

LOE ID: | 29067
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 18
Number of Exceedances: | 0
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | None of the 18 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation guideline for E. coli bacteria.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | E. coli bacteria levels should not exceed 235 MPN/100 mL in any single sample (USEPA E. coli Guideline).
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Eighteen samples were collected from the lower Calaveras River at Monte Vista Trailhead.
Temporal Representation: | Samples were collected March 2002 to December 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 16756
Pollutant: | Lead
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. The recommendation is based on staff findings that 0 of 1 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 2 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16756

LOE ID: | 29053
Pollutant: | Lead
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Lead.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Lead levels should not exceed 15 ug/L (Department of Public Health Primary MCL).
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Calaveras River at Monte Vista Trailhead.
Temporal Representation: | The samples were collected on June 10, 2002 and June 24, 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 29055
Pollutant: | Lead
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 1 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Lead.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Lead levels should not exceed the calculated value based on the formula: Criteria Maximum Concentration (1-hour Average, dissolved)=(EXP(1.273*LN(hardness)-1.46))*(1.46203-(LN(hardness)*0.145712)) (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Sample was collected at Calaveras River at Monte Vista Trailhead.
Temporal Representation: | The samples was collected on June 10, 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 16759
Pollutant: | Nickel
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. The recommendation is based on staff findings that 0 of 1 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 2 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16759

LOE ID: | 29060
Pollutant: | Nickel
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Nickel.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Nickel levels should not exceed 100 ug/L (Department of Public Health Primary MCL).
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Calaveras River at Monte Vista Trailhead.
Temporal Representation: | The samples were collected on June 10, 2002 and June 24, 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 29058
Pollutant: | Nickel
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 1 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Nickel.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Nickel levels should not exceed the calculated limit based on the formula: Criteria Maximum Concentration (1-hour Average, dissolved)=(EXP(0.846*LN(hardness)+2.255))*(0.998)(CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Calaveras River at Monte Vista Trailhead.
Temporal Representation: | The samples was collected on June 10, 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 16761
Pollutant: | Nitrate as Nitrate (NO3)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the USEPA National Ambient Water Quality Objective for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 2 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16761

LOE ID: | 29064
Pollutant: | Nitrate as Nitrate (NO3)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation guideline for Nitrate-N.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Nitrate-N levels should not to exceed 100 mg/L (USEPA National Ambient Water Quality Objective)
Guideline Reference: | National Recommended Water Quality Criteria. United States Environmental Protection Agency. Office of Water. Office of Science and Technology. 4304T
Spatial Representation: | Samples were collected at Calaveras River at Monte Vista Trailhead.
Temporal Representation: | The samples were collected on June 10, 2002 and June 24, 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 29062
Pollutant: | Nitrate as Nitrate (NO3)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Nitrate-N.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Nitrate-N levels should not exceed 45 mg/L (Department of Public Health Primary MCL).
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Calaveras River at Monte Vista Trailhead.
Temporal Representation: | The samples were collected on June 10, 2002 and June 24, 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 16732
Pollutant: | Sediment Toxicity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 1 samples exceeded the sediment toxicity objective and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16732

LOE ID: | 28944
Pollutant: | Sediment Toxicity
LOE Subgroup: | Toxicity
Matrix: | Sediment
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | One sample tested with Hyalella azteca was not toxic and did not violate the narrative toxicity objective.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 10-day Hyalella azteca sediment toxicity tests.
Guideline Reference: | Methods for Measuring the Toxicity and Bioaccumulation of Sediment-associated Contaminants with Freshwater Invertebrates, Second Edition. U.S. Environmental Protection Agency Office of Research and Development, Duluth, MI , U.S. Environmental Protection Agency Office of Water, Washington, DC EPA-600/R-99/064
Spatial Representation: | The sample was collected from Calaveras River at Monte Vista trailhead.
Temporal Representation: | The sample was collected in May 2002.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)

DECISION ID | 16769
Pollutant: | Specific Conductivity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. The recommendation is based on staff findings that 0 of 24 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16769

LOE ID: | 29069
Pollutant: | Specific Conductivity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 24
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 24 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Specific Conductivity.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | The water quality objective used was the California Secondary MCL recommended level of 900 uS/cm. The Basin Plan includes chemical constituent water quality objectives that include (by reference) secondary maximum contaminant levels (MCLs) protective of MUN (CVRWQCB, 2007a).The secondary MCLs for electrical conductivity provide a range of values including a recommended level (900 uS/cm), upper level (1600 uS/cm) and a short-term level (2200 uS/cm). The recommended concentration was used as it is intended to be protective of all drinking water uses.
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Calaveras River at Monte Vista Trailhead.
Temporal Representation: | The samples were collected from January 2002 to December 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 16735
Pollutant: | Unknown Toxicity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.6 of the Listing Policy. Under section 3.6 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 1 samples exceeded the invertebrate toxicity objective and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. In addition, None of 1 samples exceeded the vertebrate toxicity objective and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16735

LOE ID: | 28951
Pollutant: | Vertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | One water sample, collected from the lower Calaveras River under the Surface Water Ambient Monitoring Program, and tested for acute tocity with Pimephales promelas (Fathead Minnow, a vertebrate species) did not exhibit a statistically significant decrease in survival compared to control (the sample did not violate the narrative toxicity objective).
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a Fisher's Exact analysis with 4-day acute-style toxicity tests.
Guideline Reference: | Methods for Measuring the Acute Toxicity of Effluents and Receiving Waters to Freshwater and Marine Organisms, Fifth Edition. U.S. Environmental Protection Agency Office of Water, Washington, DC EPA-821-R-02-012
Spatial Representation: | One water sample was collected from the lower Calaveras River at Highway 88.
Temporal Representation: | One water sample was collected by the SWAMP on 3 September 2002.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
LOE ID: | 28953
Pollutant: | Invertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | One water sample, collected from the lower Calaveras River under the Surface Water Ambient Monitoring Program, and tested for acute tocity with Ceriodaphnia dubia (an invertebrate species) did not exhibit a statistically significant decrease in survival compared to control (the sample did not violate the narrative toxicity objective.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a Fisher's Exact analysis with 4-day acute-style toxicity tests.
Guideline Reference: | Methods for Measuring the Acute Toxicity of Effluents and Receiving Waters to Freshwater and Marine Organisms, Fifth Edition. U.S. Environmental Protection Agency Office of Water, Washington, DC EPA-821-R-02-012
Spatial Representation: | One water sample was collected from the lower Calaveras River at Highway 88.
Temporal Representation: | One water sample was collected on 3 September 2002.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)

DECISION ID | 16772
Pollutant: | Zinc
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. The recommendation is based on staff findings that 0 of 1 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 2 available concentrations exceeded the Department of Public Health Secondary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16772

LOE ID: | 29073
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 1 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Zinc.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Zinc levels should not exceed the calculated limit based on the formula: Criteria Maximum Concentration=EXP((0.8473*LN(hardness))+0.884)*(0.978) (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Calaveras River at Monte Vista Trailhead.
Temporal Representation: | The sample was collected on June 10, 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 29071
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Zinc.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Northeast Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Zinc levels should not exceed 5000 ug/L (Department of Public Health Secondary MCL).
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Calaveras River at Monte Vista Trailhead.
Temporal Representation: | The samples were collected on June 10, 2002 and June 24, 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 16774
Pollutant: | pH
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 13 samples exceeded the Basin Plan objective and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16774

LOE ID: | 29076
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | The Central Valley Regional Water Quality Control Board Surface Water Ambient Monitoring Program collected 24 samples from January 2002 to December 2002. None of the 13 samples had pH values outside the acceptable range.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | The pH of water shall not be depressed below 6.5,raised above 8.5, or changed at any time more than 0.5 units from normal ambient pH. Measurement of pH within the range of 6.5 and 8.5. A low pH has a value less than 6.5.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Calaveras River at Monte Vista trailhead.
Temporal Representation: | Sampling occurred from January 2002 to December 2002.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)