# Final 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 5 - Central Valley Region

Water Body Name: | Sutter Creek (tributary to Dry Creek, Amador County)
Water Body ID: | CAR5311100020080801155330
Water Body Type: | River & Stream

DECISION ID | 10325
Pollutant: | Arsenic
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the USEPA Primary MCL and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the California Toxics Rule and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10325

LOE ID: | 20605
Pollutant: | Arsenic
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Neither of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the USEPA Primary MCL of 10 ug/L for total arsenic
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | Total arsenic levels must not exceed the USEPA Primary MCL of 10 ug/L
Objective/Criterion Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Sutter Creek at Highway 49
Temporal Representation: | The samples were collected on June 13 ,2002 and June 26, 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 8651
Pollutant: | Arsenic
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Neither of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the CTR criterion of 340 ug/L for dissolved arsenic
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | Dissolved arsenic levels should not exceed the CTR 1-hour average maximum concentration of 340 ug/L
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Sutter Creek at Highway 49
Temporal Representation: | The samples were collected on June 13, 2002 and on June 26, 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10327
Pollutant: | Cadmium
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 2 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10327

LOE ID: | 8653
Pollutant: | Cadmium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Neither of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the calculated CTR criterion for dissolved cadmium
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | Dissolved cadmium levels should not exceed the calculated limit based on the formula: Criteria Maximum Concentration (1-hour Average dissolved)=(EXP(1.128*LN(hardness)-3.6867))*(1.136672-(LN(hardness)*0.041838))
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Sutter Creek at Highway 49
Temporal Representation: | The samples were collected on June 13, 2002 and June 26, 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 20600
Pollutant: | Cadmium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Neither of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the USEPA Primary MCL of 5 ug/L for total cadmium
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | Total cadmium levels should not exceed the USEPA Primary MCL of 5 ug/L
Objective/Criterion Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected from Sutter Creek at Highway 49
Temporal Representation: | The samples were collected on June 13, 2002 and June 26, 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10329
Pollutant: | Chromium (total)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the Department of Public Health Primary MCL for Municipal and Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met. "
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10329

LOE ID: | 20644
Pollutant: | Chromium (total)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Zero of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Chromium.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Chromium levels should not exceed 50 ug/L (Department of Public Health Primary MCL).
Guideline Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Spatial Representation: | Samples were collected at Sutter Creek at Highway 49.
Temporal Representation: | The samples were collected from June 13 2002 to June 26 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10333
Pollutant: | Copper
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 2 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. In addition, 0 of 2 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10333

LOE ID: | 20618
Pollutant: | Copper
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Copper.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | Copper levels should not exceed 1300 ug/L (Department of Public Health Primary MCL).
Objective/Criterion Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Sutter Creek at Highway 49.
Temporal Representation: | The samples were collected from June 13, 2002 to June 26, 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 8655
Pollutant: | Copper
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Zero of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Copper.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | California Toxics Rule 4-day average criteria for dissolved Copper.
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Sutter Creek at Highway 49.
Temporal Representation: | The samples were collected June 13, 2002 and June 26, 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 11667
Pollutant: | Escherichia coli (E. Coli)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. Three of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Three of 14 samples exceeded the E. Coli objective and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 11667

LOE ID: | 23320
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 14
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | The Central Valley Regional Water Quality Control Board Surface Water Ambient Monitoring Program collected 14 samples from March 2002 to December 2002. Three of the 14 samples exceeded the evaluation objective.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. The objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | The USEPA E. Coli objective of 235/100 mL in any single sample (USEPA 1986).
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Samples were collected at Sutter Creek at Highway 49.
Temporal Representation: | Sampling occurred from March 2002 to December 2002.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)

DECISION ID | 10336
Pollutant: | Lead
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 2 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10336

LOE ID: | 20712
Pollutant: | Lead
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Neither of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the Primary MCL of 15 ug/L for total lead
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | Total lead levels should not exceed 15 ug/L (Department of Public Health Primary MCL)
Objective/Criterion Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Sutter Creek at Highway 49
Temporal Representation: | The samples were collected on June 13, 2002 and on June 26, 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 8659
Pollutant: | Lead
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Neither of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the calculated CTR CMC for dissolved lead
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | Dissolved lead levels should not exceed the calculated CTR value based on the formula: Criteria Maximum Concentration (1-hour Average, dissolved)=(EXP(1.273*LN(hardness)-1.46))*(1.46203-(LN(hardness)*0.145712))
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Sutter Creek at Highway 49.
Temporal Representation: | The samples were collected on June 13, 2002 and on June 26, 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10345
Pollutant: | Nickel
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 2 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10345

LOE ID: | 20748
Pollutant: | Nickel
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Neither of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the Primary MCL of 100 ug/L for total nickel
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | Total nickel levels should not exceed 100 ug/L (Department of Public Health Primary MCL)
Objective/Criterion Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Sutter Creek at Highway 49
Temporal Representation: | The samples were collected on June 13, 2002 and on June 26, 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 8663
Pollutant: | Nickel
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the calculated CTR CMC for dissolved nickel
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | Dissolved nickel levels should not exceed the calculated CTR limit based on the formula: Criteria Maximum Concentration (1-hour Average, dissolved)=(EXP(0.846*LN(hardness)+2.255))*(0.998)
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Sutter Creek at Highway 49
Temporal Representation: | The samples were collected on June 13, 2002, and on June 26, 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10346
Pollutant: | Nitrate
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the USEPA Primary MCL and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the USEPA National Ambient Water Quality Objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10346

LOE ID: | 8667
Pollutant: | Nitrate as Nitrate (NO3)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation guideline for Nitrate-N.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Nitrate-N levels should not to exceed 100 mg/L (USEPA National Ambient Water Quality Objective)
Guideline Reference: | National Recommended Water Quality Criteria. United States Environmental Protection Agency. Office of Water. Office of Science and Technology. 4304T The Blue Book
Spatial Representation: | Samples were collected at Sutter Creek at Highway 49.
Temporal Representation: | The samples were collected from Jun 13 2002 to Jun 26 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 20758
Pollutant: | Nitrate as Nitrate (NO3)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Nitrate-N.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Nitrate-N levels should not exceed 45 mg/L (Department of Public Health Primary MCL)
Guideline Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Spatial Representation: | Samples were collected at Sutter Creek at Highway 49.
Temporal Representation: | The samples were collected from Jun 13 2002 to Jun 26 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 9223
Pollutant: | Oxygen, Dissolved
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 1 of 21 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.2 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met. "
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9223

LOE ID: | 8656
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 21
Number of Exceedances: | 1
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | One of the 21 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Dissolved Oxygen. The exceeded results are as follows: 11/7/2002 - a sample taken at Sutter Creek at Highway 49 had a result of 5.7mg/L.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | The Basin Plan Objective sets the minimum Dissolved Oxygen content at 7 mg/L
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Sutter Creek at Highway 49.
Temporal Representation: | The samples were collected from Jan 9 2002 to Dec 23 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 11668
Pollutant: | Sediment Toxicity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 1 samples exceeded the narrative toxicity objective and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 11668

LOE ID: | 23321
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Sediment
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Only one sample tested with Hyalella azteca survival.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 10-day Hyalella azteca sediment toxicity tests.
Guideline Reference: | Methods for Measuring the Toxicity and Bioaccumulation of Sediment-associated Contaminants with Freshwater Invertebrates, Second Edition. U.S. Environmental Protection Agency Office of Research and Development, Duluth, MI , U.S. Environmental Protection Agency Office of Water, Washington, DC EPA-600/R-99/064
Spatial Representation: | Sample was collected from Sutter Creek at Highway 49.
Temporal Representation: | Sample was collected on May 31, 2002.
Environmental Conditions: |
QAPP Information: | Data quality: Fair. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)

DECISION ID | 10347
Pollutant: | Selenium
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that only 1 sample is available and a minimum of 2 samples is needed for evaluation under section 3.1 for the Municipal Beneficial Use and for the Cold Water Habitat.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because it cannot be determined if applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10347

LOE ID: | 8664
Pollutant: | Selenium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Zero of the 1 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Selenium.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Selenium levels should not to exceed 5 ug/L (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Sample was collected at Sutter Creek at Highway 49.
Temporal Representation: | The sample was collected on October24 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 20273
Pollutant: | Selenium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 1 sample collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Selenium.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Selenium levels should not exceed 50 ug/L (Department of Public Health Primary MCL)
Guideline Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Spatial Representation: | The sample was collected at Sutter Creek at Highway 49.
Temporal Representation: | The sample was collected on Oct 24 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10352
Pollutant: | Specific Conductivity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 21 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.2 of the Listing Policy. Table 3.2 of the listing policy recommends listing if a sample size of 21 has 5 or more samples that exceed the evaluation criteria. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10352

LOE ID: | 20854
Pollutant: | Specific Conductivity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 21
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 21 samples collected by the Surface Water Ambient Monitoring Program exceeded the "recommended" Secondary MCL of 900 uS/cm for electrical conductivity
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | The secondary MCLs for electrical conductivity provide a range of values including a "recommended" level (900 uS/cm), upper level (1600 uS/cm) and a short-term level (2200 uS/cm). The recommended concentration was used as it is intended to be protective of all drinking water uses
Objective/Criterion Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Sutter Creek at Highway 49
Temporal Representation: | The samples were collected between January 9, 2002 and December 23, 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10353
Pollutant: | Zinc
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 2 available concentrations exceeded the Department of Public Health Secondary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10353

LOE ID: | 8666
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the calculated CTR CMC for dissolved zinc
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | Dissolved zinc levels should not exceed the calculated CTR limit based on the formula: Criteria Maximum Concentration=EXP((0.8473*LN(hardness))+0.884)*(0.978)
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Sutter Creek at Highway 49
Temporal Representation: | The samples were collected on June 13, 2002, and on June 26, 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 20771
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Zero of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the Secondary MCL for total zinc
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | Total zinc levels should not exceed 5,000 ug/L (Department of Public Health Secondary MCL)
Objective/Criterion Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Sutter Creek at Highway 49
Temporal Representation: | The samples were collected on June 13, 2002 and on June 26, 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 9226
Pollutant: | pH
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 21 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.2 of the Listing Policy. Table 3.2 of the listing policy recommends listing if a sample size of 21 has 5 or more samples that exceed the evaluation criteria. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9226

LOE ID: | 8657
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 21
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 21 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for pH.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | pH levels should not be lower than 6.5 or higher than 8.5 (Basin Plan Objective)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Sutter Creek at Highway 49.
Temporal Representation: | The samples were collected from Jan 9 2002 to Dec 23 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):