**Field Measurement Data (with YSI probe)**

**County Island (2017-18 Storm Year)**

The following results indicate the field measurements/parameters collected for the three (3) Wet weather events in 2017-2018 storm year.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Monitoring Station** | **CIMP Group Affected** | **Sample Date** | **Event Type** | **Field Parameters** | **Reason for Field Parameter Collection Being Missed** | **Resolution** |
| CUA-PVD-01 | Los Cerritos Channel | 1/7/2018 | Wet | Temp., pH, Specific Conductance, Dissolved Oxygen, & Salinity | Equipment was not available to take measurements. | To collect field data for the next sampling event |
| CUA-PVD-01 | Los Cerritos Channel | 3/10/2018 | Wet | Temp., pH, Specific Conductance, Dissolved Oxygen, & Salinity | Minor, trickle flow; less flow depth to use YSI probe to obtain field data | To collect field data for the next sampling event |
| CUA-PVD-01 | Los Cerritos Channel | 3/15/2018 | Wet | Temp., pH, Specific Conductance, Dissolved Oxygen, & Salinity | Minor, Trickle flow; less flow depth to use YSI probe to obtain field data | To collect field data for the next or future sampling events |