# Draft 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 3 - Central Coast Region

Water Body Name: | Alisal Creek (Monterey County)
Water Body ID: | CAR3097009519990222130537
Water Body Type: | River & Stream

DECISION ID | 4398
Pollutant: | Fecal Coliform
Final Listing Decision: | Do Not Delist from 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | Do Not Delist from 303(d) list (TMDL required list)(2006)
Revision Status | Revised
Sources: | Agriculture | Natural Sources | Nonpoint Source | Urban Runoff/Storm Sewers
Expected TMDL Completion Date: | 2013
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for removal from the section 303(d) list under section 4.3 (Bacteria) of the Listing Policy. Under section 4.3 a single line of evidence is adequate to assess listing status. The 2008 Line of Evidence (LOE # 10843) is identical to and replaces the 2006 LOE (LOE# 1887).Therefore, two lines of evidence are available in the administrative record to assess this pollutant. Per Table 4.2 of the Policy, at least 26 numeric samples are required in order to reliably compare data against an applicable water quality objective. However, a total of less than 26 numeric samples are available in this case. Central Coast Water Board staff require a minimum of 26 samples to make a "Use Rating" decision of Fully Supporting. Based on the readily available data and information, the weight of evidence indicates that there is insufficient justification in favor of removing this water segment-pollutant combination from the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Less than 26 samples were available for analysis. More samples are needed in order to reliably determine if a water quality objective is exceeded. Five of six samples exceeded the water contact recreation objective. 4. Pursuant to section 4.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | No new data were assessed for 2008. The decision has not changed.
SWRCB Board Decision / Staff Recommendation: | After review of the available data and information, SWRCB staff concludes that the water body-pollutant combination should not be removed from the section 303(d) list because it cannot be determined if applicable water quality standards are attained.
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 4398

LOE ID: | 1887
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 6
Number of Exceedances: | 5
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Five of 6 samples exceed the water quality objective (CCAMP, 2004).
Data Reference: | Placeholder reference 2006 303(d)
Water Quality Objective/Criterion: | Basin Plan: Fecal coliform concentration, based on minimum of not less than five samples or any 30-day period, shall not exceed a log mean of 200/100 ml, nor shall more than ten percent of the total samples during any 30-day period exceed 400/100 ml.
Objective/Criterion Reference: | Placeholder reference 2006 303(d)
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | There was one sampling site.
Temporal Representation: | Summer, fall, and winter sampling events.
Environmental Conditions: |
QAPP Information: | CCAMP QAPP.
QAPP Information Reference(s):
LOE ID: | 10843
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 6
Number of Exceedances: | 5
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 5 of 6 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 200 MPN/100 ml, nor shall more than ten percent of total samples during any 30-day period exceed 400 MPN/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected over the time period 7/28/1999-2/10/2000. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 10857
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 6
Number of Exceedances: | 3
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 3 of 6 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected over the time period 7/28/1999-2/10/2000. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 4397
Pollutant: | Nitrate
Final Listing Decision: | Do Not Delist from 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | Do Not Delist from 303(d) list (TMDL required list)(2006)
Revision Status | Revised
Sources: | Agriculture | Nonpoint Source | Urban Runoff/Storm Sewers
Expected TMDL Completion Date: | 2013
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | The pollutant name for this decision has been changed from "Nitrate as NO3" to "Nitrate". The decision has not changed. This pollutant is being considered for removal from the section 303(d) list under section 4.1 of the Listing Policy. Under section 4.1 a single line of evidence is adequate to assess listing status. Using the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.1. Four lines of evidence are available in the administrative record to assess this pollutant. Five of 6 samples exceeded the Municipal and Domestic Supply water quality objective for Nitrate and 1 of 6 samples exceeded the Agricultural Supply water quality objective for Nitrate. In addition, all 6 samples exceeded the Evaluation Guideline for Nitrate established for aquatic life beneficial uses using the Numeric Nutrient Endpoint tool. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against removing this water segment-pollutant combination from the section 303(d) list. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Five of 6 samples exceeded the Municipal and Domestic Supply water quality objective for Nitrate and this exceeds the allowable frequency calculated from the equation in Table 4.1 of the Listing Policy. 4. In addition, all 6 samples exceeded the Evaluation Guideline for Nitrate established for aquatic life beneficial uses using the Numeric Nutrient Endpoint tool and this exceeds the allowable frequency calculated from the equation in Table 4.1 of the Listing Policy. 5. Pursuant to section 4.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be removed from the section 303(d) list because applicable water quality standards for the pollutant are being exceeded.
SWRCB Board Decision / Staff Recommendation: | After review of the available data and information, SWRCB staff concludes that the water body-pollutant combination should not be removed from the section 303(d) list because it cannot be determined if applicable water quality standards are attained.
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 4397

LOE ID: | 10057
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 6
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 1 of 6 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when nitrate exceeds 30 mg/L NO3 as N in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected over the time period 7/28/1999-2/10/2000. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 10058
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 6
Number of Exceedances: | 5
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 5 of 6 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin Objective for municipal and domestic supply uses of inland surface waters (Section II.A.2) states the following: waters shall not contain concentrations of chemical constituents in excess of the limits specified in California Code of Regulations, Title 22, Article 4, Chapter 15, Section 64435, Tables 2 and 3 as listed in Table 3-2. The maximum contaminant level listed in Table 3-2 (inorganic and fluoride concentrations not to be exceeded in domestic or municipal supply) for nitrate is 10.0 mg/L (NO3 as N).
Objective/Criterion Reference: | Title 22, Division 4, Ch. 15, Article 4, Section 64431, Table 64431-A
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected over the time period 7/28/1999-2/10/2000. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 27845
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 6
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Data for this assessment unit was collected by one monitoring project: CCAMP Salinas (Salinas).
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Technical approach to develop nutrient numeric endpoints for California, Tetra Tech, June 2006. The Central Coast Region numeric target for maximum nitrate concentration is based on the Tetra Tech NNE (Nutrient Numeric Endpoint) Model and CCAMP data for 193 sites, monitored monthly for at least 1 year between January 1998 and December 2006. The model numeric target for aquatic life habitats in the Central Coast Region is 1.0 mg/L Nitrate as N.
Guideline Reference: | Technical Approach to Develop Nutrient Numeric Endpoints for California
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ].
Temporal Representation: | Data was collected over the time period 7/28/1999-2/10/2000. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 27847
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 6
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Data for this assessment unit was collected by one monitoring project: CCAMP Salinas (Salinas)
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Technical approach to develop nutrient numeric endpoints for California, Tetra Tech, June 2006. The Central Coast Region numeric target for maximum nitrate concentration is based on the Tetra Tech NNE (Nutrient Numeric Endpoint) Model and CCAMP data for 193 sites, monitored monthly for at least 1 year between January 1998 and December 2006. The model numeric target for aquatic life habitats in the Central Coast Region is 1.0 mg/L Nitrate as N.
Guideline Reference: | Technical Approach to Develop Nutrient Numeric Endpoints for California
| Technical Paper - Interpreting Narrative Objectives for Biostimulatory Substances Using the Technical Approach for Developing California Nutrient Numeric Endpoints. Central Coast Region
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected over the time period 7/28/1999-2/10/2000. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10033
Pollutant: | Boron
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. Zero of the six samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. There are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 26 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Zero of six samples exceeded the objective, and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10033

LOE ID: | 10041
Pollutant: | Boron
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Agricultural Supply
Number of Samples: | 6
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 0 of 6 samples exceed the criterion for Boron, dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. In addition, waters used for irrigation and livestock watering shall not exceed concentrations for those chemicals listed in Table 3.4 (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). Table 3-4 (page III-9) lists the maximum concentration for boron for irrigation supply is 0.75 mg/L.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected over the time period 7/28/1999-2/10/2000. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10355
Pollutant: | Chloride
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. Three of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 26 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Three of six samples exceeded the objective and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10355

LOE ID: | 10042
Pollutant: | Chloride
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 6
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 3 of 6 samples exceed the criterion for Chloride.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when chloride exceeds 106 mg/L in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected over the time period 7/28/1999-2/10/2000. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 15436
Pollutant: | Dieldrin
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. Neither sample exceeds the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither sample exceeds the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15436

LOE ID: | 19498
Pollutant: | Dieldrin
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Don Westin Toxicity study (R3_Weston) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Dieldrin.
Data Reference: | Final Data File used for assessment: Don Weston Salinas Toxicity Data
| Final Data File used for assessment: Don Weston_Salinas CCMP Data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for dieldrin is 61.8 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 2 monitoring sites [ 309SA1 - Alisal Creek at Old Stage Road, 309SA2 - Alisal Creek at Alisal Road]
Temporal Representation: | Data was collected on a single day 9/23/2005.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | No QAPP was prepared specifically for this project. However the work was conducted consistent with an approved QAPP from a previous project. That QAPP is available upon request.
QAPP Information Reference(s): | e-mail clarifying QAPP information
LOE ID: | 19499
Pollutant: | Dieldrin
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Don Westin Toxicity study (R3_Weston) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Dieldrin.
Data Reference: | Final Data File used for assessment: Don Weston Salinas Toxicity Data
| Final Data File used for assessment: Don Weston_Salinas CCMP Data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for dieldrin is 61.8 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 2 monitoring sites [ 309SA1 - Alisal Creek at Old Stage Road, 309SA2 - Alisal Creek at Alisal Road]
Temporal Representation: | Data was collected on a single day 9/23/2005.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | No QAPP was prepared specifically for this project. However the work was conducted consistent with an approved QAPP from a previous project. That QAPP is available upon request.
QAPP Information Reference(s): | e-mail clarifying QAPP information

DECISION ID | 15437
Pollutant: | Endrin
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. Neither sample exceeds the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Neither sample exceeds the Evaluation Guideline (MacDonald et al. 2000) as it applies to aquatic life objectives and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15437

LOE ID: | 19549
Pollutant: | Endrin
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Don Westin Toxicity study (R3_Weston) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Endrin.
Data Reference: | Final Data File used for assessment: Don Weston Salinas Toxicity Data
| Final Data File used for assessment: Don Weston_Salinas CCMP Data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for endrin is 207 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 2 monitoring sites [ 309SA1 - Alisal Creek at Old Stage Road, 309SA2 - Alisal Creek at Alisal Road]
Temporal Representation: | Data was collected on a single day 9/23/2005.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | No QAPP was prepared specifically for this project. However the work was conducted consistent with an approved QAPP from a previous project. That QAPP is available upon request.
QAPP Information Reference(s): | e-mail clarifying QAPP information
LOE ID: | 19526
Pollutant: | Endrin
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Don Westin Toxicity study (R3_Weston) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Endrin.
Data Reference: | Final Data File used for assessment: Don Weston Salinas Toxicity Data
| Final Data File used for assessment: Don Weston_Salinas CCMP Data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. (Water Quality Control Plan, Central Coast Basin, General Objective Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | In fresh water sediments the probable effects level (predictive of sediment toxicity) for endrin is 207 ug/Kg dry weight (MacDonald et al. 2000).
Guideline Reference: | Development and evaluation of consensus-based sediment effect concentrations for polychlorinated biphenyls. Environmental Toxicology and Chemistry. 19(5): 1403-1413
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 2 monitoring sites [ 309SA1 - Alisal Creek at Old Stage Road, 309SA2 - Alisal Creek at Alisal Road]
Temporal Representation: | Data was collected on a single day 9/23/2005.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | No QAPP was prepared specifically for this project. However the work was conducted consistent with an approved QAPP from a previous project. That QAPP is available upon request.
QAPP Information Reference(s): | e-mail clarifying QAPP information

DECISION ID | 10360
Pollutant: | Low Dissolved Oxygen
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Eight lines of evidence are available in the administrative record to assess these pollutants. One of the 6 samples exceed the dissolved oxygen water quality objective for Cold Freshwater Habitat but none of the 6 samples exceed the dissolved oxygen water quality objective for Warm Freshwater Habitat. However, four of 6 samples exceed the general water quality objective for oxygen saturation (when applied as a single sample maximum). This also exceeds the Basin Plan objective which states that the median oxygen saturation value shall not fall below 85%. This does not exceed the allowable frequency in table 3.2 of the listing policy which states that a minimum of five samples must exceed the objective in order to recommending adding the water segment-pollutant combination to the Section 303(d) list. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 26 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. One of the 6 samples exceed the dissolved oxygen water quality objective for Cold Freshwater Habitat but none of the 6 samples exceed the dissolved oxygen water quality objective for Warm Freshwater Habitat. However, four of 6 samples exceed the general water quality objective for oxygen saturation (when applied as a single sample maximum). None of these exceed the allowable frequency listed in Table 3.2 of the Listing Policy. In addition, the median value did not exceed the General Objective. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10360

LOE ID: | 12835
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, dissolved oxygen concentration shall not be reduced below 5.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected on a single day 10/1/1999. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 12849
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 1 of 1 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected on a single day 10/1/1999. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 12635
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 5
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 3 of 5 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected over the time period 7/28/1999-2/10/2000. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 12633
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 5
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 1 of 5 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected over the time period 7/28/1999-2/10/2000. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 12834
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected on a single day 10/1/1999. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 12636
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 5
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 3 of 5 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected over the time period 7/28/1999-2/10/2000. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 12634
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 5
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 0 of 5 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, dissolved oxygen concentration shall not be reduced below 5.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected over the time period 7/28/1999-2/10/2000. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 12578
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 1 of 1 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected on a single day 10/1/1999. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10354
Pollutant: | Nitrogen, ammonia (Total Ammonia)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 26 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Zero of 6 samples exceeded the evaluation guideline and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10354

LOE ID: | 10028
Pollutant: | Ammonia as Nitrogen
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 6
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 0 of 6 samples exceed the criterion for Ammonia as N, Total.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | USEPA Health Advisory 2006 Edition of the Drinking Water Standards and Health Advisories (EPA 822-R-06-013, 2006).
Objective/Criterion Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Evaluation Guideline: | EPA's Lifetime Health advisory level for total ammonia is 30.0 mg/L as stated on page 8 of the 2006 edition of the drinking water standards and health advisories. This Advisory Level is defined as "the concentration of a chemical in drinking water that is not expected to cause any adverse noncarcinogenic effects for up to ten days of exposure."
Guideline Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected over the time period 7/28/1999-2/10/2000. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10361
Pollutant: | Salinity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. Neither of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Zero of 2 samples exceeded the objective and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10361

LOE ID: | 12652
Pollutant: | Salinity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Salinity.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when salinity exceeds 3.0 ppt in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected over the time period 7/28/1999-2/10/2000. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 16087
Pollutant: | Sediment Toxicity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.6 of the Listing Policy. Under section 3.6 a single line of evidence is necessary to assess listing status for toxicity. Two lines of evidence are available in the administrative record to assess this pollutant in sediment samples. One of the 2 samples were toxic to invertebrate test organisms (exhibit a significant increase in mortality compared to the laboratory control) and therefore do not exceed the narrative General Objective for toxicity, set to protect for aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. One of the 2 samples were toxic to invertebrate test organisms and this does not exceed the allowable frequency in table 3.1 of the listing policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16087

LOE ID: | 23550
Pollutant: | Invertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 1
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Don Westin Toxicity study (R3_Weston) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 1 of 2 samples exceed the criterion for Toxicity, Hyalella azteca Survival (%) 10 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: Don Weston Salinas Toxicity Data
| Final Data File used for assessment: Don Weston_Salinas CCMP Data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 2 monitoring sites [ 309SA1 - Alisal Creek at Old Stage Road, 309SA2 - Alisal Creek at Alisal Road]
Temporal Representation: | Data was collected on a single day 9/23/2005.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | No QAPP was prepared specifically for this project. However the work was conducted consistent with an approved QAPP from a previous project. That QAPP is available upon request.
QAPP Information Reference(s): | e-mail clarifying QAPP information
LOE ID: | 23551
Pollutant: | Invertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Sediment
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 1
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Don Westin Toxicity study (R3_Weston) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 1 of 2 samples exceed the criterion for Toxicity, Hyalella azteca Survival (%) 10 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: Don Weston Salinas Toxicity Data
| Final Data File used for assessment: Don Weston_Salinas CCMP Data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 2 monitoring sites [ 309SA1 - Alisal Creek at Old Stage Road, 309SA2 - Alisal Creek at Alisal Road]
Temporal Representation: | Data was collected on a single day 9/23/2005.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | No QAPP was prepared specifically for this project. However the work was conducted consistent with an approved QAPP from a previous project. That QAPP is available upon request.
QAPP Information Reference(s): | e-mail clarifying QAPP information

DECISION ID | 15438
Pollutant: | Chlorophyll-a
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture
Expected TMDL Completion Date: | 2013
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. Five of the 6 samples exceed the Evaluation Guideline (North Carolina Administrative code, Title 15A) and the General Water Quality Objective set to protect aquatic life beneficial uses. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification for placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Five of the 6 samples exceed the Evaluation Guideline (North Carolina Administrative code, Title 15A) and the General Water Quality Objective set to protect aquatic life beneficial uses and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15438

LOE ID: | 10044
Pollutant: | Chlorophyll-a
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 6
Number of Exceedances: | 5
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 5 of 6 samples exceed the criterion for Chlorophyll a.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Evaluation Guideline: | North Carolina Administrative code (NCAC), Title 15A - Environmental and Natural Resources, Subchapter 2B-Surface water and wetland standards, Rule 0211-Fresh surface water quality standards for class C waters (Class C is defined as freshwaters protected for secondary recreation, fishing, aquatic life including propagation and survival, and wildlife). Section 3(a) of Rule 0211 applies to all fresh surface waters and states that chlorophyll a is not to exceed 40 ug/L.
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected over the time period 7/28/1999-2/10/2000. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 10043
Pollutant: | Chlorophyll-a
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 6
Number of Exceedances: | 5
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 5 of 6 samples exceed the criterion for Chlorophyll a.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Evaluation Guideline: | North Carolina Administrative code (NCAC), Title 15A - Environmental and Natural Resources, Subchapter 2B-Surface water and wetland standards, Rule 0211-Fresh surface water quality standards for class C waters (Class C is defined as freshwaters protected for secondary recreation, fishing, aquatic life including propagation and survival, and wildlife). Section 3(a) of Rule 0211 applies to all fresh surface waters and states that chlorophyll a is not to exceed 40 ug/L.
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected over the time period 7/28/1999-2/10/2000. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 10362
Pollutant: | Sodium
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture | Nonpoint Source | Urban Runoff/Storm Sewers
Expected TMDL Completion Date: | 2018
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.2 of the Listing Policy. One line of evidence is available in the administrative record to assess this pollutant. Based on section 3.2 the site exceeded numeric objectives for conventional pollutants. Using the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Six of 6 samples exceeded the Agricultural Supply water quality objective and this meets or exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10362

LOE ID: | 10059
Pollutant: | Sodium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Agricultural Supply
Number of Samples: | 6
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Alisal Creek (Salinas) to determine beneficial use support and results are as follows: 6 of 6 samples exceed the criterion for Sodium.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when sodium exceeds 69 mg/L in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Alisal Creek (Salinas) was collected at 1 monitoring site [ 309UAL-Salinas Reclamation Canal at Old Stage Road ]
Temporal Representation: | Data was collected over the time period 7/28/1999-2/10/2000. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):