# Draft 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 3 - Central Coast Region

Water Body Name: | Carneros Creek (Monterey County)
Water Body ID: | CAR3060001020090115165216
Water Body Type: | River & Stream

DECISION ID | 16136
Pollutant: | Ammonia (Unionized)
Final Listing Decision: | Do Not Delist from 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for removal from the section 303(d) list under section 4.1 of the Listing Policy. Under this section a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. However, they summarize the exact same data. LOE #26650 is the LOE used to determine the listing status in 2006. However, this LOE contains an error. This LOE states that 3 of 9 samples exceed the general objective. This is incorrect - one of the counted exceedances is actually equal to (and does not exceed) the objective. Therefore LOE #26650 is replaced with the revised sample count in LOE #26659. This does not change the Decision. Two of the 9 samples exceed the General water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against removing this water segment-pollutant combination from the section 303(d) list. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Two of the 9 samples exceed the General water quality objective and this exceeds the allowable frequency calculated from the equation in Table 4.1 of the Listing Policy. 4. Pursuant to section 4.11 of the Listing Policy, no additional data and information are available indicating that standards are met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be removed from the section 303(d) list because applicable water quality standards for the pollutant are being exceeded.
SWRCB Board Decision / Staff Recommendation: | After review of the available data and information, SWRCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16136

LOE ID: | 26659
Pollutant: | Ammonia (Unionized)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 9
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 2 of 9 samples exceed the criterion for Ammonia as N, Unionized.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin General Objective, Chapter III, Section II.A.2 (General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries) states that the discharge of wastes shall not cause concentrations of unionized ammonia (NH3) to exceed 0.025 mg/l (as N) in receiving waters (page III-4) .
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road].
Temporal Representation: | Data was collected over the time period 1/23/2006-12/18/2006. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 26650
Pollutant: | Ammonia (Unionized)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 9
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Three out of 9 samples exceeded the general water quality objective (CCAMP, 2004; SWAMP, 2004).
Data Reference: | Placeholder reference 2006 303(d)
Water Quality Objective/Criterion: | The discharge of wastes shall not cause concentrations of unionized ammonia (NH3) to exceed 0.025 mg/L (as N) in receiving waters (Region 3 Basin Plan, Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a. General Objectives, page III-4)
Objective/Criterion Reference: | Placeholder reference 2006 303(d)
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from one site.
Temporal Representation: | Samples were collected from March 1999 to March 2000.
Environmental Conditions: | Water body is located in the Bolsa Nueva hydrologic unit. The site is Carneros Creek in Los Lomas at Blohm Road (306CAR).
QAPP Information: | CCAMP, SWAMP QAPP.
QAPP Information Reference(s):

DECISION ID | 16159
Pollutant: | Escherichia coli (E. Coli)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.3 of the Listing Policy. Under section 3.3 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Four of the 10 samples exceed the Evaluation Guideline (USEPA Ambient Water Quality Criteria for Bacteria, 1986) as it applies to the Water Contact Recreation beneficial use. Two of the 10 samples exceed the water quality objective for Non-Contact Recreation. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 26 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Four of the 10 samples exceed the Evaluation Guideline (USEPA Ambient Water Quality Criteria for Bacteria, 1986) as it applies to the Water Contact Recreation beneficial use. Two of the 10 samples exceed the water quality objective for Non-Contact Recreation. Neither of these exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16159

LOE ID: | 26704
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Carneros Creek to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | USEPA Ambient Water Quality Criteria for Bacteria -1986.
Objective/Criterion Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | Single sample maximum allowable density for E. coli in freshwater is 235 MPN/100mL (as stated in Table 4, page 15)
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306-CARNE-1 - Carneros Creek]
Temporal Representation: | Data was collected on a single day 5/1/2004. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 26664
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 9
Number of Exceedances: | 2
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 2 of 9 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml. E. coli is a fecal coliform.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road]
Temporal Representation: | Data was collected over the time period 1/23/2006-12/18/2006. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rot
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 26705
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Carneros Creek to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml. E. coli is a fecal coliform.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306-CARNE-1 - Carneros Creek]
Temporal Representation: | Data was collected on a single day 5/1/2004. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 26663
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 9
Number of Exceedances: | 4
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 4 of 9 samples exceed the criterion for Escherichia coli.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | USEPA Ambient Water Quality Criteria for Bacteria -1986.
Objective/Criterion Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | Single sample maximum allowable density for E. coli in freshwater is 235 MPN/100mL (as stated in Table 4, page 15)
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road]
Temporal Representation: | Data was collected over the time period 1/23/2006-12/18/2006. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rot
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 16164
Pollutant: | Nitrate
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Six lines of evidence are available in the administrative record to assess this pollutant. A total of 193 of the 3585 samples exceed the water quality objective for Municipal and Domestic Supply. In addition, none of the 9 nitrate + nitrite samples exceed the OEHHA public Health Goal in Drinking Water (December 1997) as it applies to the Municipal and Domestic Supply beneficial use. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. A total of 193 of the 3585 samples exceed the water quality objective for Municipal and Domestic Supply. In addition, none of the 9 nitrate + nitrite samples exceed the OEHHA public Health Goal in Drinking Water (December 1997) as it applies to the Municipal and Domestic Supply beneficial use. Neither of these exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16164

LOE ID: | 26701
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 3371
Number of Exceedances: | 189
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Monterey Area Research Consortium (R3_MARC) data for Carneros Creek to determine beneficial use support and results are as follows: 189 of 3371 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: Marc Los Huertos Water Quality Data, file A
| Final Data File used for assessment: Marc Los Huertos Water Quality Data, file B
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin Objective for municipal and domestic supply uses of inland surface waters (Section II.A.2) states the following: waters shall not contain concentrations of chemical constituents in excess of the limits specified in California Code of Regulations, Title 22, Article 4, Chapter 15, Section 64435, Tables 2 and 3 as listed in Table 3-2. The maximum contaminant level listed in Table 3-2 (inorganic and fluoride concentrations not to be exceeded in domestic or municipal supply) for nitrate is 10.0 mg/L (NO3 as N).
Objective/Criterion Reference: | Title 22, Division 4, Ch. 15, Article 4, Section 64431, Table 64431-A
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 9 monitoring sites [ CA-SMC - Carneros Creek at San Miguel Canyon Rd., CA-COR - Carneros Creek at Corey Rd., CA-KIR - Carneros Creek at Kirby Park, CA-BIR - Carneros Creek at Bend in road,
Temporal Representation: | Data was collected over the time period 10/4/2000-3/20/2007.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 26681
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 171
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed National Estuarine Research Reserve Monitoring Program (R3_ESNERR) data for Carneros Creek to determine beneficial use support and results are as follows: 4 of 171 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Field Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 94-04
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin Objective for municipal and domestic supply uses of inland surface waters (Section II.A.2) states the following: waters shall not contain concentrations of chemical constituents in excess of the limits specified in California Code of Regulations, Title 22, Article 4, Chapter 15, Section 64435, Tables 2 and 3 as listed in Table 3-2. The maximum contaminant level listed in Table 3-2 (inorganic and fluoride concentrations not to be exceeded in domestic or municipal supply) for nitrate is 10.0 mg/L (NO3 as N).
Objective/Criterion Reference: | Title 22, Division 4, Ch. 15, Article 4, Section 64431, Table 64431-A
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CARBLR - Carneros Creek]
Temporal Representation: | Data was collected over the time period 1/20/1990-12/4/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | QAPP was adopted for work conducted since 2005. Prior to 2005 no QAPP was in place and data entry was completed by volunteers. Multiple errors were identified in data and were flagged by RB staff (in communication with Elkhorn Slough Program staff) prior
QAPP Information Reference(s):
LOE ID: | 26658
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 21
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 0 of 21 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin Objective for municipal and domestic supply uses of inland surface waters (Section II.A.2) states the following: waters shall not contain concentrations of chemical constituents in excess of the limits specified in California Code of Regulations, Title 22, Article 4, Chapter 15, Section 64435, Tables 2 and 3 as listed in Table 3-2. The maximum contaminant level listed in Table 3-2 (inorganic and fluoride concentrations not to be exceeded in domestic or municipal supply) for nitrate is 10.0 mg/L (NO3 as N).
Objective/Criterion Reference: | Title 22, Division 4, Ch. 15, Article 4, Section 64431, Table 64431-A
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road]
Temporal Representation: | Data was collected over the time period 3/29/1999-12/18/2006. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rot
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 26689
Pollutant: | Nitrate/Nitrite (Nitrite + Nitrate as N)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 9
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed National Estuarine Research Reserve Monitoring Program (R3_ESNERR) data for Carneros Creek to determine beneficial use support and results are as follows: 0 of 9 samples exceed the criterion for Nitrate/Nitrite
Data Reference: | Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Field Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 94-04
Water Quality Objective/Criterion: | OEHHA public Health Goals for Nitrate and Nitrogen in Drinking Water (December 1997). Page 6.
Objective/Criterion Reference: | Public health goals for nitrate and nitrite in drinking water
Evaluation Guideline: | OEHHA Public Health Goal states that sum of the concentration of nitrate + nitrite shall not exceed 10 mg/L (NO3+NO2 expressed as N).
Guideline Reference: | Public health goals for nitrate and nitrite in drinking water
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CARBLR - Carneros Creek]
Temporal Representation: | Data was collected over the time period 1/10/2006-12/4/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | QAPP was adopted for work conducted since 2005. Prior to 2005 no QAPP was in place and data entry was completed by volunteers. Multiple errors were identified in data and were flagged by RB staff (in communication with Elkhorn Slough Program staff) prior
QAPP Information Reference(s):
LOE ID: | 26702
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Carneros Creek to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin Objective for municipal and domestic supply uses of inland surface waters (Section II.A.2) states the following: waters shall not contain concentrations of chemical constituents in excess of the limits specified in California Code of Regulations, Title 22, Article 4, Chapter 15, Section 64435, Tables 2 and 3 as listed in Table 3-2. The maximum contaminant level listed in Table 3-2 (inorganic and fluoride concentrations not to be exceeded in domestic or municipal supply) for nitrate is 10.0 mg/L (NO3 as N).
Objective/Criterion Reference: | Title 22, Division 4, Ch. 15, Article 4, Section 64431, Table 64431-A
| Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306-CARNE-1 - Carneros Creek]
Temporal Representation: | Data was collected on a single day 5/1/2004. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 26654
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 21
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 0 of 21 samples exceed the criterion for Nitrate as N.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain concentrations of chemical constituents in amounts which adversely affect the agricultural beneficial use. Interpretation of adverse effect shall be as derived from the University of California Agricultural Extension Service guidelines provided in Table 3-3 (Central Coast Waterboard Basin Plan, Chapter III, Section II.A.2 Objectives for all Inland and Surface Waters, Enclosed Bays and Estuaries). In Table 3-3 of the Basin Plan (page III-8), water quality guidelines state that severe problems may occur when nitrate exceeds 30 mg/L NO3 as N in irrigation supply water.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road].
Temporal Representation: | Data was collected over the time period 3/29/1999-12/18/2006. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 16156
Pollutant: | Nitrogen, ammonia (Total Ammonia)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Three lines of evidence are available in the administrative record to assess this pollutant. None of the 3538 samples exceed the water quality objective for Municipal & Domestic Supply. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of the 3538 samples exceed the water quality objective for Municipal & Domestic Supply and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16156

LOE ID: | 26680
Pollutant: | Ammonia as Nitrogen
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 165
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed National Estuarine Research Reserve Monitoring Program (R3_ESNERR) data for Carneros Creek to determine beneficial use support and results are as follows: 0 of 165 samples exceed the criterion for Ammonia As N,
Data Reference: | Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Field Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 94-04
Water Quality Objective/Criterion: | USEPA Health Advisory 2006 Edition of the Drinking Water Standards and Health Advisories (EPA 822-R-06-013, 2006).
Objective/Criterion Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Evaluation Guideline: | EPA's Lifetime Health advisory level for total ammonia is 30.0 mg/L as stated on page 8 of the 2006 edition of the drinking water standards and health advisories. This Advisory Level is defined as "the concentration of a chemical in drinking water that is not expected to cause any adverse noncarcinogenic effects for up to ten days of exposure."
Guideline Reference: | Quality Criteria for Water 1986. United States Environmental Protection Agency. Office of Water. Regulations and Standards. Washington D.C. EPA 440/5-86-001.
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CARBLR - Carneros Creek]
Temporal Representation: | Data was collected over the time period 1/20/1990-12/4/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | QAPP was adopted for work conducted since 2005. Prior to 2005 no QAPP was in place and data entry was completed by volunteers. Multiple errors were identified in data and were flagged by RB staff (in communication with Elkhorn Slough Program staff) prior
QAPP Information Reference(s):
LOE ID: | 26660
Pollutant: | Ammonia as Nitrogen
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 21
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 0 of 21 samples exceed the criterion for Ammonia as N, Total.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | USEPA Health Advisory 2006 Edition of the Drinking Water Standards and Health Advisories (EPA 822-R-06-013, 2006).
Objective/Criterion Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Evaluation Guideline: | EPA's Lifetime Health advisory level for total ammonia is 30.0 mg/L as stated on page 8 of the 2006 edition of the drinking water standards and health advisories. This Advisory Level is defined as "the concentration of a chemical in drinking water that is not expected to cause any adverse noncarcinogenic effects for up to ten days of exposure."
Guideline Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road].
Temporal Representation: | Data was collected over the time period 3/29/1999-12/18/2006. Salinas watershed area is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 26698
Pollutant: | Ammonia as Nitrogen
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 3352
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Monterey Area Research Consortium (R3_MARC) data for Carneros Creek to determine beneficial use support and results are as follows: 0 of 3352 samples exceed the criterion for Ammonia As N, Total.
Data Reference: | Final Data File used for assessment: Marc Los Huertos Water Quality Data, file A
| Final Data File used for assessment: Marc Los Huertos Water Quality Data, file B
Water Quality Objective/Criterion: | USEPA Health Advisory 2006 Edition of the Drinking Water Standards and Health Advisories (EPA 822-R-06-013, 2006).
Objective/Criterion Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Evaluation Guideline: | EPA's Lifetime Health advisory level for total ammonia is 30.0 mg/L as stated on page 8 of the 2006 edition of the drinking water standards and health advisories. This Advisory Level is defined as "the concentration of a chemical in drinking water that is not expected to cause any adverse noncarcinogenic effects for up to ten days of exposure."
Guideline Reference: | 2006 edition of the drinking water standards and health advisories. EPA 822-R-03-013
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 9 monitoring sites [ CA-SMC - Carneros Creek at San Miguel Canyon Rd., CA-COR - Carneros Creek at Corey Rd., CA-KIR - Carneros Creek at Kirby Park, CA-BIR - Carneros Creek at Bend in road,
Temporal Representation: | Data was collected over the time period 10/4/2000-3/20/2007.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):

DECISION ID | 16165
Pollutant: | Temperature, water
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Five lines of evidence are available in the administrative record to assess this pollutant. Sixty-six of the 816 samples exceed the Evaluation Guideline (Moyle 1976) applied to protect the Cold Freshwater Habitat beneficial use. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Sixty-six of the 816 samples exceed the Evaluation Guideline (Moyle 1976) applied to protect the Cold Freshwater Habitat beneficial use and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16165

LOE ID: | 26673
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 22
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 1 of 22 samples exceed the criterion for Water Temperature.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Board that such alteration in temperature does not adversely affect beneficial uses (General Objective in Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Inland Fishes of California (Moyle 1976) states that for rainbow trout the optimum range for growth and completion of most life stages is 13-21 degrees C (page 129).
Guideline Reference: | Inland Fishes of California
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road]
Temporal Representation: | Data was collected over the time period 3/1/1999-12/18/2006. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rota
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 26688
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 189
Number of Exceedances: | 35
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed National Estuarine Research Reserve Monitoring Program (R3_ESNERR) data for Carneros Creek to determine beneficial use support and results are as follows: 35 of 189 samples exceed the criterion for Water Tempera
Data Reference: | Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Field Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 94-04
Water Quality Objective/Criterion: | Natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Board that such alteration in temperature does not adversely affect beneficial uses (General Objective in Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Inland Fishes of California (Moyle 1976) states that for rainbow trout the optimum range for growth and completion of most life stages is 13-21 degrees C (page 129).
Guideline Reference: | Inland Fishes of California
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CARBLR - Carneros Creek]
Temporal Representation: | Data was collected over the time period 1/20/1990-10/10/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | QAPP was adopted for work conducted since 2005. Prior to 2005 no QAPP was in place and data entry was completed by volunteers. Multiple errors were identified in data and were flagged by RB staff (in communication with Elkhorn Slough Program staff) prior
QAPP Information Reference(s):
LOE ID: | 26693
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 602
Number of Exceedances: | 30
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Monterey Area Research Consortium (R3_MARC) data for Carneros Creek to determine beneficial use support and results are as follows: 30 of 602 samples exceed the criterion for Water Temperature.
Data Reference: | Final Data File used for assessment: Marc Los Huertos Water Quality Data, file A
| Final Data File used for assessment: Marc Los Huertos Water Quality Data, file B
Water Quality Objective/Criterion: | Natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Board that such alteration in temperature does not adversely affect beneficial uses (General Objective in Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Inland Fishes of California (Moyle 1976) states that for rainbow trout the optimum range for growth and completion of most life stages is 13-21 degrees C (page 129).
Guideline Reference: | Inland Fishes of California
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 9 monitoring sites [ CA-COR - Carneros Creek at Corey Rd., CA-SMC - Carneros Creek at San Miguel Canyon Rd., CA-KIR - Carneros Creek at Kirby Park, CA-BIR - Carneros Creek at Bend in road,
Temporal Representation: | Data was collected over the time period 10/4/2000-2/11/2007.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 26706
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Carneros Creek to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for Water Temperature.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | Natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Board that such alteration in temperature does not adversely affect beneficial uses (General Objective in Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Inland Fishes of California (Moyle 1976) states that for rainbow trout the optimum range for growth and completion of most life stages is 13-21 degrees C (page 129).
Guideline Reference: | Inland Fishes of California
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306-CARNE-1 - Carneros Creek]
Temporal Representation: | Data was collected on a single day 5/1/2004. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 26676
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Carneros Creek to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Water Temperature.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Board that such alteration in temperature does not adversely affect beneficial uses (General Objective in Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Inland Fishes of California (Moyle 1976) states that for rainbow trout the optimum range for growth and completion of most life stages is 13-21 degrees C (page 129).
Guideline Reference: | Inland Fishes of California
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road]
Temporal Representation: | Data was collected over the time period 7/6/1999-7/27/1999. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 16162
Pollutant: | Unknown Toxicity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 and section 3.6 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Three lines of evidence are available in the administrative record to assess this pollutant in water samples. None of the samples were toxic to test organisms (exhibited a significant increase in mortality or decrease in cell density compared to the laboratory control) and therefore do not exceed the narrative General Objective for toxicity, set to protect for aquatic life beneficial uses. The following is a summary of the results from individual toxicity tests. None of the 3 samples (tested for toxicity to plants) exhibited significant reduction in cell density relative to the control. In addition, none of the 2 samples (tested for toxicity to vertebrate test organisms) exhibited a significant increase in mortality compared to the laboratory control. Lastly, none of the 2 samples, tested for toxicity to invertebrate test organisms exhibited a significant increase in mortality compared to the laboratory control. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. However, there are an insufficient number of samples to make a "use rating" decision. Central Coast Water Board staff require a minimum of 16 samples to make a "use rating" decision of Fully Supporting. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of the samples were toxic to test organisms. Therefore, this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16162

LOE ID: | 26712
Pollutant: | Vertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Toxicity, Pimephales promelas Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road]
Temporal Representation: | Data was collected over the time period 6/15/2006-2/14/2007. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 26711
Pollutant: | Invertebrate Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 0 of 2 samples exceed the criterion for Toxicity, Ceriodaphnia dubia Survival (%) 7 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction of survival of test organism relative to the control (alpha < 0.05) and test organism survival is 20% less than the control survival.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road]
Temporal Representation: | Data was collected over the time period 6/15/2006-2/14/2007. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 26714
Pollutant: | Plant Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 3
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 0 of 3 samples exceed the criterion for Toxicity, Selenastrum capricornutum Growth (Cell Density) 4 days. Toxicity is defined by SWAMP (2004) as follows: Significant toxicity in the survival endpoint when compared to the negative control based on a statistical test with alpha of less than 5%, and less than the evaluation threshold (both criteria are met).
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations which are toxic to, or which produce detrimental physiological responses in, human, plant, animal, or aquatic life. Compliance with this objective will be determined by use of indicator organisms, analyses of species diversity, population density, growth anomalies, toxicity bioassays of appropriate duration, or other appropriate methods as specified by the Regional Board (Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Significant reduction in cell count of test organism relative to the control (alpha < 0.05) and cell count <80% of control.
Guideline Reference: | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road]
Temporal Representation: | Data was collected over the time period 6/15/2006-2/15/2007. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation year (winter and summer) at a subset of sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 16157
Pollutant: | Chlorophyll-a
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.2 of the Listing Policy. Two lines of evidence are available in the administrative record to assess this pollutant. Based on section 3.2 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Twenty-two of 44 samples exceeded the water quality objective and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16157

LOE ID: | 26651
Pollutant: | Chlorophyll-a
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 23
Number of Exceedances: | 13
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 13 of 23 samples exceed the criterion for Chlorophyll a.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Evaluation Guideline: | North Carolina Administrative code (NCAC), Title 15A - Environmental and Natural Resources, Subchapter 2B-Surface water and wetland standards, Rule 0211-Fresh surface water quality standards for class C waters (Class C is defined as freshwaters protected for secondary recreation, fishing, aquatic life including propagation and survival, and wildlife). Section 3(a) of Rule 0211 applies to all fresh surface waters and states that chlorophyll a is not to exceed 40 ug/L.
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road].
Temporal Representation: | Data was collected over the time period 3/29/1999-12/18/2006. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 26687
Pollutant: | Chlorophyll-a
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 21
Number of Exceedances: | 9
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed National Estuarine Research Reserve Monitoring Program (R3_ESNERR) data for Carneros Creek to determine beneficial use support and results are as follows: 9 of 21 samples exceed the criterion for Chlorophyll a.
Data Reference: | Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Field Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 94-04
Water Quality Objective/Criterion: | Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect beneficial uses (general objective for biostimulatory substances, Water Quality Control Plan, Central Coast Basin, Chapter III, Section II).
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| Water quality standards table
Evaluation Guideline: | North Carolina Administrative code (NCAC), Title 15A - Environmental and Natural Resources, Subchapter 2B-Surface water and wetland standards, Rule 0211-Fresh surface water quality standards for class C waters (Class C is defined as freshwaters protected for secondary recreation, fishing, aquatic life including propagation and survival, and wildlife). Section 3(a) of Rule 0211 applies to all fresh surface waters and states that chlorophyll a is not to exceed 40 ug/L.
Guideline Reference: | North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
| North Carolina standards, criteria, or toxic concentrations. Adopted per title 15A North Carolina Administrative Code subchapter 2B - Surface water and wetland standards
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CARBLR - Carneros Creek]
Temporal Representation: | Data was collected over the time period 7/31/2001-5/5/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | QAPP was adopted for work conducted since 2005. Prior to 2005 no QAPP was in place and data entry was completed by volunteers. Multiple errors were identified in data and were flagged by RB staff (in communication with Elkhorn Slough Program staff) prior
QAPP Information Reference(s):

DECISION ID | 16160
Pollutant: | Fecal Coliform
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture | Natural Sources
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.3 of the Listing Policy. Two lines of evidence are available in the administrative record to assess this pollutant. Based on section 3.3 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Fifteen of 18 samples exceeded the water quality objective for Water Contact Recreation and 5 of 18 samples exceeded the water quality objective for Non-Contact Recreation. Each of these exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16160

LOE ID: | 26662
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 18
Number of Exceedances: | 5
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 5 of 18 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 2000/100 ml, nor shall more than ten percent of samples collected during any 30-day period exceed 4000/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road].
Temporal Representation: | Data was collected over the time period 4/26/1999-12/18/2006. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 26661
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 18
Number of Exceedances: | 15
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 15 of 18 samples exceed the criterion for Coliform, Fecal.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: Fecal coliform concentration, based on a minimum of not less than five samples for any 30-day period, shall not exceed a log mean of 200 MPN/100 ml, nor shall more than ten percent of total samples during any 30-day period exceed 400 MPN/100 ml.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road].
Temporal Representation: | Data was collected over the time period 4/26/1999-12/18/2006. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 16158
Pollutant: | Low Dissolved Oxygen
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.2 of the Listing Policy. Eight lines of evidence are available in the administrative record to assess these pollutants. Two water quality objectives are assessed: Two hundred eighty-eight of the 793 samples exceed the dissolved oxygen water quality objective for Cold Freshwater Habitat and 79 of 125 samples exceed the general water quality objective for oxygen saturation which states that the median oxygen saturation value shall not fall below 85%. In this case the median value did exceed this criterion. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Two hundred eighty-eight of the 793 samples exceed the dissolved oxygen water quality objective for Cold Freshwater Habitat and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. In addition, 79 of 125 samples exceed the general water quality objective for oxygen saturation which states that the median oxygen saturation value shall not fall below 85%. In this case the median value did exceed this criterion. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16158

LOE ID: | 26671
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 22
Number of Exceedances: | 13
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 13 of 22 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road]
Temporal Representation: | Data was collected over the time period 3/1/1999-12/18/2006. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rota
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 26690
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 170
Number of Exceedances: | 78
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed National Estuarine Research Reserve Monitoring Program (R3_ESNERR) data for Carneros Creek to determine beneficial use support and results are as follows: 78 of 170 samples exceed the criterion for Oxygen, Disso
Data Reference: | Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Field Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 94-04
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CARBLR - Carneros Creek]
Temporal Representation: | Data was collected over the time period 1/20/1990-10/10/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | QAPP was adopted for work conducted since 2005. Prior to 2005 no QAPP was in place and data entry was completed by volunteers. Multiple errors were identified in data and were flagged by RB staff (in communication with Elkhorn Slough Program staff) prior
QAPP Information Reference(s):
LOE ID: | 26674
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Carneros Creek to determine beneficial use support and results are as follows: 1 of 2 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road]
Temporal Representation: | Data was collected over the time period 7/6/1999-7/27/1999. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 26672
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 22
Number of Exceedances: | 15
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 15 of 22 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road]
Temporal Representation: | Data was collected over the time period 3/1/1999-12/18/2006. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rota
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 26703
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Carneros Creek to determine beneficial use support and results are as follows: 1 of 1 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306-CARNE-1 - Carneros Creek]
Temporal Representation: | Data was collected on a single day 5/1/2004. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 26699
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 598
Number of Exceedances: | 195
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Monterey Area Research Consortium (R3_MARC) data for Carneros Creek to determine beneficial use support and results are as follows: 195 of 598 samples exceed the criterion for Oxygen, Dissolved.
Data Reference: | Final Data File used for assessment: Marc Los Huertos Water Quality Data, file A
| Final Data File used for assessment: Marc Los Huertos Water Quality Data, file B
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, Cold Water Habitat Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: The dissolved oxygen concentration shall not be reduced below 7.0 mg/l at any time.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 9 monitoring sites [ CA-COR - Carneros Creek at Corey Rd., CA-SMC - Carneros Creek at San Miguel Canyon Rd., CA-KIR - Carneros Creek at Kirby Park, CA-BIR - Carneros Creek at Bend in road,
Temporal Representation: | Data was collected over the time period 10/4/2000-2/11/2007.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 26679
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 101
Number of Exceedances: | 63
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed National Estuarine Research Reserve Monitoring Program (R3_ESNERR) data for Carneros Creek to determine beneficial use support and results are as follows: 63 of 101 samples exceed the criterion for Oxygen, Satur
Data Reference: | Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Field Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 94-04
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CARBLR - Carneros Creek]
Temporal Representation: | Data was collected over the time period 11/18/1996-10/10/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | QAPP was adopted for work conducted since 2005. Prior to 2005 no QAPP was in place and data entry was completed by volunteers. Multiple errors were identified in data and were flagged by RB staff (in communication with Elkhorn Slough Program staff) prior
QAPP Information Reference(s):
LOE ID: | 26675
Pollutant: | Dissolved oxygen saturation
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Diurnal Dissolved Oxygen Sampling (DO) data for Carneros Creek to determine beneficial use support and results are as follows: 1 of 2 samples exceed the criterion for Oxygen, Saturation.
Data Reference: | Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: Median values should not fall below 85% saturation as a result of controllable water quality conditions.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road]
Temporal Representation: | Data was collected over the time period 7/6/1999-7/27/1999. Diurnal monitoring conducted in summer months at all CCAMP monitoring sites.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 16166
Pollutant: | Turbidity
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.2 of the Listing Policy. Three lines of evidence are available in the administrative record to assess this pollutant. Based on section 3.2 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. A total of 172 out of 332 samples exceeded the Evaluation Guideline (Sigler et al., 1984) applied to protect for aquatic life beneficial uses and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16166

LOE ID: | 26692
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 137
Number of Exceedances: | 71
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Monterey Area Research Consortium (R3_MARC) data for Carneros Creek to determine beneficial use support and results are as follows: 71 of 137 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: Marc Los Huertos Water Quality Data, file A
| Final Data File used for assessment: Marc Los Huertos Water Quality Data, file B
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 8 monitoring sites [ CA-SMC - Carneros Creek at San Miguel Canyon Rd., CA-KIR - Carneros Creek at Kirby Park, CA-COR - Carneros Creek at Corey Rd., CA-BIR - Carneros Creek at Bend in road,
Temporal Representation: | Data was collected over the time period 9/21/2005-2/11/2007.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 26691
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 186
Number of Exceedances: | 95
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed National Estuarine Research Reserve Monitoring Program (R3_ESNERR) data for Carneros Creek to determine beneficial use support and results are as follows: 95 of 186 samples exceed the criterion for Turbidity(NTU
Data Reference: | Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Field Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 94-04
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CARBLR - Carneros Creek]
Temporal Representation: | Data was collected over the time period 1/20/1990-10/10/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | QAPP was adopted for work conducted since 2005. Prior to 2005 no QAPP was in place and data entry was completed by volunteers. Multiple errors were identified in data and were flagged by RB staff (in communication with Elkhorn Slough Program staff) prior
QAPP Information Reference(s):
LOE ID: | 26678
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 9
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 6 of 9 samples exceed the criterion for Turbidity(NTU).
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Waters shall be free of changes in turbidity that cause nuisance or adversely affect beneficial uses. Water Quality Control Plan, Central Coast Basin, Chapter III, Section II.A.2 Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: | Sigler et al. (1984) states that turbidities of 25 NTU's or greater caused reduction in juvenile salmonid growth due to interference with their ability to find food.
Guideline Reference: | Effects of chronic turbidity on density and growth of steelheads and coho salmon. Transactions of the American Fisheries Society 113:142-150
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road]
Temporal Representation: | Data was collected over the time period 1/23/2006-12/18/2006. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rot
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):

DECISION ID | 16167
Pollutant: | pH
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under sections 2.1 and 3.2 of the Listing Policy. Sixteen lines of evidence are available in the administrative record to assess this pollutant. Based on section 3.2 the site exceeded numeric objectives for conventional pollutants. According to the binomial distribution, waters shall be placed on the section 303(d) list if the number of measured exceedances supports rejection of the null hypothesis as presented in Table 3.2. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. A total of 145 out of 832 samples exceed the Cold Freshwater Habitat water quality objective and 172 out of 832 samples exceed the numeric objectives for Municipal & Domestic Supply, Non-Contact Recreation and Water Contact Recreation. Each of these exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 16167

LOE ID: | 26695
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 642
Number of Exceedances: | 109
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Monterey Area Research Consortium (R3_MARC) data for Carneros Creek to determine beneficial use support and results are as follows: 109 of 642 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Marc Los Huertos Water Quality Data, file A
| Final Data File used for assessment: Marc Los Huertos Water Quality Data, file B
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin, Section II.A.2. Municipal and Domestic Supply Objectives, Section II.A.2.a states the following: The pH value shall neither be depressed below 6.5 or raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 9 monitoring sites [ CA-COR - Carneros Creek at Corey Rd., CA-SMC - Carneros Creek at San Miguel Canyon Rd., CA-KIR - Carneros Creek at Kirby Park, CA-BIR - Carneros Creek at Bend in road,
Temporal Representation: | Data was collected over the time period 10/4/2000-2/11/2007.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 26694
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 642
Number of Exceedances: | 71
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Monterey Area Research Consortium (R3_MARC) data for Carneros Creek to determine beneficial use support and results are as follows: 71 of 642 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Marc Los Huertos Water Quality Data, file A
| Final Data File used for assessment: Marc Los Huertos Water Quality Data, file B
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 9 monitoring sites [ CA-COR - Carneros Creek at Corey Rd., CA-SMC - Carneros Creek at San Miguel Canyon Rd., CA-KIR - Carneros Creek at Kirby Park, CA-BIR - Carneros Creek at Bend in road,
Temporal Representation: | Data was collected over the time period 10/4/2000-2/11/2007.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 26697
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 642
Number of Exceedances: | 109
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Monterey Area Research Consortium (R3_MARC) data for Carneros Creek to determine beneficial use support and results are as follows: 109 of 642 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Marc Los Huertos Water Quality Data, file A
| Final Data File used for assessment: Marc Los Huertos Water Quality Data, file B
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 9 monitoring sites [ CA-COR - Carneros Creek at Corey Rd., CA-SMC - Carneros Creek at San Miguel Canyon Rd., CA-KIR - Carneros Creek at Kirby Park, CA-BIR - Carneros Creek at Bend in road,
Temporal Representation: | Data was collected over the time period 10/4/2000-2/11/2007.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 26709
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Carneros Creek to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306-CARNE-1 - Carneros Creek]
Temporal Representation: | Data was collected on a single day 5/1/2004. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 26710
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Carneros Creek to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306-CARNE-1 - Carneros Creek]
Temporal Representation: | Data was collected on a single day 5/1/2004. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 26686
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 180
Number of Exceedances: | 59
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed National Estuarine Research Reserve Monitoring Program (R3_ESNERR) data for Carneros Creek to determine beneficial use support and results are as follows: 59 of 180 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Field Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 94-04
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CARBLR - Carneros Creek]
Temporal Representation: | Data was collected over the time period 1/20/1990-10/10/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | QAPP was adopted for work conducted since 2005. Prior to 2005 no QAPP was in place and data entry was completed by volunteers. Multiple errors were identified in data and were flagged by RB staff (in communication with Elkhorn Slough Program staff) prior
QAPP Information Reference(s):
LOE ID: | 26685
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 180
Number of Exceedances: | 59
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed National Estuarine Research Reserve Monitoring Program (R3_ESNERR) data for Carneros Creek to determine beneficial use support and results are as follows: 59 of 180 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Field Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 94-04
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CARBLR - Carneros Creek]
Temporal Representation: | Data was collected over the time period 1/20/1990-10/10/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | QAPP was adopted for work conducted since 2005. Prior to 2005 no QAPP was in place and data entry was completed by volunteers. Multiple errors were identified in data and were flagged by RB staff (in communication with Elkhorn Slough Program staff) prior
QAPP Information Reference(s):
LOE ID: | 26707
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Carneros Creek to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306-CARNE-1 - Carneros Creek]
Temporal Representation: | Data was collected on a single day 5/1/2004. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 26708
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Coastal Watershed Council (Snapshot day monitoring) (R3_Snap) data for Carneros Creek to determine beneficial use support and results are as follows: 0 of 1 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Monterey Bay National Marine Sanctuary Volunteer Monitoring Network Data. 2003-2006
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin, Section II.A.2. Municipal and Domestic Supply Objectives, Section II.A.2.a states the following: The pH value shall neither be depressed below 6.5 or raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306-CARNE-1 - Carneros Creek]
Temporal Representation: | Data was collected on a single day 5/1/2004. Coastal Watershed Council Snapshot Day Monitoring is conducted annually.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | State Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 26684
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 180
Number of Exceedances: | 59
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed National Estuarine Research Reserve Monitoring Program (R3_ESNERR) data for Carneros Creek to determine beneficial use support and results are as follows: 59 of 180 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Field Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 94-04
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin, Section II.A.2. Municipal and Domestic Supply Objectives, Section II.A.2.a states the following: The pH value shall neither be depressed below 6.5 or raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CARBLR - Carneros Creek]
Temporal Representation: | Data was collected over the time period 1/20/1990-10/10/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | QAPP was adopted for work conducted since 2005. Prior to 2005 no QAPP was in place and data entry was completed by volunteers. Multiple errors were identified in data and were flagged by RB staff (in communication with Elkhorn Slough Program staff) prior
QAPP Information Reference(s):
LOE ID: | 26665
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 9
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 4 of 9 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road].
Temporal Representation: | Data was collected over the time period 1/23/2006-12/18/2006. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 26666
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 9
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 4 of 9 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin, Section II.A.2. Municipal and Domestic Supply Objectives, Section II.A.2.a states the following: The pH value shall neither be depressed below 6.5 or raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road].
Temporal Representation: | Data was collected over the time period 1/23/2006-12/18/2006. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 26667
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 9
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 4 of 9 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road].
Temporal Representation: | Data was collected over the time period 1/23/2006-12/18/2006. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rotation.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 26696
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 642
Number of Exceedances: | 109
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed Monterey Area Research Consortium (R3_MARC) data for Carneros Creek to determine beneficial use support and results are as follows: 109 of 642 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: Marc Los Huertos Water Quality Data, file A
| Final Data File used for assessment: Marc Los Huertos Water Quality Data, file B
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for water contact recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 9 monitoring sites [ CA-COR - Carneros Creek at Corey Rd., CA-SMC - Carneros Creek at San Miguel Canyon Rd., CA-KIR - Carneros Creek at Kirby Park, CA-BIR - Carneros Creek at Bend in road,
Temporal Representation: | Data was collected over the time period 10/4/2000-2/11/2007.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | Regional Board approved QAPP. Multiple errors were identified in data and were flagged or fixed by RB staff (in communication with Project staff) prior to assessment of data.
QAPP Information Reference(s):
LOE ID: | 26668
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 9
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed CCAMP Salinas (Salinas) data for Carneros Creek to determine beneficial use support and results are as follows: 4 of 9 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: CCAMP Salinas Toxicity data
| Final Data File used for assessment: CCAMP Water Quality Data_file1
| Final Data File used for assessment: CCAMP Water Quality Data_file2
| Final Data File used for assessment: CCAMP Water Quality Data_file3
Water Quality Objective/Criterion: | The Water Quality Control Plan, Central Coast Basin objective for non-contact water recreation uses (Section II.A.2. Objectives for All Inland Surface Waters, Enclosed Bays, and Estuaries, II.A.2.a) states the following: pH value shall neither be depressed below 6.5 nor raised above 8.3.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CAR-Carneros Creek in Los Lomas at Blohm Road]
Temporal Representation: | Data was collected over the time period 1/23/2006-12/18/2006. Salinas watershed is one of five annual rotation areas that are monitored for conventional pollutants by CCAMP staff monthly for one year. Toxicity monitoring is conducted twice during the rot
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | All data was collected following the Standard Operating Procedures and Data Quality Objectives outlined in the SWAMP QAMP, (Puckett, 2002). QA data are included in submission. All data are flagged as appropriate.
QAPP Information Reference(s):
LOE ID: | 26682
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 180
Number of Exceedances: | 70
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Central Coast Regional Board Staff assessed National Estuarine Research Reserve Monitoring Program (R3_ESNERR) data for Carneros Creek to determine beneficial use support and results are as follows: 70 of 180 samples exceed the criterion for pH.
Data Reference: | Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Field Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 2006
| Final Data File used for assessment: ESNERR (Elkhorn Slough National Reserve) Water Quality Data from 94-04
Water Quality Objective/Criterion: | Water Quality Control Plan, Central Coast Basin, General Objective, Chapter III, Section II.A.2 General Objectives for all Inland Surface Waters, Enclosed Bays and Estuaries states the following: For waters not mentioned by a specific beneficial use, the pH value shall not be depressed below 7.0 or raised above 8.5.
Objective/Criterion Reference: | Water Quality Control Plan Central Coast Region (R3) Basin Plan
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Data for this line of evidence for Carneros Creek was collected at 1 monitoring site [ 306CARBLR - Carneros Creek]
Temporal Representation: | Data was collected over the time period 1/20/1990-10/10/2006.
Environmental Conditions: | Staff is not aware of any special conditions that might effect interpretation of the data.
QAPP Information: | QAPP was adopted for work conducted since 2005. Prior to 2005 no QAPP was in place and data entry was completed by volunteers. Multiple errors were identified in data and were flagged by RB staff (in communication with Elkhorn Slough Program staff) prior
QAPP Information Reference(s):