# Draft 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 5 - Central Valley Region

Water Body Name: | Hospital Creek (San Joaquin and Stanislaus Counties)
Water Body ID: | CAR5411000020070511113812
Water Body Type: | River & Stream

DECISION ID | 9119
Pollutant: | Arsenic
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. One of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. One of 15 samples exceeded the USEPA Primary MCL for Arsenic and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9119

LOE ID: | 8447
Pollutant: | Arsenic
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 11
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | None of the 11 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Arsenic.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Westside Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Arsenic levels should not exceed 10 ug/L (USEPA Primary MCL).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals - 2007 for toxicity data
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Hospital Creek at River Road.
Temporal Representation: | The samples were collected from Aug 29 2001 to Jun 24 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 26572
Pollutant: | Arsenic
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 4
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | One of 4 samples collected by the Westside San Joaquin River Water Quality Coalition exceed the criteria.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Arsenic levels should not exceed 10 ug/L (USEPA Primary MCL).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals - 2007 for toxicity data
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Hospital Creek at River Road.
Temporal Representation: | Samples were collected monthly from July 2006 - October 2006.
Environmental Conditions: |
QAPP Information: | Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region.
QAPP Information Reference(s):

DECISION ID | 9120
Pollutant: | Cadmium
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 6 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9120

LOE ID: | 8450
Pollutant: | Cadmium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 6
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Asses Water Quality: | Zero of the 6 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Cadmium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Westside Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Cadmium levels should not exceed the calculated limit based on the formula: Criteria Maximum Concentration (1-hour Average dissolved)=(EXP(1.128*LN(hardness)-3.6867))*(1.136672-(LN(hardness)*0.041838)) (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals - 2007 for toxicity data
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Hospital Creek at River Road.
Temporal Representation: | The samples were collected from Sep 26 2001 to Sep 25 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 12889
Pollutant: | Chlorpyrifos
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 14 available 4-day average concentrations exceeded the 4-day average maximum concentration criterion and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12889

LOE ID: | 22282
Pollutant: | Chlorpyrifos
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 14 water samples were collected from Hospital Creek from July 2004 through August 2006, representing 14 4-day average concentrations and 14 1-hour average concentrations.0 of 14 4-day average concentrations exceeded the 4-day maximum concentration guideline of 0.015 µg/L.0 of 14 1-hour average concentrations exceeded the maximum 1-hour concentration of 0.025 µg/L.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Department of Fish and Game Hazard Assessment Criteria - 0.015 µg/L 4-day average and 0.025 µg/L 1-hour average (Siepmann and Finlayson, 2000, with minor corrections to significant figures as described in Beaulaurier et al., 2005).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Samples were collected from Hospital Creek at River Road
Temporal Representation: | Samples were collected monthly from July 2004 through August 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):

DECISION ID | 14498
Pollutant: | Methyl Parathion
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 10 samples exceeded the interim water quality criterion and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. In addition, 6 samples had concentrations less than quantitation limits (0.1 µg/L) and quantitation limits greater than the water quality criteria concentrations. Therefore the results for these samples were not used in this analysis in accordance with section 6.1.5.5 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 14498

LOE ID: | 22339
Pollutant: | Methyl Parathion
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 2 Water sample was collected from Hospital Creek in June and August 2001, representing 2 concentrations.0 of 2 available concentrations exceeded the interim water quality criterion 0.08 µg/L.
Data Reference: | Surface Water database (SWDB) for Central Valley waterbodies, 2000-2005
| Correspondence between the Department of Pesticide Regulation and Central Valley Regional Water Quality Control Board regarding water quality data for waterbodies in the Central Valley
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Department of Fish and Game Hazard Assessment Criteria - Interim water quality criterion is 0.08 µg/L (Menconi and Harrington, 1992).
Guideline Reference: | Hazard Assessment of the Insecticide Methyl Parathion to Aquatic Organisms in the Sacramento River System. California Department of Fish and Game. Environmental Services Division. Administrative Report 92-1
Spatial Representation: | Samples were collected from Hospital at River Road near Patterson California_USGS NAWQA site.
Temporal Representation: | Samples were collected on July 21 and August 2, 2001.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Minimum requirements for the CDPR Surface Water Database are: Name of the sampling agency or organization, Date that each sample was collected, Date of each sample analysis, County where samples were taken, Detailed sampling location information (including latitude and longitude or township/range/section if available), detailed map or description of each sampling site (i.e., address, cross roads, etc.), Name or description of water body sampled, Name of the active ingredient analyzed for; concentration detected (with unit of measurement), and limit of quantitation, Description of analytical QA/QC plan, or statement that no formal plan exists. Additional optional requirements are included on DPR's webpage at http://www.cdpr.ca.gov/docs/emon/surfwtr/caps/req.htm
QAPP Information Reference(s): | Standard Operating Procedure for Conducting Surface Water Monitoring for Pesticides
LOE ID: | 22340
Pollutant: | Methyl Parathion
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 8
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 14 water samples were collected from Hospital Creek from July 2004 through August 2006, representing 8 concentrations.0 of 8 available concentrations exceeded the interim water quality criterion 0.08 µg/L. 6 water samples had method detection limits (0.1 µg/L) higher than the Criterion (0.08 µg/L). So the 6 samples were not included in this analysis.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Department of Fish and Game Hazard Assessment Criteria - Interim water quality criterion is 0.08 µg/L (Menconi and Harrington, 1992).
Guideline Reference: | Hazard Assessment of the Insecticide Methyl Parathion to Aquatic Organisms in the Sacramento River System. California Department of Fish and Game. Environmental Services Division. Administrative Report 92-1
Spatial Representation: | Samples were collected from Hospital Creek at River Road.
Temporal Representation: | Samples were collected from July 2004 through August 2006 at variable intervals (e.g. monthly, bi-monthly)
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):

DECISION ID | 9122
Pollutant: | Nickel
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 10 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9122

LOE ID: | 8455
Pollutant: | Nickel
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 10
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Asses Water Quality: | Zero of the 10 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Nickel.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Westside Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Nickel levels should not exceed the calculated limit based on the formula: Criteria Maximum Concentration (1-hour Average, dissolved)=(EXP(0.846*LN(hardness)+2.255))*(0.998)(CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals - 2007 for toxicity data
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Hospital Creek at River Road.
Temporal Representation: | The samples were collected from Jan 24 2001 to Sep 25 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 9123
Pollutant: | Nitrate as Nitrate (NO3)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 8 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. Table 3.1 of the listing policy recommends listing if a sample size of 8 has 2 or more samples that exceed the evaluation criteria.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9123

LOE ID: | 8456
Pollutant: | Nitrate as Nitrate (NO3)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 8
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Asses Water Quality: | Zero of the 8 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation guideline for Nitrate-N.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Westside Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Nitrate-N levels should not to exceed 100 mg/L (USEPA National Ambient Water Quality Objective)
Guideline Reference: | National Recommended Water Quality Criteria. United States Environmental Protection Agency. Office of Water. Office of Science and Technology. 4304T
Spatial Representation: | Samples were collected at Hospital Creek at River Road.
Temporal Representation: | The samples were collected from Jan 24 2001 to Sep 25 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 14500
Pollutant: | Oxygen, Dissolved
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Three lines of evidence are available in the administrative record to assess this pollutant. One of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. One of 82 samples fell below the minimum criterion water quality objective listed in the Sacramento/San Joaquin River Basin Plan and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 14500

LOE ID: | 22357
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 25
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Twenty-five samples were taken from Hospital Creek between 2004 and 2006. None of the twenty-five samples fell below the Water Quality Objective for minimum dissolved oxygen content in surface water.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | From the Sacramento/San Joaquin River Basin Plan the (WARM) Warm Freshwater Habitat criterion is a Minimum Dissolved Oxygen content of 5mg/L.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road in San Joaquin County.
Temporal Representation: | Samples were collected between July 2004 and October 2006. Samples were collected at monthly intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 22359
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 6
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Six samples were taken from Hospital Creek between 1993 and 2001. None of the six samples fell below the Water Quality Objective for minimum dissolved oxygen content in surface water.
Data Reference: | National Water Quality Assessment database, San Joaquin and Tulare Basins data
Water Quality Objective/Criterion: | From the Sacramento/San Joaquin River Basin Plan the (WARM) Warm Freshwater Habitat criterion is a Minimum Dissolved Oxygen content of 5mg/L.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek below the confluence of Ingram Creek near Gray, CA in San Joaquin County.
Temporal Representation: | Samples were collected between March 1993 and September 2001. Samples were collected at monthly intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Good. In accordance with section 6.1.4 of the Listing Policy, data from major monitoring programs in California and Published USGS reports are considered of adequate quality.
QAPP Information Reference(s): | National Field Manual for the Collection of Water-Quality Data, Techniques of Water-Resources Investigations, Book 9, Handbooks for Water-Resources Investigations
LOE ID: | 22358
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 51
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Fifty-one samples were taken from Hospital Creek between 2001 and 2005. One of the fifty-one samples fell below the Water Quality Objective for minimum dissolved oxygen content in surface water.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | From the Sacramento/San Joaquin River Basin Plan the (WARM) Warm Freshwater Habitat criterion is a Minimum Dissolved Oxygen content of 5mg/L.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road in San Joaquin County.
Temporal Representation: | Samples were collected between June 2001 and November 2005. Samples were collected at monthly intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)

DECISION ID | 14499
Pollutant: | Zinc
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 4 samples exceeded the 4-day maximum criterion for total zinc and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 14499

LOE ID: | 22355
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 4
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Four samples were taken from Hospital Creek in 2006. None of the four samples exceeds guidelines for total zinc. No samples exceed the 4-day average concentration levels.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | California Toxics Rule Criteria (USEPA) - Freshwater Aquatic Life ProtectionContinuous Concentration (4-day Average) calculated based on the following formula (e{.8473xLN[hardness]}+.884) U.S. Environmental Protection Agency, Federal Register, Volume 65, No. 97 (Thursday, 18 May 2000), pp. 31682-31719 [California Toxics Rule]; and Federal Register, Volume 66, No. 30 (Tuesday, 13 February 2001), pp. 9960-9962 [California Toxics Rule Correction] http://www.gpoaccess.gov/fr/browse.html.
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
| Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road in San Joaquin County.
Temporal Representation: | Samples were collected between July and October 2006. Samples were collected at monthly intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):

DECISION ID | 14501
Pollutant: | pH (high)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. Two of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Two of 48 samples had pH values higher than the pH objective and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 14501

LOE ID: | 22360
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 32
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | The Westside San Joaquin River Water Quality Coalition collected 32 samples from August 2004 to October 2006. One sample had a pH higher than 8.5 and did not meet the evaluation objective.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | The pH of water shall not be depressed below 6.5,raised above 8.5, or changed at any time more than 0.5 units from normal ambient pH.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Measurement of pH within the range of 6.5 and 8.5. A high pH value is greater than 8.5
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at Road 33 and River Road.
Temporal Representation: | Sampling occurred from August 2004 to October 2006
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 22361
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 16
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | The Central Valley Regional Water Quality Control Board Surface Water Ambient Monitoring Program collected 16 samples from November 2004 to November 2005. One of the 16 samples had a pH value over 8.5 and did not meet the evaluation objective.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | The pH of water shall not be depressed below 6.5,raised above 8.5, or changed at any time more than 0.5 units from normal ambient pH.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Measurement of pH within the range of 6.5 and 8.5. A high pH value is greater than 8.5
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at Highway 33.
Temporal Representation: | Sampling occurred from November 2004 to November 2005
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)

DECISION ID | 14502
Pollutant: | pH (low)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. Four of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Four of 48 samples had pH values lower than the pH objective and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 14502

LOE ID: | 22374
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 16
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | The Central Valley Regional Water Quality Control Board Surface Water Ambient Monitoring Program collected 16 samples from November 2004 to November 2005. Three of the 16 samples had a pH value lower than 6.5 and did not meet the evaluation objective.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | The pH of water shall not be depressed below 6.5,raised above 8.5, or changed at any time more than 0.5 units from normal ambient pH.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Measurement of pH within the range of 6.5 and 8.5. A low pH value is lower than 6.5.
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at Highway 33.
Temporal Representation: | Sampling occurred from November 2004 to November 2005
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
LOE ID: | 22373
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 32
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | The Westside San Joaquin River Water Quality Coalition collected 32 samples from August 2004 to October 2006. One sample had a pH lower than 6.5 and did not meet the evaluation objective.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | The pH of water shall not be depressed below 6.5,raised above 8.5, or changed at any time more than 0.5 units from normal ambient pH.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Measurement of pH within the range of 6.5 and 8.5. A low pH value is lower than 6.5.
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at Road 33 and River Road.
Temporal Representation: | Sampling occurred from August 2004 to October 2006
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):

DECISION ID | 12887
Pollutant: | Copper
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess this pollutant. Three of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Three of 4 samples exceed the 4-day maximum criterion for total copper and this exceeds the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12887

LOE ID: | 22356
Pollutant: | Copper
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 4
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Four samples were taken from Hospital Creek in 2006. Three of the four samples exceed guidelines for total copper. Three samples exceed the 4-day average concentration levels.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | California Toxics Rule Criteria (USEPA) - Freshwater Aquatic Life ProtectionContinuous Concentration (4-day Average) calculated based on the fallowing formula (e{.8545xLN[hardness]}-1.702) which incorporates hardnessU.S. Environmental Protection Agency, Federal Register, Volume 65, No. 97 (Thursday, 18 May 2000), pp. 31682-31719 [California Toxics Rule]; and Federal Register, Volume 66, No. 30 (Tuesday, 13 February 2001), pp. 9960-9962 [California Toxics Rule Correction] http://www.gpoaccess.gov/fr/browse.html.
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
| Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road in San Joaquin County.
Temporal Representation: | Samples were collected between July and October 2006. Samples were collected at monthly intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):

DECISION ID | 12886
Pollutant: | DDE
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess this pollutant. Three of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Three of 3 samples exceed the California Toxic Rule/USEPA (CTR/USEPA) criteria limit of 0.00059 μg/L for DDE based on a human health carcinogenic risk level of 10-6 for consumption of water and aquatic organisms and this exceeds the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12886

LOE ID: | 22283
Pollutant: | DDE
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Commercial or recreational collection of fish, shellfish, or organisms
Number of Samples: | 3
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Three water samples were taken from Hospital Creek between June 1994 and August 2001. All of the three samples exceed the California Toxic Rule/USEPA (CTR/USEPA) criteria limit of 0.00059 µg/L for DDE based on a human health carcinogenic risk level of 10-6 for consumption of water and aquatic organisms.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | - Sacramento/San Joaquin River Basin Plan (CVRWQCB, 2007a).Pesticides: Total identifiable persistent chlorinated hydrocarbon pesticides shall not be present in the water column at concentrations detectable within the accuracy of analytical methods approved by the Environmental Protection Agency or the Executive Officer.- California Toxics Rule Criteria (USEPA, 2000)Inland Surface Waters based on drinking water and aquatic organism consumption. The criteria are based on human health protection for carcinogenicity at 1-in-a-million risk level (30-day average) for DDE of 0.00059 µg/L.
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
| Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road in Stanislaus County.
Temporal Representation: | Samples were collected between June 1994 and August of 2006. Samples were collected at monthly intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):

DECISION ID | 12885
Pollutant: | DDT
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess this pollutant. Four of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Four of 5 samples exceed the California Toxic Rule/USEPA (CTR/USEPA) criteria limit of 0.00059 μg/L for total DDT based on a human health carcinogenic risk level of 10-6 for consumption of water and aquatic organisms and this exceeds the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12885

LOE ID: | 22300
Pollutant: | DDT
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Commercial or recreational collection of fish, shellfish, or organisms
Number of Samples: | 5
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Five water samples were taken from Hospital Creek between June 1994 and August 2006. Four (4) of the five (5) samples exceed the California Toxic Rule/USEPA (CTR/USEPA) criteria limit of 0.00059 µg/L for total DDT based on a human health carcinogenic risk level of 10-6 for consumption of water and aquatic organisms (4,4'-DDT; DDE,p,p¿).
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | - Sacramento/San Joaquin River Basin Plan (CVRWQCB, 2007a).Pesticides: Total identifiable persistent chlorinated hydrocarbon pesticides shall not be present in the water column at concentrations detectable within the accuracy of analytical methods approved by the Environmental Protection Agency or the Executive Officer.- California Toxics Rule Criteria (USEPA, 2000)Inland Surface Waters based on drinking water and aquatic organism consumption. The criteria are based on human health protection for carcinogenicity at 1-in-a-million risk level (30-day average) with a limit of 0.00059 µg/L for DDT.
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
| Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road in Stanislaus County.
Temporal Representation: | Samples were collected between June 1994 and August of 2006. Samples were collected at monthly intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):

DECISION ID | 12891
Pollutant: | Dieldrin
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess this pollutant. Three of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Three of 4 samples exceed the California Toxic Rule/USEPA (CTR/USEPA) criteria for Dieldrin of 0.00014 μg/L based on a human health 10-6 carcinogenic risk level for water and fish consumption and this exceeds the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12891

LOE ID: | 22301
Pollutant: | Dieldrin
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Commercial or recreational collection of fish, shellfish, or organisms
Number of Samples: | 4
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Four water samples were taken from Hospital Creek between June 1994 and August 2001. All of the four samples exceeded the CTR criterion for Dieldrin of 0.00014 µg/L for water and fish consumption.
Data Reference: | Surface Water database (SWDB) for Central Valley waterbodies, 2000-2005
| Correspondence between the Department of Pesticide Regulation and Central Valley Regional Water Quality Control Board regarding water quality data for waterbodies in the Central Valley
Water Quality Objective/Criterion: | - Sacramento/San Joaquin River Basin Plan CVRWQCB. 2007Pesticides: Total identifiable persistent chlorinated hydrocarbon pesticides shall not be present in the water column at concentrations detectable within the accuracy of analytical methods approved by the Environmental Protection Agency or the Executive Officer.- California Toxics Rule Criteria (USEPA, 2000):Criteria based on Human Health Protection (30-day average) with a Dieldrin limit of less than 0.00014 µg/L for water and fish consumption.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road in Stanislaus County.
Temporal Representation: | Samples were collected between June 1994 and August 2001 at irregular intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s): | Standard Operating Procedure for Conducting Surface Water Monitoring for Pesticides

DECISION ID | 14387
Pollutant: | Dimethoate
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. Seven of the samples exceed the Evaluation Guideline and, therefore, the narrative toxicity water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Three of 14 water samples exceed the dimethoate Evaluation Guideline of 0.2 ug/L, and this exceeds the narrative toxicity object and the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 14387

LOE ID: | 26104
Pollutant: | Dimethoate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Sixteen water samples were collected from Hospital Creek, under the Irrigated Lands Regulatory Program, between July 2004 and August 2006. Two of the samples had concentrations less than the quantitation limit (2 ug/L), which is greater than the Evaluation Guideline value of 0.2 ug/L. Therefore, these 2 samples were not used in this assessment. Three of the 14 remaining water samples contained dimethoate at concentrations that exceeded the Evaluation Guideline value of 0.2 µg/L.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses. All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. Where valid testing has developed 96 hour LC50 values for aquatic organisms (the concentration that kills one half of the test organisms in 96 hours), the Board will consider one tenth of this value for the most sensitive species tested as the upper limit (daily maximum) for the protection of aquatic life. Other available technical information on the pesticide (such as Lowest Observed Effect Concentrations and No Observed Effect Levels), the water bodies and the organisms involved will be evaluated to determine if lower concentrations are required to meet the narrative objectives (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | The one-tenth of 96-hour LC50 value, tested with dimethoate on the most sensitive species in freshwater (Cyclops strenuus, a copepod crustacean), is 0.2 µg/L.
Guideline Reference: | Ecotoxicity database. U.S. Environmental Protection Agency, Office of Pesticide Programs
Spatial Representation: | Water samples were collected from Hospital Creek at River Road.
Temporal Representation: | Samples were collected every two weeks or monthly between July 2004 and August 2006.
Environmental Conditions: |
QAPP Information: | Data Quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826 ) requirements.
QAPP Information Reference(s): | Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region

DECISION ID | 12884
Pollutant: | Escherichia coli (E. Coli)
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. Fifty-two of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Fifty-two of 105 samples exceed the E. Coli objective and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12884

LOE ID: | 22302
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 52
Number of Exceedances: | 21
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | The Westside San Joaquin River Water Quality Coalition collected 52 samples from July 2004 to October 2006. Seventeen out of the 21 samples collected exceeded the evaluation objective.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. The objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | The USEPA E. Coli objective of 235/100 mL in any single sample (USEPA 1986).
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Samples were collected at Hospital Creek at River Road.
Temporal Representation: | Monthly sampling occurred July 2004 to October 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 22303
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 53
Number of Exceedances: | 31
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | The Central Valley Regional Water Quality Control Board Surface Water Ambient Monitoring Program collected 16 samples from July 2002 to November 2005. Thirty-one out of 53 samples exceeded the evaluation objective.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. The objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | The USEPA E. Coli objective of 235/100 mL in any single sample (USEPA 1986).
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Samples were collected at Hospital Creek at Highway 33 and Hospital Creek at River Road.
Temporal Representation: | Sampling occurred from July 2002 to November 2005.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)

DECISION ID | 12880
Pollutant: | Lead
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess this pollutant. Two of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Two of 4 samples exceed the 4-day maximum criterion for total lead and this exceeds the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12880

LOE ID: | 25659
Pollutant: | Lead
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 4
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Four samples were taken from Hospital Creek in 2006. Two of the four samples exceed guidelines for total lead. Two samples exceed the 4-day average concentration levels.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
Water Quality Objective/Criterion: | California Toxics Rule Criteria (USEPA) - Freshwater Aquatic Life ProtectionContinuous Concentration (4-day Average) calculated based on the following formula (e{1.273xLN[hardness]}-4.705)
Objective/Criterion Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Hospital Creek at River Road.
Temporal Representation: | Monthly sampling from July 2006 - October 2006.
Environmental Conditions: |
QAPP Information: | Monitoring Reporting Program Order No. R5-2003-0826 for Coalition Groups Under Resolution No. R5-2003-0105 Conditional Waiver of Waste Discharge Requirements for Discharges from Irrigated Lands
QAPP Information Reference(s):

DECISION ID | 12879
Pollutant: | Pyrethroids
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess this pollutant. Three of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Three of 3 samples exceed the narrative toxicity objective and this exceeds the allowable frequency listed in Table 3.1 of the Listing Policy. Sediment-bound pyrethroid pesticide concentrations were used to calculate toxic units (TUs) of multiple pyrethroid pesticides observed in sediments. Pyrethroid TU analyses correlated with distribution and magnitude of toxicity. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12879

LOE ID: | 22319
Pollutant: | Pyrethroids
LOE Subgroup: | Pollutant-Sediment
Matrix: | Sediment
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 3
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Three of three statistically significant sediment toxicity testing samples violated the narrative toxicity objective. The three toxic (Mean mortality) sediment samples were collected from:Hospital Creek at Highway 338/27/04: 9810/13/04: 100Hospital Creek at River Road9/13/04: 25Toxicity observations were associated with pyrethroid pesticides. LC50s for sediment-bound pyrethroids were used in this study as toxicity threshold benchmarks in a Toxic Unit (TU) analysis normalized to organic carbon content. The TU analysis of Hospital Creek sediment samples demonstrated that the three samples with significant bioassay mortality had pyrethroid TUs well above 1.0. The samples collected on 8/27/04, 9/13/04, and 10/13/04 had 15.59, 2.47, and 5.57 TUs of pyrethroids, respectively. Chlorpyrifos was observed in two of three samples but at well below 1.0 TU. Bifenthrin appeared to play a dominant role in the toxic samples, followed by lambda-cyhalothrin, and esfenvalerate. Traces of permethrin were also observed in the 8/27/04 sample.LC50 concentrations for a 10-day exposure of Hyalella azteca to pyrethroid contaminated sediments were determined by Amweg et al., 2005. (Amweg, E.L., D.P. Weston, and N.M Ureda. 2005. Use and toxicity of pyrethroid pesticides in the Central Valley, California, U.S.A. Environ. Toxicol. Chem. 24:966-972 (with correction in Environ. Toxicol. Chem. 24:1300-1301)).
Data Reference:
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses. (CVRWQCB, 2007)All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control sediment using Dunnett¿s test in 10-day Hyalella azteca sediment toxicity tests. Arcsin squareroot transformation was used when necessary to meet the assumptions of normality and homogeneity of variance. Steel¿s test was used for comparison to control if these assumptions were not met after transformation.
Guideline Reference:
Spatial Representation: | Samples were collected from two locations on Hospital Creek in San Joaquin County. Sediment toxicity was observed from each of the three samples. Sample locations:Hospital Creek at Highway 33Hospital Creek at River Road
Temporal Representation: | Samples were collected August 2004 ¿ October 2004.Agricultural land use.
Environmental Conditions: |
QAPP Information: | Data quality: Good.. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):

DECISION ID | 12878
Pollutant: | Salinity
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Four lines of evidence are available in the administrative record to assess this pollutant. Twenty-six of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Twenty-six of 106 samples exceed the water quality objectives for electrical conductivity and total dissolved solids (collectively salinity) and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12878

LOE ID: | 22394
Pollutant: | Salinity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 6
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Six samples were taken from Hospital Creek between 2000 and 2002. Four of the 6 samples exceed the California Secondary MCL for TDS in surface water.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | The water quality objective used was the California Secondary MCL recommended level of 500 mg/L. The Basin Plan includes chemical constituent water quality objectives that include (by reference) secondary maximum contaminant levels (MCL¿s) protective of MUN (CVRWQCB, 2007a).The secondary MCL¿s for TDS provide a range of values including a recommended level (500 mg/L), upper level (1000 mg/L) and a short-term level (1500 mg/L). The ¿recommended¿ concentration was used as it is intended to be protective of all drinking water uses. Though individual listing evaluations did not look at the water supply source serving the given geographic area, there are certain areas that receive supply waters (such as the Delta Mendota Canal) that at times may be elevated above the recommended level of the secondary MCL. Where future information is made available to document this to be the case, these water bodies may be re-evaluated in future listing cycles.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road in Stanislaus County.
Temporal Representation: | Samples were collected between October 2000 and November 2005. Samples were collected at monthly intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
LOE ID: | 22375
Pollutant: | Salinity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 22
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Twenty-two samples were taken from Hospital Creek between 2004 and 2006. None of the twenty-two samples exceed the California Secondary MCL for EC in surface water.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | The water quality objective used was the California Secondary MCL recommended level of 900 uS/cm. The Basin Plan includes chemical constituent water quality objectives that include (by reference) secondary maximum contaminant levels (MCL¿s) protective of MUN (CVRWQCB, 2007a).The secondary MCL¿s for electrical conductivity provide a range of values including a recommended level (900 uS/cm), upper level (1600 uS/cm) and a short-term level (2200 uS/cm). The ¿recommended¿ concentration was used as it is intended to be protective of all drinking water uses. Though individual listing evaluations did not look at the water supply source serving the given geographic area, there are certain areas that receive supply waters (such as the Delta Mendota Canal) that at times may be elevated above the recommended level of the secondary MCL. Where future information is made available to document this to be the case, these water bodies may be re-evaluated in future listing cycles.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road in San Joaquin County.
Temporal Representation: | Samples were collected between July 2004 and October 2006. Samples were collected at monthly intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 22376
Pollutant: | Salinity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 57
Number of Exceedances: | 17
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Fifty-seven samples were taken from Hospital Creek between 2000 and 2005. Seventeen of the fifty-seven samples exceed the California Secondary MCL for EC in surface water.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | The water quality objective used was the California Secondary MCL recommended level of 900 uS/cm. The Basin Plan includes chemical constituent water quality objectives that include (by reference) secondary maximum contaminant levels (MCL¿s) protective of MUN (CVRWQCB, 2007a).The secondary MCL¿s for electrical conductivity provide a range of values including a recommended level (900 uS/cm), upper level (1600 uS/cm) and a short-term level (2200 uS/cm). The ¿recommended¿ concentration was used as it is intended to be protective of all drinking water uses. Though individual listing evaluations did not look at the water supply source serving the given geographic area, there are certain areas that receive supply waters (such as the Delta Mendota Canal) that at times may be elevated above the recommended level of the secondary MCL. Where future information is made available to document this to be the case, these water bodies may be re-evaluated in future listing cycles.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road and Highway 33 in San Joaquin County.
Temporal Representation: | Samples were collected between October 2000 and November 2005. Samples were collected at monthly intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
LOE ID: | 22377
Pollutant: | Salinity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 21
Number of Exceedances: | 5
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Twenty-one samples were taken from Hospital Creek between 2004 and 2006. Five of the twenty-one samples exceed the California Secondary MCL for TDS in surface water.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | The water quality objective used was the California Secondary MCL recommended level of 500 mg/L. The Basin Plan includes chemical constituent water quality objectives that include (by reference) secondary maximum contaminant levels (MCL¿s) protective of MUN (CVRWQCB, 2007a).The secondary MCL¿s for TDS provide a range of values including a recommended level (500 mg/L), upper level (1000 mg/L) and a short-term level (1500 mg/L). The ¿recommended¿ concentration was used as it is intended to be protective of all drinking water uses. Though individual listing evaluations did not look at the water supply source serving the given geographic area, there are certain areas that receive supply waters (such as the Delta Mendota Canal) that at times may be elevated above the recommended level of the secondary MCL. Where future information is made available to document this to be the case, these water bodies may be re-evaluated in future listing cycles.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road in San Joaquin County.
Temporal Representation: | Samples were collected between July 2004 and October 2006. Samples were collected at monthly intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):

DECISION ID | 12881
Pollutant: | Sediment Toxicity
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. Two of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Two of 3 samples exceed the narrative toxicity objective and this exceeds the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12881

LOE ID: | 22398
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Sediment
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 1
Data and Information Type: | TOXICITY TESTING
Data Used to Asses Water Quality: | One of the 2 samples tested with Hyalella azteca were toxic and violated the narrative toxicity objective. One sample collected at River Road exhibited a statistically significant decrease in survival compared to the control. The sample date and percent of control (in parentheses) are as follows:11 September 2006(1)
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | ¿All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.¿ (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 10-day Hyalella azteca sediment toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road.
Temporal Representation: | Samples were collected in September 2004 and September 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 22104
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Sediment
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 1
Data and Information Type: | TOXICITY TESTING
Data Used to Asses Water Quality: | One sample tested with Hyalella azteca was toxic and violated the narrative toxicity objective. One sample collected at River Road exhibited a statistically significant decrease in survival compared to the control. The sample date and percent of control (in parentheses) are as follows:30 March 2005 (22)
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | ¿All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.¿ (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 10-day Hyalella azteca sediment toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road.
Temporal Representation: | The sample was collected in March 2005.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)

DECISION ID | 12877
Pollutant: | Trifluralin
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Three lines of evidence are available in the administrative record to assess this pollutant. Two of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Two of 17 samples exceed the narrative toxicity objective and this exceeds the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12877

LOE ID: | 22336
Pollutant: | Trifluralin
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 12
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 12 water samples were collected from Hospital Creek at River Road near Patterson from July 2004 through June 2006 representing 12 concentrations.0 of 12 concentrations exceeded the maximum concentration of 0.70 µg/L.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | The Board will use the best available technical information to evaluate compliance with the narrative objectives. ¿Other available technical information on the pesticide (such as Lowest Observed Effect Concentrations and No Observed Effect Levels), the water bodies and organisms involved will be evaluated to determine if lower concentrations are required to meet the narrative objectives.¿ (CRWQCB, 2006).Lowest Observed Effects Concentration for Pimephales promelas is 0.7 ug/L Ecotoxicity Study 1582-09-8 (USEPA, 2008)
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road near Patterson, CA.
Temporal Representation: | Samples were collected at variable intervals (biweekly, weekly, monthly) from July 2004 through June 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 22320
Pollutant: | Trifluralin
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 2 water samples were collected from Hospital Creek at River Road Near Patterson in June 2001 and August 2001 representing 2 concentrations.1 of 2 concentrations exceeded the maximum concentration of 0.70 µg/L.
Data Reference: | Correspondence between the Department of Pesticide Regulation and Central Valley Regional Water Quality Control Board regarding water quality data for waterbodies in the Central Valley
| Report and data files for pesticides in the Sacramento River, Winter 2005
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | The Board will use the best available technical information to evaluate compliance with the narrative objectives. ¿Other available technical information on the pesticide (such as Lowest Observed Effect Concentrations and No Observed Effect Levels), the water bodies and organisms involved will be evaluated to determine if lower concentrations are required to meet the narrative objectives.¿ (CRWQCB, 2006).Lowest Observed Effects Concentration for Pimephales promelas is 0.7 ug/L Ecotoxicity Study 1582-09-8 (USEPA, 2008)
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Cree at River Road near Patterson, CA.
Temporal Representation: | Samples were collected in June 2001 and August 2001.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Minimum requirements for the CDPR Surface Water Database are: Name of the sampling agency or organization, Date that each sample was collected, Date of each sample analysis, County where samples were taken, Detailed sampling location information (including latitude and longitude or township/range/section if available), detailed map or description of each sampling site (i.e., address, cross roads, etc.), Name or description of water body sampled, Name of the active ingredient analyzed for; concentration detected (with unit of measurement), and limit of quantitation, Description of analytical QA/QC plan, or statement that no formal plan exists. Additional optional requirements are included on DPR's webpage at http://www.cdpr.ca.gov/docs/emon/surfwtr/caps/req.htm
QAPP Information Reference(s): | Standard Operating Procedure for Conducting Surface Water Monitoring for Pesticides
LOE ID: | 22321
Pollutant: | Trifluralin
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 3
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 3 water samples were collected from Hospital Creek at River Road near Patterson in March 1994, June 2001 and August 2001 representing 3 concentrations.1 of 3 concentrations exceeded the maximum concentration of 0.70 µg/L.
Data Reference: | National Water Quality Assessment database, San Joaquin and Tulare Basins data
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | The Board will use the best available technical information to evaluate compliance with the narrative objectives. ¿Other available technical information on the pesticide (such as Lowest Observed Effect Concentrations and No Observed Effect Levels), the water bodies and organisms involved will be evaluated to determine if lower concentrations are required to meet the narrative objectives.¿ (CRWQCB, 2006).Lowest Observed Effects Concentration for Pimephales promelas is 0.7 ug/L Ecotoxicity Study 1582-09-8 (USEPA, 2008)
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road near Patterson, CA.
Temporal Representation: | Samples were collected In March 1994, June 2001 and August 2001.
Environmental Conditions: |
QAPP Information: | Data quality: Good. In accordance with section 6.1.4 of the Listing Policy, data from major monitoring programs in California and Published USGS reports are considered of adequate quality.
QAPP Information Reference(s):

DECISION ID | 12882
Pollutant: | Unknown Toxicity
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Agriculture
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Five lines of evidence are available in the administrative record to assess this pollutant. Eight of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Two of 14 samples tested with selenastrum exceed the narrative toxicity objective and this exceeds the allowable frequency listed in Table 3.1 of the Listing Policy. In addition, 5 of 29 samples tested with ceriodaphnia exceed the narrative toxicity objective and this exceeds the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12882

LOE ID: | 22396
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 2
Data and Information Type: | TOXICITY TESTING
Data Used to Asses Water Quality: | 2 of the 14 samples tested with Ceriodaphnia dubia were toxic and violated the narrative toxicity objective. Two samples collected at River Road exhibited a statistically significant decrease in survival compared to the control. The sample dates and percent of control (in parentheses) are as follows:29 December 2004 (55)3 January 2006 (0)
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | ¿All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.¿ (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 4-day acute-style toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road.
Temporal Representation: | Samples were collected from July 2004 to August 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 22397
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 15
Number of Exceedances: | 3
Data and Information Type: | TOXICITY TESTING
Data Used to Asses Water Quality: | 3 of the 15 samples tested with Ceriodaphnia dubia were toxic and violated the narrative toxicity objective. Three samples collected at River Road exhibited a statistically significant decrease in survival compared to the control. The sample dates and percent of control (in parentheses) are as follows:23 March 2005 (0)19 April 2005 (0)16 August 2005 (0)
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | ¿All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.¿ (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a Fisher¿s Exact analysis with 48-hour acute-style toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road.
Temporal Representation: | Samples were collected from March 2001 to November 2005.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
LOE ID: | 22338
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Asses Water Quality: | Zero of the 13 samples tested with Pimephales promelas were toxic and violated the narrative toxicity objective.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | ¿All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.¿ (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a Fisher Exact analysis with 4-day acute-style toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road.
Temporal Representation: | Samples were collected from January 2001 to November 2005.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
LOE ID: | 22337
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 1
Data and Information Type: | TOXICITY TESTING
Data Used to Asses Water Quality: | One of the 14 samples tested with Pimephales promelas was toxic and violated the narrative toxicity objective. One sample collected at Hospital Creek at River Road exhibited a statistically significant decrease in survival compared to the control. The sample date and percent of control (in parentheses) is as follows:13 June 2006 (55)
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | ¿All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.¿ (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 4-day acute-style toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road.
Temporal Representation: | Samples were collected from July 2004 to August 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 22105
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 2
Data and Information Type: | TOXICITY TESTING
Data Used to Asses Water Quality: | Two of 14 samples tested with Selenastrum capricornutum were toxic and violated the narrative toxicity objective. Two samples collected at River Road exhibited a statistically significant decrease in growth compared to the control. The sample date and percent of control (in parentheses) are as follows:29 December 2004 (15)15 February 2005 (12)
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | ¿All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.¿ (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 4-day chronic-style toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from Hospital Creek at River Road.
Temporal Representation: | Samples were collected from July 2004 to August 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):