# Draft 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 5 - Central Valley Region

Water Body Name: | Merced River, Lower (McSwain Reservoir to San Joaquin River)
Water Body ID: | CAR5357000019980817154245
Water Body Type: | River & Stream

DECISION ID | 7421
Pollutant: | Chlorpyrifos
Final Listing Decision: | Do Not Delist from 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | List on 303(d) list (TMDL required list)(2006)
Revision Status | Revised
Sources: | Agriculture
Expected TMDL Completion Date: | 2008
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for removal on the section 303(d) list under sections 2.2 and 3.1 of the Listing Policy. Under 3.1 of the Policy, a minimum of one line of evidence is needed to assess listing status. Eight lines of evidence are available in the administrative record to assess this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against removing this water segment-pollutant combination from the section 303(d) list. There is sufficient justification to place it in the Being Addressed portion of the 303(d) list because a TMDL has been completed and approved by RWQCB and USEPA, and is expected to result in attainment of the standard.. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section NUMBER of the Policy. 2. The data used satisfies the data quantity requirements of section NUMBER of the Policy. 3. Eight of 167 available 4-day average concentrations exceeded the 4-day average maximum concentration criterion more than once every three years. In addition, 4 of 228 available 1-hour average concentrations exceeded the 1-hour average concentration criterion more than once every three years. 4. The San Joaquin River Organophosphorous Pesticide TMDL has been approved by the Central Valley Water Board in 2005 and approved by USEPA on 12/20/2006. 5. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be removed from the section 303(d) list because applicable water quality standards for the pollutant are being exceeded.
SWRCB Board Decision / Staff Recommendation: | N/A
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 7421

LOE ID: | 22243
Pollutant: | Chlorpyrifos
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 9
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 13 water samples were collected from Merced River between March and August 2004, representing 9 4-day average concentrations and 13 1-hour average concentrations.0 of 9 available 4-day average concentrations exceeded the 4-day maximum concentration guideline of 0.015 µg/L. 0 of 13 available 1-hour average concentrations exceeded the maximum 1-hour concentration of 0.025 µg/L.
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Department of Fish and Game Hazard Assessment Criteria - 0.015 µg/L 4-day average and 0.025 µg/L 1-hour average (Siepmann and Finlayson, 2000, with minor corrections to significant figures as described in Beaulaurier et al., 2005).
Guideline Reference:
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected at weekly interval in March, July, and August 2004.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 22244
Pollutant: | Chlorpyrifos
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 8 water samples were collected from Merced River in January and February 2005, representing 2 4-day average concentrations and 8 1-hour average concentrations.1 of 2 available 4-day average concentrations exceeded the 4-day maximum concentration guideline of 0.015 µg/L. 3 of 8 available 1-hour average concentrations exceeded the maximum 1-hour concentration of 0.025 µg/L.
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Department of Fish and Game Hazard Assessment Criteria - 0.015 µg/L 4-day average and 0.025 µg/L 1-hour average (Siepmann and Finlayson, 2000, with minor corrections to significant figures as described in Beaulaurier et al., 2005).
Guideline Reference:
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected at daily in January and February 2005.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 22254
Pollutant: | Chlorpyrifos
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 14 water samples were collected from Merced River between March and August 2005, representing 14 4-day average concentrations and 14 1-hour average concentrations.2 of 14 available 4-day average concentrations exceeded the 4-day maximum concentration guideline of 0.015 µg/L. 0 of 14 available 1-hour average concentrations exceeded the maximum 1-hour concentration of 0.025 µg/L.
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Department of Fish and Game Hazard Assessment Criteria - 0.015 µg/L 4-day average and 0.025 µg/L 1-hour average (Siepmann and Finlayson, 2000, with minor corrections to significant figures as described in Beaulaurier et al., 2005).
Guideline Reference:
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected at weekly in March, July, and August 2005.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 22255
Pollutant: | Chlorpyrifos
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 13 water samples were collected from Merced River between March and August 2006, representing 13 4-day average concentrations and 13 1-hour average concentrations.1 of 13 available 4-day average concentrations exceeded the 4-day maximum concentration guideline of 0.015 µg/L. 0 of 13 available 1-hour average concentrations exceeded the maximum 1-hour concentration of 0.025 µg/L.
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Department of Fish and Game Hazard Assessment Criteria - 0.015 µg/L 4-day average and 0.025 µg/L 1-hour average (Siepmann and Finlayson, 2000, with minor corrections to significant figures as described in Beaulaurier et al., 2005).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected weekly in March, July, and August 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 22242
Pollutant: | Chlorpyrifos
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 10 water samples were collected from Merced River in February 2004, representing 2 4-day average concentrations and 10 1-hour average concentrations.0 of 2 available 4-day average concentrations exceeded the 4-day maximum concentration guideline of 0.015 µg/L. 0 of 10 available 1-hour average concentrations exceeded the maximum 1-hour concentration of 0.025 µg/L.
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Department of Fish and Game Hazard Assessment Criteria - 0.015 µg/L 4-day average and 0.025 µg/L 1-hour average (Siepmann and Finlayson, 2000, with minor corrections to significant figures as described in Beaulaurier et al., 2005).
Guideline Reference:
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected daily during two storms in February 2004.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 22241
Pollutant: | Chlorpyrifos
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 5
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 17 water samples were collected from Merced River from January to March 2003, representing 5 4-day average concentrations and 17 1-hour average concentrations.0 of 5 available 4-day average concentrations exceeded the 4-day maximum concentration guideline of 0.015 µg/L. 0 of 17 available 1-hour average concentrations exceeded the maximum 1-hour chlorpyrifos concentration of 0.025 µg/L.
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Department of Fish and Game Hazard Assessment Criteria - 0.015 µg/L 4-day average and 0.025 µg/L 1-hour average (Siepmann and Finlayson, 2000, with minor corrections to significant figures as described in Beaulaurier et al., 2005).
Guideline Reference:
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected daily during two storms in February and March 2003.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 22257
Pollutant: | Chlorpyrifos
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 109
Number of Exceedances: | 4
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 140 water samples were collected from Merced River from January 2000 through June 2005, representing 109 4-day average concentrations and 140 1-hour average concentrations. 4 of 109 4-day average concentrations exceeded the 4-day maximum concentration guideline of 0.015 µg/L.1 of 140 1-hour average concentrations exceeded the maximum 1-hour concentration of 0.025 µg/L.
Data Reference: | Surface Water database (SWDB) for Central Valley waterbodies, 2000-2005
| Correspondence between the Department of Pesticide Regulation and Central Valley Regional Water Quality Control Board regarding water quality data for waterbodies in the Central Valley
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Department of Fish and Game Hazard Assessment Criteria - 0.015 µg/L 4-day average and 0.025 µg/L 1-hour average (Siepmann and Finlayson, 2000, with minor corrections to significant figures as described in Beaulaurier et al., 2005).
Guideline Reference:
Spatial Representation: | Samples were collected at variable intervals from Merced River at River Road Bridge near Newman.
Temporal Representation: | Samples were collected weekly between January 2000 and June 2005.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Minimum requirements for the CDPR Surface Water Database are: Name of the sampling agency or organization, Date that each sample was collected, Date of each sample analysis, County where samples were taken, Detailed sampling location information (including latitude and longitude or township/range/section if available), detailed map or description of each sampling site (i.e., address, cross roads, etc.), Name or description of water body sampled, Name of the active ingredient analyzed for; concentration detected (with unit of measurement), and limit of quantitation, Description of analytical QA/QC plan, or statement that no formal plan exists. Additional optional requirements are included on DPR's webpage at http://www.cdpr.ca.gov/docs/emon/surfwtr/caps/req.htm
QAPP Information Reference(s): | Standard Operating Procedure for Conducting Surface Water Monitoring for Pesticides
LOE ID: | 22256
Pollutant: | Chlorpyrifos
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 17 water samples were collected from Merced River from July 2004 through September 2006, representing 13 4-day average concentrations and 13 1-hour average concentrations.0 of 13 4-day average concentrations exceeded the 4-day maximum concentration guideline of 0.015 µg/L.0 of 13 1-hour average concentrations exceeded the maximum 1-hour concentration of 0.025 µg/L. 4 samples were not used in this analysis because of the quantitation limit (0.0254 µg/L) greater than the water quality criteria concentrations (0.015 µg/L).
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Department of Fish and Game Hazard Assessment Criteria - 0.015 µg/L 4-day average and 0.025 µg/L 1-hour average (Siepmann and Finlayson, 2000, with minor corrections to significant figures as described in Beaulaurier et al., 2005).
Guideline Reference:
Spatial Representation: | Samples were collected from Merced River at Santa Fe.
Temporal Representation: | Samples were collected weekly from July 2004 through September 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 4476
Pollutant: | Chlorpyrifos
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Not Recorded
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 0
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Asses Water Quality: | Unspecified--This LOE is a placeholder to support a 303(d) listing decision made prior to 2006.
Data Reference: | Placeholder reference pre-2006 303(d)
Water Quality Objective/Criterion: | Unspecified
Objective/Criterion Reference: | Placeholder reference pre-2006 303(d)
Evaluation Guideline: | Unspecified
Guideline Reference: | Placeholder reference pre-2006 303(d)
Spatial Representation: | Unspecified
Temporal Representation: | Unspecified
Environmental Conditions: | Unspecified
QAPP Information: | Unspecified
QAPP Information Reference(s):

DECISION ID | 7422
Pollutant: | Diazinon
Final Listing Decision: | Do Not Delist from 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | List on 303(d) list (TMDL required list)(2006)
Revision Status | Revised
Sources: | Agriculture
Expected TMDL Completion Date: | 2008
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for removal on the section 303(d) list under sections 2.2 and 3.1 of the Listing Policy. Under 3.1 of the Policy, a minimum of one line of evidence is needed to assess listing status. Eight lines of evidence are available in the administrative record to assess this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against removing this water segment-pollutant combination from the section 303(d) list. There is sufficient justification to place it in the Being Addressed portion of the 303(d) list because a TMDL has been completed and approved by RWQCB and USEPA, and is expected to result in attainment of the standard.. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section NUMBER of the Policy. 2. The data used satisfies the data quantity requirements of section NUMBER of the Policy. 3. One of 181 available 4-day average concentrations exceeded the 4-day average maximum concentration criterion more than once every three years. In addition, 3 of 248 available 1-hour average concentrations exceeded the 1-hour average concentration criterion more than once every three years. 4. The San Joaquin River Organophosphorous Pesticide TMDL has been approved by the Central Valley Water Board in 2005 and approved by USEPA on 12/20/2006. 5. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be removed from the section 303(d) list because applicable water quality standards for the pollutant are being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 7422

LOE ID: | 23044
Pollutant: | Diazinon
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 107
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 140 Water samples were collected from Merced River from January 2000 through June 2005, representing 107 4-day average concentrations and 140 1-hour average concentrations.1 of 107 available 4-day average concentrations exceeded the 4-day maximum concentration guideline of 0.1 µg/L. 3 of 140 available 1-hour average concentrations exceeded the maximum 1-hour concentration of 0.16 µg/L.
Data Reference: | Surface Water database (SWDB) for Central Valley waterbodies, 2000-2005
| Correspondence between the Department of Pesticide Regulation and Central Valley Regional Water Quality Control Board regarding water quality data for waterbodies in the Central Valley
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Fish and Game Hazard Assessment Criteria - 0.160 µg/L 1-hour average and 0.100 µg/L 4-day average concentration not to be exceeded more than once every three years (Siepmann and Finlayson, 2000 and Finlayson, 2004).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected at variable intervals (e.g. hourly, weekly, monthly) from January 2000 through June 2005.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Minimum requirements for the CDPR Surface Water Database are: Name of the sampling agency or organization, Date that each sample was collected, Date of each sample analysis, County where samples were taken, Detailed sampling location information (including latitude and longitude or township/range/section if available), detailed map or description of each sampling site (i.e., address, cross roads, etc.), Name or description of water body sampled, Name of the active ingredient analyzed for; concentration detected (with unit of measurement), and limit of quantitation, Description of analytical QA/QC plan, or statement that no formal plan exists. Additional optional requirements are included on DPR's webpage at http://www.cdpr.ca.gov/docs/emon/surfwtr/caps/req.htm
QAPP Information Reference(s): | Standard Operating Procedure for Conducting Surface Water Monitoring for Pesticides
LOE ID: | 23043
Pollutant: | Diazinon
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 22 water samples were collected from Merced River from January through August 2006, representing 15 4-day average concentrations and 22 1-hour average concentrations.0 of 15 available 4-day average concentrations exceeded the 4-day maximum concentration guideline of 0.10 µg/L. 0 of 22 available 1-hour average concentrations exceeded the maximum 1-hour concentration of 0.16 µg/L.
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Fish and Game Hazard Assessment Criteria ¿ 0.160 µg/L 1-hour average and 0.100 µg/L 4-day average concentration not to be exceeded more than once every three years (Siepmann and Finlayson, 2000 and Finlayson, 2004).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected at daily and weekly intervals from January through August 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 23042
Pollutant: | Diazinon
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 14 water samples were collected from Merced River from March through August 2005, representing 14 4-day average concentrations and 14 1-hour average concentrations.0 of 14 available 4-day average concentrations exceeded the 4-day maximum concentration guideline of 0.10 µg/L. 0 of 14 available 1-hour average concentrations exceeded the maximum 1-hour concentration of 0.16 µg/L.
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Fish and Game Hazard Assessment Criteria - 0.160 µg/L 1-hour average and 0.100 µg/L 4-day average concentration not to be exceeded more than once every three years (Siepmann and Finlayson, 2000 and Finlayson, 2004).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected at weekly interval from January through March 2005.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 23041
Pollutant: | Diazinon
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 6
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 14 water samples were collected from Merced River from January through March 2005, representing 6 4-day average concentrations and 14 1-hour average concentrations.0 of 6 available 4-day average concentrations exceeded the 4-day maximum concentration guideline of 0.10 µg/L. 0 of 14 available 1-hour average concentrations exceeded the maximum 1-hour concentration of 0.16 µg/L.
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Fish and Game Hazard Assessment Criteria - 0.160 µg/L 1-hour average and 0.100 µg/L 4-day average concentration not to be exceeded more than once every three years (Siepmann and Finlayson, 2000 and Finlayson, 2004).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected at variable intervals (hourly, daily, and weekly) from January through March 2005.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 23025
Pollutant: | Diazinon
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 13 water samples were collected from Merced River from March to August 2004, representing 13 4-day average concentrations and 13 1-hour average concentrations.0 of 13 available 4-day average concentrations exceeded the 4-day maximum concentration guideline of 0.10 µg/L. 0 of 13 available 1-hour average concentrations exceeded the maximum 1-hour concentration of 0.16 µg/L.
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Fish and Game Hazard Assessment Criteria - 0.160 µg/L 1-hour average and 0.100 µg/L 4-day average concentration not to be exceeded more than once every three years (Siepmann and Finlayson, 2000 and Finlayson, 2004).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected at variable intervals (weekly or biweekly) from March to August 2004.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 23024
Pollutant: | Diazinon
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 10 water samples were collected from Merced River in February 2004, representing 2 4-day average concentrations and 10 1-hour average concentrations.0 of 2 available 4-day average concentrations exceeded the 4-day maximum concentration guideline of 0.10 µg/L. 1 of 10 available 1-hour average concentrations exceeded the maximum 1-hour concentration of 0.16 µg/L.
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Fish and Game Hazard Assessment Criteria - 0.160 µg/L 1-hour average and 0.100 µg/L 4-day average concentration not to be exceeded more than once every three years (Siepmann and Finlayson, 2000 and Finlayson, 2004).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected at variable intervals (hourly and daily) during two storm events in February 2004.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 23023
Pollutant: | Diazinon
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 19
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 19 water samples were collected from Merced River from March to August 2003, representing 19 4-day average concentrations and 19 1-hour average concentrations.0 of 19 available 4-day average concentrations exceeded the 4-day maximum concentration guideline of 0.1 µg/L. 0 of 19 available 1-hour average concentrations exceeded the maximum 1-hour concentration of 0.16 µg/L.
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Fish and Game Hazard Assessment Criteria - 0.160 µg/L 1-hour average and 0.100 µg/L 4-day average concentration not to be exceeded more than once every three years (Siepmann and Finlayson, 2000 and Finlayson, 2004).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected at variable intervals (biweekly and weekly) from March through August 2003.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 23022
Pollutant: | Diazinon
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 6
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 17 water samples were collected from Merced River from February to March 2003, representing 6 4-day average concentrations and 19 1-hour average concentrations.0 of 6 available 4-day average concentrations exceeded the 4-day maximum concentration guideline of 0.10 µg/L. 0 of 17 available 1-hour average concentrations exceeded the maximum 1-hour concentration of 0.16 µg/L.
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007). All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Fish and Game Hazard Assessment Criteria - 0.160 µg/L 1-hour average and 0.100 µg/L 4-day average concentration not to be exceeded more than once every three years (Siepmann and Finlayson, 2000 and Finlayson, 2004).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected at variable intervals (hourly or daily) from February to March 2003.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 4477
Pollutant: | Diazinon
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Not Recorded
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 0
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Asses Water Quality: | Unspecified--This LOE is a placeholder to support a 303(d) listing decision made prior to 2006.
Data Reference: | Placeholder reference pre-2006 303(d)
Water Quality Objective/Criterion: | Unspecified
Objective/Criterion Reference: | Placeholder reference pre-2006 303(d)
Evaluation Guideline: | Unspecified
Guideline Reference: | Placeholder reference pre-2006 303(d)
Spatial Representation: | Unspecified
Temporal Representation: | Unspecified
Environmental Conditions: | Unspecified
QAPP Information: | Unspecified
QAPP Information Reference(s):

DECISION ID | 10161
Pollutant: | Ammonia
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 2 available concentrations exceeded the CMC Guideline for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 2 available concentrations exceeded the USEPA Health Advisory for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10161

LOE ID: | 6336
Pollutant: | Ammonia
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Asses Water Quality: | 0 of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation guideline for Ammonia.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Ammonia levels should not to exceed the calculated limit. Freshwater Aquatic Life Protection (Salmonid present) Criteria Maximum Concentration (CMC) (1-hour Average (mg N/L)) calculated based on the following formula: CMC = (0.275/(1 + 107.204-pH)) + (39.0/(1 + 10pH-7.204)) which incorporates pH (US EPA, 2005: Appendix C)
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from May 25 2000 to Jul 27 2000
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 20480
Pollutant: | Ammonia
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 2
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Ammonia.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Ammonia levels should not exceed 30 mg/L (USEPA Health Advisory)
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from May 25 2000 to Jul 27 2000
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10163
Pollutant: | Arsenic
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 13 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 5 available concentrations exceeded the USEPA Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10163

LOE ID: | 20441
Pollutant: | Arsenic
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 5
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 5 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Arsenic.
Data Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Arsenic levels should not exceed 10 ug/L (USEPA Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Mar 20 2003 to Jun 30 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 6338
Pollutant: | Arsenic
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Asses Water Quality: | 0 of the 13 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Arsenic.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Arsenic levels should not exceed 340 ug/L maximum concentration for 1-hour average (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals - 2007 for toxicity data
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Aug 29 2001 to Nov 20 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10164
Pollutant: | Boron
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 64 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. Table 3.1 of the listing policy recommends listing if a sample size of 64 has 6 or more samples that exceed the evaluation criteria. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10164

LOE ID: | 21070
Pollutant: | Boron
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 64
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 64 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Boron.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Boron levels should not exceed 1000 ug/L (Department of Health Services Health Advisory)
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Jan 28 1998 to Nov 29 2005
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10165
Pollutant: | Cadmium
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 6 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 5 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10165

LOE ID: | 20443
Pollutant: | Cadmium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 5
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 5 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Cadmium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Cadmium levels should not exceed 5 ug/L (Department of Public Health Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Mar 20 2003 to Jun 30 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 6340
Pollutant: | Cadmium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 6
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Asses Water Quality: | 0 of the 6 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Cadmium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Cadmium levels should not exceed the calculated limit based on the formula: Criteria Maximum Concentration (1-hour Average dissolved)=(EXP(1.128*LN(hardness)-3.6867))*(1.136672-(LN(hardness)*0.041838)) (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals - 2007 for toxicity data
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Sep 26 2001 to Nov 20 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10167
Pollutant: | Chloride
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 27 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. Table 3.1 of the listing policy recommends listing if a sample size of 27 has 3 or more samples that exceed the evaluation criteria. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10167

LOE ID: | 20842
Pollutant: | Chloride
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 27
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 27 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Chloride.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Chloride levels should not exceed 250 mg/L (USEPA Maximum Contaminant Level)
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Jan 28 1998 to Jun 30 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10168
Pollutant: | Chromium (total)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 15 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10168

LOE ID: | 20778
Pollutant: | Chromium (total)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 15 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Chromium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Chromium levels should not exceed 50 ug/L (Department of Public Health Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Jun 24 1998 to Jun 30 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10170
Pollutant: | Copper
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 13 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 15 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10170

LOE ID: | 6342
Pollutant: | Copper
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Asses Water Quality: | 0 of the 13 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Copper.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Copper levels should not exceed calculated limit based on the formula: Criteria Maximum Concentration (1-hour Average, dissolved)=(EXP(0.9422*LN(hardness)-1.7))*(0.96) (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals - 2007 for toxicity data
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Oct 26 2000 to Nov 20 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 20801
Pollutant: | Copper
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 15 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Copper.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Copper levels should not exceed 1300 ug/L (Department of Public Health Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Jun 24 1998 to Jun 30 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 14795
Pollutant: | Dacthal
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. Zero of 143 water samples exceed the narrative toxicity water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Zero of 143 water samples contained dacthal at concentrations above the Evaluation Guideline for dacthal of 0.008 ug/L (none of the samples exceeded the narrative toxicity objective), and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 14795

LOE ID: | 26155
Pollutant: | Dacthal
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 143
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Zero of 143 water samples collected from Merced River by the United States Geological Survey, under the National Water Information System program, between January 2000 and August 2005 exceeded the USEPA National Ambient Water Quality Criterion for dacthal (DCPA) of 0.008 µg/L.
Data Reference: | National Water Quality Assessment database, Sacramento Study Unit data
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | USEPA National Ambient Water Quality Criterion for dacthal (DCPA) of 0.008 µg/L.
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Water samples were collected from the Merced River at River Road.
Temporal Representation: | Samples were collected hourly, daily or weekly from the Merced River between January 2000 and August 2005.
Environmental Conditions: |
QAPP Information: | Data Quality: Good: U.S. Geological Survey, variously dated, National field manual for the collection of water-quality data: U.S. Geological Survey Techniques of Water-Resources Investigations, book 9, chaps. A1-A9, available online at http://pubs.water.usgs.gov/twri9A
QAPP Information Reference(s): | National field manual for the collection of water quality data. Reston, VA. U.S. Geological Survey. Office of Water Quality
| Field measurements: U.S. Geological Survey Techniques of Water-Resources Investigations, book 9, chap. A6. In United States Geological Survey (USGS). Variously dated. National field manual for the collection of water-quality data: U.S. Geological Survey Techniques of Water-Resources Investigations, book 9, chaps. A1-A9, available online at http://pubs.water.usgs.gov/twri9A.

DECISION ID | 10171
Pollutant: | Lead
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 14 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 15 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10171

LOE ID: | 20791
Pollutant: | Lead
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 15 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Lead.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Lead levels should not exceed 15 ug/L (Department of Public Health Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Jun 24 1998 to Jun 30 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 6345
Pollutant: | Lead
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Asses Water Quality: | 0 of the 14 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Lead.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Lead levels should not exceed the calculated value based on the formula: Criteria Maximum Concentration (1-hour Average, dissolved)=(EXP(1.273*LN(hardness)-1.46))*(1.46203-(LN(hardness)*0.145712)) (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals - 2007 for toxicity data
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Oct 26 2000 to Nov 20 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10176
Pollutant: | Nickel
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 14 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 15 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10176

LOE ID: | 6352
Pollutant: | Nickel
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Asses Water Quality: | 0 of the 14 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Nickel.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Nickel levels should not exceed the calculated limit based on the formula: Criteria Maximum Concentration (1-hour Average, dissolved)=(EXP(0.846*LN(hardness)+2.255))*(0.998)(CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals - 2007 for toxicity data
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Oct 26 2000 to Nov 20 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 20847
Pollutant: | Nickel
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 15 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Nickel.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Nickel levels should not exceed 100 ug/L (Department of Public Health Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Jun 24 1998 to Jun 30 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10177
Pollutant: | Nitrate as Nitrate (NO3)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 15 available concentrations exceeded the USEPA Primary MCL and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is based on staff findings that 0 of 15 available concentrations exceeded the USEPA National Ambient Water Quality Objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10177

LOE ID: | 6353
Pollutant: | Nitrate as Nitrate (NO3)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Asses Water Quality: | 0 of the 15 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation guideline for Nitrate-N.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Nitrate-N levels should not to exceed 100 mg/L (USEPA National Ambient Water Quality Objective)
Guideline Reference: | National Recommended Water Quality Criteria. United States Environmental Protection Agency. Office of Water. Office of Science and Technology. 4304T
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Jun 29 2000 to Oct 24 2001
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 20485
Pollutant: | Nitrate as Nitrate (NO3)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 15 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Nitrate-N.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Nitrate-N levels should not exceed 45 mg/L (Department of Public Health Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Jun 29 2000 to Oct 24 2001
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 13803
Pollutant: | Oxygen, Dissolved
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess this pollutant. One of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. One of 20 samples fell below the minimum criterion water quality objective listed in the Sacramento/San Joaquin River Basin Plan and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 13803

LOE ID: | 22229
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 20
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Twenty samples were taken from the Lower Merced River between 2004 and 2006. One of the twenty samples fell below the Water Quality Objective for minimum dissolved oxygen content in surface water.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | From the Sacramento/San Joaquin River Basin Plan the (COLD) Cold Freshwater Habitat criterion is a Minimum Dissolved Oxygen content of 7mg/L.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from the Lower Merced River at Santa Fe Avenue in Merced County.
Temporal Representation: | Samples were collected between July 2004 and September 2006. Samples were collected at bi-monthly and monthly intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):

DECISION ID | 13820
Pollutant: | Sediment Toxicity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 7 samples exceeded the narrative toxicity objective and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 13820

LOE ID: | 23062
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Sediment
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 6
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Asses Water Quality: | None of the 6 samples tested with Hyalella azteca were toxic and violated the narrative toxicity objective.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.¿ (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 10-day Hyalella azteca sediment toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from Merced River at Santa Fe
Temporal Representation: | Samples were collected in August 2004 and August 2006
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 23063
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Sediment
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Asses Water Quality: | One sample tested with Hyalella azteca was not toxic nor did it violate the narrative toxicity objective.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | ¿All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.¿ (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 10-day Hyalella azteca sediment toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from Merced River at River Road
Temporal Representation: | The sample was collected in May 2002
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)

DECISION ID | 10178
Pollutant: | Selenium
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 69 available concentrations exceeded the Department of Public Health Primary MCL and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is based on staff findings that 0 of 69 available concentrations exceeded the Basin Plan Objective for Selenium and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10178

LOE ID: | 6936
Pollutant: | Selenium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 69
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Asses Water Quality: | 0 of the 69 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Selenium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Selenium levels should not to exceed 5 ug/L (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals - 2007 for toxicity data
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Jan 28 1998 to Nov 29 2005
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 21071
Pollutant: | Selenium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 69
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 69 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Selenium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Evaluation Guideline: | Selenium levels should not exceed 50 ug/L (Department of Public Health Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Jan 28 1998 to Nov 29 2005
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 13828
Pollutant: | Simazine
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Nine lines of evidence are available in the administrative record to assess this pollutant. One of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. One of 235 samples exceeded the drinking water standard (4 µg/L) and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 13828

LOE ID: | 22214
Pollutant: | Simazine
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 140
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 140 water samples were collected from Merced River from January 2000 through June 2005, representing 140 concentrations.1 of 140 concentrations exceeded the MCLs for drinking water standard (4 ug/L)
Data Reference: | Surface Water database (SWDB) for Central Valley waterbodies, 2000-2005
| Correspondence between the Department of Pesticide Regulation and Central Valley Regional Water Quality Control Board regarding water quality data for waterbodies in the Central Valley
Water Quality Objective/Criterion: | At a minimum, water designated for use as domestic or municipal supply (MUN) shall not contain concentrations of chemical constituents in excess of the maximum contaminant levels (MCLs) specified in the following provisions of Title 22 of the California Code of Regulations, which are incorporated by reference into this plan: Tables 64431-A (Inorganic Chemicals) and 64431-B (Fluoride) of Section 64431, Table 64444-A (Organic Chemicals) of Section 64444, and Tables 64449-A (Secondary Maximum Contaminant Levels-Consumer Acceptance Limits) and 64449-B (Secondary Maximum Contaminant Levels-Ranges) of Section 64449. The Maximum Contaminant Level (MCL) for simazine is 4 ug/L.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Spatial Representation: | Samples were collected from Merced River at River Road near Newman.
Temporal Representation: | Samples were collected at variable intervals (e.g. several samples per day, daily, and weekly) from January 2000 through June 2005.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Minimum requirements for the CDPR Surface Water Database are: Name of the sampling agency or organization, Date that each sample was collected, Date of each sample analysis, County where samples were taken, Detailed sampling location information (including latitude and longitude or township/range/section if available), detailed map or description of each sampling site (i.e., address, cross roads, etc.), Name or description of water body sampled, Name of the active ingredient analyzed for; concentration detected (with unit of measurement), and limit of quantitation, Description of analytical QA/QC plan, or statement that no formal plan exists. Additional optional requirements are included on DPR's webpage at http://www.cdpr.ca.gov/docs/emon/surfwtr/caps/req.htm
QAPP Information Reference(s): | Standard Operating Procedure for Conducting Surface Water Monitoring for Pesticides
LOE ID: | 22212
Pollutant: | Simazine
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 13 water samples were collected from Merced River between March and August 2006, representing 13 concentrations. 0 of 13 available concentrations exceeded MCL (4 µg/L).
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | At a minimum, water designated for use as domestic or municipal supply (MUN) shall not contain concentrations of chemical constituents in excess of the maximum contaminant levels (MCLs) specified in the following provisions of Title 22 of the California Code of Regulations, which are incorporated by reference into this plan: Tables 64431-A (Inorganic Chemicals) and 64431-B (Fluoride) of Section 64431, Table 64444-A (Organic Chemicals) of Section 64444, and Tables 64449-A (Secondary Maximum Contaminant Levels-Consumer Acceptance Limits) and 64449-B (Secondary Maximum Contaminant Levels-Ranges) of Section 64449. The Maximum Contaminant Level (MCL) for simazine is 4 ug/L.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected at weekly in March, July, and August 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 22211
Pollutant: | Simazine
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 9
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 9 water samples were collected from Merced River between March and August 2005, representing 9 concentrations. 0 of 9 available concentrations exceeded the MCL (4 µg/L).
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | At a minimum, water designated for use as domestic or municipal supply (MUN) shall not contain concentrations of chemical constituents in excess of the maximum contaminant levels (MCLs) specified in the following provisions of Title 22 of the California Code of Regulations, which are incorporated by reference into this plan: Tables 64431-A (Inorganic Chemicals) and 64431-B (Fluoride) of Section 64431, Table 64444-A (Organic Chemicals) of Section 64444, and Tables 64449-A (Secondary Maximum Contaminant Levels-Consumer Acceptance Limits) and 64449-B (Secondary Maximum Contaminant Levels-Ranges) of Section 64449. The Maximum Contaminant Level (MCL) for simazine is 4 ug/L.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Spatial Representation: |
Temporal Representation: | Samples were collected at weekly in March, July, and August 2005.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 22210
Pollutant: | Simazine
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 9
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 9 water samples were collected from Merced River in January and February 2005, representing 9 concentrations.0 of 9 available concentrations exceeded the MCL (4 µg/L).
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | At a minimum, water designated for use as domestic or municipal supply (MUN) shall not contain concentrations of chemical constituents in excess of the maximum contaminant levels (MCLs) specified in the following provisions of Title 22 of the California Code of Regulations, which are incorporated by reference into this plan: Tables 64431-A (Inorganic Chemicals) and 64431-B (Fluoride) of Section 64431, Table 64444-A (Organic Chemicals) of Section 64444, and Tables 64449-A (Secondary Maximum Contaminant Levels-Consumer Acceptance Limits) and 64449-B (Secondary Maximum Contaminant Levels-Ranges) of Section 64449. The Maximum Contaminant Level (MCL) for simazine is 4 ug/L.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected at daily in two storms in January and February 2005.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 22199
Pollutant: | Simazine
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 13 water samples were collected from Merced River between March and August 2004, representing 13 concentrations.0 of 13 available concentrations exceeded the MCL (4 µg/L).
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | At a minimum, water designated for use as domestic or municipal supply (MUN) shall not contain concentrations of chemical constituents in excess of the maximum contaminant levels (MCLs) specified in the following provisions of Title 22 of the California Code of Regulations, which are incorporated by reference into this plan: Tables 64431-A (Inorganic Chemicals) and 64431-B (Fluoride) of Section 64431, Table 64444-A (Organic Chemicals) of Section 64444, and Tables 64449-A (Secondary Maximum Contaminant Levels-Consumer Acceptance Limits) and 64449-B (Secondary Maximum Contaminant Levels-Ranges) of Section 64449. The Maximum Contaminant Level (MCL) for simazine is 4 ug/L.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected at weekly interval in March, July, and August 2004.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 22198
Pollutant: | Simazine
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 10
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 10 water samples were collected from Merced River in February 2004, representing 10 concentrations.0 of 10 available concentrations exceeded the MCL (4 µg/L).
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | At a minimum, water designated for use as domestic or municipal supply (MUN) shall not contain concentrations of chemical constituents in excess of the maximum contaminant levels (MCLs) specified in the following provisions of Title 22 of the California Code of Regulations, which are incorporated by reference into this plan: Tables 64431-A (Inorganic Chemicals) and 64431-B (Fluoride) of Section 64431, Table 64444-A (Organic Chemicals) of Section 64444, and Tables 64449-A (Secondary Maximum Contaminant Levels-Consumer Acceptance Limits) and 64449-B (Secondary Maximum Contaminant Levels-Ranges) of Section 64449. The Maximum Contaminant Level (MCL) for simazine is 4 ug/L.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected daily during two storms in February 2004.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 22213
Pollutant: | Simazine
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 5
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 5 water samples were collected from Merced River from July 2004 through September 2006, representing 5 concentrations.0 of 5 concentrations exceeded the MCL (4 µg/L).
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | At a minimum, water designated for use as domestic or municipal supply (MUN) shall not contain concentrations of chemical constituents in excess of the maximum contaminant levels (MCLs) specified in the following provisions of Title 22 of the California Code of Regulations, which are incorporated by reference into this plan: Tables 64431-A (Inorganic Chemicals) and 64431-B (Fluoride) of Section 64431, Table 64444-A (Organic Chemicals) of Section 64444, and Tables 64449-A (Secondary Maximum Contaminant Levels-Consumer Acceptance Limits) and 64449-B (Secondary Maximum Contaminant Levels-Ranges) of Section 64449. The Maximum Contaminant Level (MCL) for simazine is 4 ug/L.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Merced River at Santa Fe.
Temporal Representation: | Samples were collected weekly from July 2004 through September 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 22197
Pollutant: | Simazine
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 19
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 19 water samples were collected from Merced River from March to August 2003, representing 19 concentrations.0 of 19 available concentrations exceeded the MCL (4 µg/L)
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | At a minimum, water designated for use as domestic or municipal supply (MUN) shall not contain concentrations of chemical constituents in excess of the maximum contaminant levels (MCLs) specified in the following provisions of Title 22 of the California Code of Regulations, which are incorporated by reference into this plan: Tables 64431-A (Inorganic Chemicals) and 64431-B (Fluoride) of Section 64431, Table 64444-A (Organic Chemicals) of Section 64444, and Tables 64449-A (Secondary Maximum Contaminant Levels-Consumer Acceptance Limits) and 64449-B (Secondary Maximum Contaminant Levels-Ranges) of Section 64449. The Maximum Contaminant Level (MCL) for simazine is 4 ug/L.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected biweekly from March through August 2003.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 22196
Pollutant: | Simazine
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 17
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 17 water samples were collected from Merced River from January to March 2003, representing 17 concentrations.0 of 17 available concentrations exceeded the MCL (4 µg/L)
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | At a minimum, water designated for use as domestic or municipal supply (MUN) shall not contain concentrations of chemical constituents in excess of the maximum contaminant levels (MCLs) specified in the following provisions of Title 22 of the California Code of Regulations, which are incorporated by reference into this plan: Tables 64431-A (Inorganic Chemicals) and 64431-B (Fluoride) of Section 64431, Table 64444-A (Organic Chemicals) of Section 64444, and Tables 64449-A (Secondary Maximum Contaminant Levels-Consumer Acceptance Limits) and 64449-B (Secondary Maximum Contaminant Levels-Ranges) of Section 64449. The Maximum Contaminant Level (MCL) for simazine is 4 ug/L.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected daily during two storms from January through March 2003.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006

DECISION ID | 10179
Pollutant: | Specific Conductivity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 134 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.2 of the Listing Policy. Table 3.2 of the listing policy recommends listing if a sample size of 134 has 12 or more samples that exceed the evaluation criteria. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10179

LOE ID: | 20453
Pollutant: | Specific Conductivity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 134
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 134 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Specific Conductivity.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | The water quality objective used was the California Secondary MCL recommended level of 900 uS/cm. The Basin Plan includes chemical constituent water quality objectives that include (by reference) secondary maximum contaminant levels (MCLs) protective of MUN (CVRWQCB, 2007a).The secondary MCLs for electrical conductivity provide a range of values including a recommended level (900 uS/cm), upper level (1600 uS/cm) and a short-term level (2200 uS/cm). The recommended concentration was used as it is intended to be protective of all drinking water uses.
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Jan 28 1998 to Nov 29 2005
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10180
Pollutant: | Total Dissolved Solids
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 13 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. Table 3.1 of the listing policy recommends listing if a sample size of 13 has 2 or more samples that exceed the evaluation criteria. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10180

LOE ID: | 20452
Pollutant: | Total Dissolved Solids
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 13 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Total Dissolved Solids.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | The water quality objective used was the California Secondary MCL recommended level of 500 mg/L. The Basin Plan includes chemical constituent water quality objectives that include (by reference) secondary maximum contaminant levels (MCLs) protective of MUN (CVRWQCB, 2007a).The secondary MCLs for TDS provide a range of values including a recommended level (500 mg/L), upper level (1000 mg/L) and a short-term level (1500 mg/L). The recommended concentration was used as it is intended to be protective of all drinking water uses.
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Jun 24 1998 to Nov 28 2001
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10181
Pollutant: | Zinc
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 21 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 15 available concentrations exceeded the Department of Public Health Secondary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10181

LOE ID: | 20807
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | 0 of the 15 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Zinc.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Zinc levels should not exceed 5000 ug/L (Department of Public Health Secondary MCL)
Guideline Reference: | Compilation of Water Quality Goals - 2007 for toxicity data
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Apr 27 2000 to Jun 30 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 6357
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 21
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Asses Water Quality: | 0 of the 21 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Zinc.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Dissolved Zinc levels should not exceed the calculated limit based on the formula: Criteria Maximum Concentration=EXP((0.8473*LN(hardness))+0.884)*(0.978) (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals - 2007 for toxicity data
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Merced River at River Road.
Temporal Representation: | The samples were collected from Apr 27 2000 to Jun 30 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 13807
Pollutant: | pH
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. Four of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Four of 121 samples exceeded the pH objective and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 13807

LOE ID: | 22225
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 20
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | The East San Joaquin Water Quality Coalition collected 20 samples from July 2004 to September 2006. One out of 20 samples was outside the acceptable range; the sample was lower than the acceptable range.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | The pH of water shall not be depressed below 6.5,raised above 8.5, or changed at any time more than 0.5 units from normal ambient pH.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Measurement of pH within the range of 6.5 and 8.5
Guideline Reference:
Spatial Representation: | Samples were collected from Merced River at Santa Fe.
Temporal Representation: | Sampling occurred from July 2004 to September 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 22226
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 101
Number of Exceedances: | 3
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | The Central Valley Regional Water Quality Control Board Surface Water Ambient Monitoring Program collected 101 samples from January 1998 to November 2005. Three out of 101 samples were outside the acceptable range; all three samples were higher than the acceptable range.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | The pH of water shall not be depressed below 6.5,raised above 8.5, or changed at any time more than 0.5 units from normal ambient pH.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Measurement of pH within the range of 6.5 and 8.5
Guideline Reference:
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Sampling occurred from January 1998 to November 2005.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)

DECISION ID | 13836
Pollutant: | Escherichia coli (E. Coli)
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. Seven of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Seven of 34 samples exceed the E. Coli objective and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 13836

LOE ID: | 22231
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 22
Number of Exceedances: | 6
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | The Central Valley Regional Water Quality Control Board Surface Water Ambient Monitoring Program collected 72 samples from January 2003 to January 2004. Six out of 22 samples exceeded the evaluation objective.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. The objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | The USEPA E. Coli objective of 235/100 mL in any single sample (USEPA 1986).
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Samples were collected at four locations: Merced River at Highway 49, Merced River at Merced Falls, Merced River at Highway 99, and Merced River at River Road.
Temporal Representation: | Sampling occurred from January 2003 to March 2004.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
LOE ID: | 22230
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 12
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | The East San Joaquin Water Quality Coalition collected 12 samples from July 2004 to March 2006. One out of the 12 samples collected exceeded the evaluation objective.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. The objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | The USEPA E. Coli objective of 235/100 mL in any single sample (USEPA 1986).
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Samples were collected at Merced River at Sante Fe.
Temporal Representation: | Sampling occurred July 2004 to March 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):

DECISION ID | 15209
Pollutant: | Temperature, water
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy (Policy). Six lines of evidence are available in the administrative record to assess this pollutant. These are temperature data on five life stages for anadromous fish and information on the historical and current state of the fishery. A large number of seven-day averages of maximum (7DADM) daily temperatures exceeded the anadromous fish life stage temperature criteria. Based on readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. One hundred seven of 130 yearly maximum 7DADM values calculated from temperature data collected during the adult migration life stage (Julian weeks 36 through 43) from 1991 to 2007 exceeded the narrative temperature objective, and this exceeds the minimum criteria for listing from Table 3.2 of the Policy. 4. Ninety-five of 96 yearly maximum 7DADM values calculated from temperature data collected during the spawning life stage (Julian weeks 40 through 50) from 1991 to 2007 exceeded the narrative temperature objective, and this exceeds the minimum criteria for listing from Table 3.2 of the Policy. 5. One hundred two of 125 yearly maximum 7DADM values calculated from temperature data collected during the smoltification life stage (Julian weeks 11 through 24) from 1992 to 2007 exceeded the narrative temperature objective, and this exceeds the minimum criteria for listing from Table 3.2 of the Policy. 6. One hundred two of 125 yearly maximum 7DADM values calculated from temperature data collected during the juvenile rearing life stage (Julian weeks 11 through 24) from 1992 to 2007 exceeded the narrative temperature objective, and this exceeds the minimum criteria for listing from Table 3.2 of the Policy. 7. Thiry-one of 47 yearly maximum 7DADM values calculated from temperature data collected during the steelhead summer rearing life stage (Julian weeks 24 through 47) from 1992 to 2007 exceeded the narrative temperature objective, and this exceeds the minimum criteria for listing from Table 3.2 of the Policy. 8. Pursuant to section 3.11 of the Policy, no additional data and information are available indicating that standards are not met. 9. The data used satisfies the data quality requirements of section 6.1.4.5.7 of the Policy.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB-CVR staff concludes that the water body pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15209

LOE ID: | 26541
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Not Specified
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Fish Migration
Number of Samples: | 0
Number of Exceedances: | 0
Data and Information Type: | QUALITATIVE (EVALUATED) ASSESSMENT - UNSPECIFIED
Data Used to Asses Water Quality: | Historically, spring-run and fall-run salmon and steelhead occurred in the Merced River. The spawning beds extended from the mouth of the river to Exchequer Dam, about 12 miles (G.H. Clark, 1929). Today, only the fall-run has survived. In 1852, Native Americans were observed harvesting salmon at Merced Falls. In November 1877, John Muir noted that salmon were abundant in deep pools. Unconfirmed reports suggest that both salmon and steelhead migrated as far up the South Fork as Wawona and in the mainstem as far as into Yosemite Valley. Reports from early residents along the river speak of high populations of fish coming up the river to spawn in the summer and fall. In 1920, the Fish and Game Commission received a letter from a resident stating that there were fifty salmon in the past for each one now (1920). In 1928, a statement from Fish and Game said there were several hundred salmon in the fall. In 1961, the fall-run was described as poor. Estimates averaged about 250 salmon per year. By the end of the six year drought, 1986-1992, escapement populations drastically declined believed to be attributed to low flow and elevated water temperatures during adult immigation and juvenile (smolt) spring-out migration from the Merced River. Between 1993 and 1998, salmon escapement improved when flow and water temperature improved. However, with the higher spring flows and cooler spring water of 1998 and 1999, the population has steadily declined since 2000. In 2000, fall-run salmon escapement numbers (over 13,000 spawners) have dramatically declined to only 2,000 spawners in 2006, a drop of about 84% below the year 2000 peak abundance. There is a strong correlation between annual spring flow magnitude and future year adult production (Mesick and Marston 2007). As spring flow increases, smolt survival increases (CDFG Annual Reports). However, as temperatures begin to rise while salmon smolts out migrate, juveniles are still trying to migrate from the upper reach of the Merced River to the lower reaches of the Merced River, harming both critical life stages (Merced Irrigation District 1999-2005). In addition to warm spring temperatures, the Department of Fish and Game submitted data to the Regional Water Quality Control Board regarding warm water temperatures present in the lower Merced River during the fall adult upstream migration season for the years 1998 thru 2005 (Tables 9 and 10 in CDFGs Letter to the RWQCB, 2007). Also, the Department of Fish and Game submitted data regarding warm water temperatures present in the lower Merced River spawning habitat reaches during the first half of the spawning season for years 1998 thru 2005 (Table 13 in CDFGs Letter to the RWQCB, 2007). Steelhead in the Merced River are listed winter run. Juvenile rainbow trout have been caught in rotary screw traps out-migrating the Merced River. Anecdotal reports by anglers suggest that steelhead populations are good following years where summer rearing conditions are good (e.g. presence of cold water temperatures). State and Federal agencies believe their abundance trends mirrors those of salmon causing them to be listed as threatened in the Central Valley. The Department of Fish and Game submitted data to the Regional Water Quality Control Board regarding warm water temperatures present in the lower Merced River juvenile steelhead rearing reaches during the summer for years 1999 thru 2005 (Table 20 in CDFGs Letter to the RWQCB, 2007).
Data Reference:
Water Quality Objective/Criterion: | The natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Water Board that such alteration in temperature does not adversely affect beneficial uses. In determining compliance with the water quality objectives for temperature, appropriate averaging periods may be applied provided that beneficial uses will be fully protected. (Central Valley Regional Board Basin Plan, Pg. III-8.00, Water Quality Objectives)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | In the absence of necessary data to interpret numeric water quality objectives, recent temperature monitoring data shall be compared to the temperature requirements of aquatic life in the water segment. In many cases, fisheries, particularly salmonids, represent the beneficial uses most sensitive to temperature. Information on current and historic conditions and distribution of sensitive beneficial uses (e.g., fishery resources) in the water segment is necessary, as well as recent temperature data reflective of conditions experienced by the most sensitive life stage of the aquatic life species. If temperature data from past (historic) periods corresponding to times when the beneficial use was fully supported are not available, information about presence/absence or abundance of sensitive aquatic life species shall be used to infer past (historic) temperature conditions if loss of habitat, diversions, toxic spills, and other factors are also listed. (SWRCB, 2004)
Guideline Reference:
Spatial Representation: | Merced River
Temporal Representation: | Information references from year 1929 to 2006.
Environmental Conditions: |
QAPP Information: | San Joaquin River Fall-Run Chinook Salmon and Steelhead Rainbow Trout Historical Population Trend Summary. Dean Marston. September 2007.
QAPP Information Reference(s):
LOE ID: | 26540
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Not Specified
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 47
Number of Exceedances: | 31
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Stream temperatures were measured by CDFG using data loggers (Stowaways, Tidbits and Hobo Temp Pros). Monitoring occurred from 1992 to 2007 depending on the monitoring station, identified by a river mile. The 7DADM was recorded weekly for each river mile. The maximum 7DADM value was calculated for each year. Based on the data provided, 31 out of 47 maximum 7DADM values exceeded the <18°C criteria from 1992 to 2007.
Data Reference: | Cover letter, data and information regarding elevated water temperatures in the San Joaquin, Merced, Stanislaus, and Tuolumne rivers
| Access and DSS database files of water temperature data, one each for the San Joaquin, Merced, Stanislaus, and Tuolumne rivers
Water Quality Objective/Criterion: | The natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Water Board that such alteration in temperature does not adversely affect beneficial uses. In determining compliance with the water quality objectives for temperature, appropriate averaging periods may be applied provided that beneficial uses will be fully protected. (Central Valley Regional Board Basin Plan, Pg. III-8.00, Water Quality Objectives)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | The guideline used was the 2003 US EPA Region 10 Guidance for Pacific Northwest State and Tribal Temperature Water Quality Standards (USEPA, 2003). The document includes recommended temperature criteria for salmon and trout based on different life stages. The recommended temperature for steelhead summer rearing is <18°C for a 7DADM. The steelhead summer rearing life stage occurs from river mile 42 (Hwy 59 Bridge) to river mile 52 (Merced River Hatchery). This life stage occurs during Julian weeks 24 through 37, which is approximately June 15th through September 15th.
Guideline Reference: | EPA Region 10 Guidance for Pacific Northwest State and Tribal Temperature Water Quality Standards. EPA 910-B-03-002. U.S. Environmental Protection Agency Region 10 Office of Water, Seattle, WA.
Spatial Representation: | The steelhead summer rearing life stage occurs from river mile 42 (Hwy 59 Bridge) to river mile 52 (Merced River Hatchery). Stream temperatures were monitored at the following stream locations during the steelhead summer rearing life stage: River Miles 42 (Hwy 59 Bridge), 43 (Robinson), 44 (upper Robinson), 46 (G Street Bridge), 47 (NRS), and 52 (Merced River Hatchery).
Temporal Representation: | The steelhead summer rearing life stage occurs during Julian weeks 24 through 37, which is approximately June 15th through September 15th. Data was collected during this life stage on a continuous basis (hourly intervals) from 1992 through 2007, depending on the station and year monitored. Refer to the CDFG 2007 report (Gordus, 2007) for specific years for each location.
Environmental Conditions: |
QAPP Information: | Data is supported by a Quality Assurance Project Plan (QAPP) pursuant to the requirements of 40 CFR 31.45 and are acceptable for use in developing the section 303(d) list.
QAPP Information Reference(s):
LOE ID: | 26539
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Not Specified
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 125
Number of Exceedances: | 102
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Stream temperatures were measured by CDFG using data loggers (Stowaways, Tidbits and Hobo Temp Pros). Monitoring occurred from 1992 to 2007 depending on the monitoring station, identified by a river mile. The 7DADM was recorded weekly for each river mile. The maximum 7DADM value was calculated for each year. Based on the data provided, 102 out of 125 maximum 7DADM values exceeded the <16°C criteria from 1992 to 2007.
Data Reference: | Cover letter, data and information regarding elevated water temperatures in the San Joaquin, Merced, Stanislaus, and Tuolumne rivers
| Access and DSS database files of water temperature data, one each for the San Joaquin, Merced, Stanislaus, and Tuolumne rivers
Water Quality Objective/Criterion: | The natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Water Board that such alteration in temperature does not adversely affect beneficial uses. In determining compliance with the water quality objectives for temperature, appropriate averaging periods may be applied provided that beneficial uses will be fully protected. (Central Valley Regional Board Basin Plan, Pg. III-8.00, Water Quality Objectives)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | The guideline used was the 2003 US EPA Region 10 Guidance for Pacific Northwest State and Tribal Temperature Water Quality Standards (USEPA, 2003). The document includes recommended temperature criteria for salmon and trout based on different life stages. The recommended temperature for salmon and trout juvenile rearing is <16°C for a 7DADM. The juvenile rearing life stage occurs from river mile 52 (Merced River Hatchery) to river mile 0 (confluence with the San Joaquin River). This life stage occurs during Julian weeks 11 to 24, which is approximately March 15th through June 15th.
Guideline Reference: | EPA Region 10 Guidance for Pacific Northwest State and Tribal Temperature Water Quality Standards. EPA 910-B-03-002. U.S. Environmental Protection Agency Region 10 Office of Water, Seattle, WA.
Spatial Representation: | The juvenile rearing life stage occurs from river mile 52 (Merced River Hatchery) to river mile 0 (confluence with the San Joaquin River). Stream temperatures were monitored at the following stream locations during the juvenile rearing life stage: River Miles 0 (confluence with the San Joaquin River), 1 (Hatfield Park), 4 (below and above Stevinson Spill), 12 (NRS), 13 (Haggaman Park), 21 (above Livingston Spill), 22 (Hwy 99 Bridge), 28 (near Santa Fe Bridge), 30.5 (Dry Creek above Merced River), 31 (Shaffer Bridge), 39 (Gallo Ranch Bridge), 40 (on the Ratzlaff property), 41 (Hwy 59 Bridge), 42 (Hwy 59 Bridge), 43 (Robinson), 44 (upper Robinson), 46 (G Street Bridge), 47 (NRS), and 52 (Merced River Hatchery).
Temporal Representation: | The juvenile rearing life stage occurs during Julian weeks 11 to 24, which is approximately March 15th through June 15th. Data was collected during this life stage on a continuous basis (hourly intervals) from 1992 through 2007, depending on the station and year monitored. Refer to the CDFG 2007 report (Gordus, 2007) for specific years for each location.
Environmental Conditions: |
QAPP Information: | Data is supported by a Quality Assurance Project Plan (QAPP) pursuant to the requirements of 40 CFR 31.45 and are acceptable for use in developing the section 303(d) list.
QAPP Information Reference(s):
LOE ID: | 26233
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Not Specified
Fraction: | None
Beneficial Use: | Fish Migration
Number of Samples: | 130
Number of Exceedances: | 107
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Stream temperatures were measured by California Department of Fish and Game (CDFG) using data loggers (Stowaways, Tidbits and Hobo Temp Pros). Monitoring occurred from 1991 to 2007 depending on the monitoring station, identified by a river mile. The 7DADM was recorded weekly for each river mile. The maximum 7DADM value was calculated for each year. Based on the data provided, 107 out of 130 maximum 7DADM values exceeded the <18oC criteria from 1991 to 2007.
Data Reference: | Cover letter, data and information regarding elevated water temperatures in the San Joaquin, Merced, Stanislaus, and Tuolumne rivers
| Access and DSS database files of water temperature data, one each for the San Joaquin, Merced, Stanislaus, and Tuolumne rivers
Water Quality Objective/Criterion: | The natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Water Board that such alteration in temperature does not adversely affect beneficial uses. In determining compliance with the water quality objectives for temperature, appropriate averaging periods may be applied provided that beneficial uses will be fully protected. (Central Valley Regional Board Basin Plan, Pg. III-8.00, Water Quality Objectives)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | The guideline used was the 2003 US EPA Region 10 Guidance for Pacific Northwest State and Tribal Temperature Water Quality Standards (USEPA, 2003). The document includes recommended temperature criteria for salmon and trout based on different life stages. The recommended temperature for salmon and trout adult migration is <18oC for a 7DADM. The adult migration life stage occurs from river mile 0 (confluence with the San Joaquin River) to river mile 52 (Merced River Hatchery). This life stage occurs during Julian weeks 36 through 43, which is approximately September 1st through October 31st.
Guideline Reference: | EPA Region 10 Guidance for Pacific Northwest State and Tribal Temperature Water Quality Standards. EPA 910-B-03-002. U.S. Environmental Protection Agency Region 10 Office of Water, Seattle, WA.
Spatial Representation: | The adult migration life stage occurs from river mile 0 (confluence with the San Joaquin River) to river mile 52 (Merced River Hatchery). Stream temperatures were monitored at the following stream locations during the adult migration life stage: River Miles 0 (confluence with the San Joaquin River), 1 (Hatfield Park), 4 (above and below Stevinson Spill), 12 (NRS), 13 (Haggaman Park), 21 (above Livingston Spill), 22 (Hwy 99 Bridge), 28 (near Santa Fe Bridge), 30.5 (Dry Creek), 31 (Shaffer Bridge), 39 (Gallo Ranch Bridge), 40 (on the Ratzlaff property), 41 (Hwy 59 Bridge), 42 (NRS), 43 (Robinson), 44 (upper Robinson), 46 (G Street Bridge), 47 (NRS) and 52 (Merced River Hatchery).
Temporal Representation: | The adult migration life stage occurs during Julian weeks 36 through 43, which is approximately September 1st through October 31st. Data was collected during this life stage on a continuous basis (hourly intervals) from 1991 through 2007, depending on the station and year monitored. Refer to the CDFG 2007 report (Gordus, 2007) for specific years for each location.
Environmental Conditions: |
QAPP Information: | Data is supported by a Quality Assurance Project Plan (QAPP) pursuant to the requirements of 40 CFR 31.45 and are acceptable for use in developing the section 303(d) list.
QAPP Information Reference(s):
LOE ID: | 26538
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Not Specified
Fraction: | None
Beneficial Use: | Fish Migration
Number of Samples: | 125
Number of Exceedances: | 102
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Stream temperatures were measured by CDFG using data loggers (Stowaways, Tidbits and Hobo Temp Pros). Monitoring occurred from 1992 to 2007 depending on the monitoring station, identified by a river mile. The 7DADM was recorded weekly for each river mile. The maximum 7DADM value was calculated for each year. Based on the data provided, 102 out of 125 maximum 7DADM values exceeded the <16°C criteria from 1992 to 2007.
Data Reference: | Cover letter, data and information regarding elevated water temperatures in the San Joaquin, Merced, Stanislaus, and Tuolumne rivers
| Access and DSS database files of water temperature data, one each for the San Joaquin, Merced, Stanislaus, and Tuolumne rivers
Water Quality Objective/Criterion: | The natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Water Board that such alteration in temperature does not adversely affect beneficial uses. In determining compliance with the water quality objectives for temperature, appropriate averaging periods may be applied provided that beneficial uses will be fully protected. (Central Valley Regional Board Basin Plan, Pg. III-8.00, Water Quality Objectives)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | The guideline used was the 2003 US EPA Region 10 Guidance for Pacific Northwest State and Tribal Temperature Water Quality Standards (USEPA, 2003). The document includes recommended temperature criteria for salmon and trout based on different life stages. The recommended temperature for salmon and trout smoltification is <16°C for a 7DADM. The smoltification life stage occurs from river mile 52 (Merced River Hatchery) to river mile 0 (confluence with the San Joaquin River). This life stage occurs during Julian weeks 11 to 24, which is approximately March 15th through June 15th.
Guideline Reference: | EPA Region 10 Guidance for Pacific Northwest State and Tribal Temperature Water Quality Standards. EPA 910-B-03-002. U.S. Environmental Protection Agency Region 10 Office of Water, Seattle, WA.
Spatial Representation: | The smoltification life stage occurs from river mile 52 (Merced River Hatchery) to river mile 0 (confluence with the San Joaquin River). Stream temperatures were monitored at the following stream locations during the smoltification life stage: River Miles 0 (confluence with the San Joaquin River), 1 (Hatfield Park), 4 (below and above Stevinson Spill), 12 (NRS), 13 (Haggaman Park), 21 (above Livingston Spill), 22 (Hwy 99 Bridge), 28 (near Santa Fe Bridge), 30.5 (Dry Creek above Merced River), 31, (Shaffer Bridge), 39 (Gallo Ranch Bridge), 40 (on the Ratzlaff property), 41 (Hwy 59 Bridge), 42 (Hwy 59 Bridge), 43 (Robinson), 44 (upper Robinson), 46 (G Street Bridge), 47 (NRS), and 52 (Merced River Hatchery).
Temporal Representation: | The smoltification life stage occurs during Julian weeks 11 to 24, which is approximately March 15th through June 15th. Data was collected during this life stage on a continuous basis (hourly intervals) from 1992 through 2007, depending on the station and year monitored. Refer to the CDFG 2007 report (Gordus, 2007) for specific years for each location.
Environmental Conditions: |
QAPP Information: | Data is supported by a Quality Assurance Project Plan (QAPP) pursuant to the requirements of 40 CFR 31.45 and are acceptable for use in developing the section 303(d) list.
QAPP Information Reference(s):
LOE ID: | 26537
Pollutant: | Temperature, water
LOE Subgroup: | Pollutant-Water
Matrix: | Not Specified
Fraction: | None
Beneficial Use: | Fish Spawning
Number of Samples: | 96
Number of Exceedances: | 95
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Asses Water Quality: | Stream temperatures were measured by CDFG using data loggers (Stowaways, Tidbits and Hobo Temp Pros). Monitoring occurred from 1991 to 2007 depending on the monitoring station, identified by a river mile. The 7DADM was recorded weekly for each river mile. The maximum 7DADM value was calculated for each year. Based on the data provided, 95 out of 96 maximum 7DADM values exceeded the <13°C criteria from 1991 to 2007.
Data Reference: | Cover letter, data and information regarding elevated water temperatures in the San Joaquin, Merced, Stanislaus, and Tuolumne rivers
| Access and DSS database files of water temperature data, one each for the San Joaquin, Merced, Stanislaus, and Tuolumne rivers
Water Quality Objective/Criterion: | The natural receiving water temperature of intrastate waters shall not be altered unless it can be demonstrated to the satisfaction of the Regional Water Board that such alteration in temperature does not adversely affect beneficial uses. In determining compliance with the water quality objectives for temperature, appropriate averaging periods may be applied provided that beneficial uses will be fully protected. (Central Valley Regional Board Basin Plan, Pg. III-8.00, Water Quality Objectives)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | The guideline used was the 2003 US EPA Region 10 Guidance for Pacific Northwest State and Tribal Temperature Water Quality Standards (USEPA, 2003). The document includes recommended temperature criteria for salmon and trout based on different life stages. The recommended temperature for salmon and trout spawning is <13°C for a 7DADM. The spawning life stage occurs from river mile 28 (near Santa Fe Bridge) to river mile 52 (Merced River Hatchery). This life stage occurs during Julian weeks 40 through 50, which is approximately October 1st through December 15th.
Guideline Reference: | EPA Region 10 Guidance for Pacific Northwest State and Tribal Temperature Water Quality Standards. EPA 910-B-03-002. U.S. Environmental Protection Agency Region 10 Office of Water, Seattle, WA.
Spatial Representation: | The spawning life stage occurs from river mile 28 (near Santa Fe Bridge) to river mile 52 (Merced River Hatchery). Stream temperatures were monitored at the following stream locations during the spawning life stage: River Miles 28 (near Santa Fe Bridge), 30.5 (Dry Creek above Merced River), 31 (Shaffer Bridge), 39 (Gallo Ranch Bridge), 40 (on the Ratzlaff property), 41 (Hwy 59 Bridge), 42 (NRS), 43 (Robinson), 44 (upper Robinson), 46 (G Street Bridge), 47 (NRS), and 52 (Merced River Hatchery).
Temporal Representation: | The spawning life stage occurs during Julian Weeks 40 through 50, which is approximately October 1st through December 15th. Data was collected during this life stage on a continuous basis (hourly intervals) from 1991 through 2007, depending on the station and year monitored. Refer to the CDFG 2007 report (Gordus, 2007) for specific years for each location.
Environmental Conditions: |
QAPP Information: | Data is supported by a Quality Assurance Project Plan (QAPP) pursuant to the requirements of 40 CFR 31.45 and are acceptable for use in developing the section 303(d) list.
QAPP Information Reference(s):

DECISION ID | 12692
Pollutant: | Unknown Toxicity
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Six lines of evidence are available in the administrative record to assess this pollutant. Nine of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Three of 29 samples tested with ceriodaphnia exceed the narrative toxicity objcective and this exceeds the allowable frequency listed in Table 3.1 of the Listing Policy. In addition, 5 of 11 chronic samples tested with fathead minnow exceed the narrative toxicity objcective and this exceeds the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12692

LOE ID: | 23080
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 11
Number of Exceedances: | 5
Data and Information Type: | TOXICITY TESTING
Data Used to Asses Water Quality: | Five of the 11 samples tested with Pimephales promelas were toxic and violated the narrative toxicity objective. Fiver samples collected at River Road exhibited a statistically significant decrease in survival compared to the control. The sample dates and percent of control (in parentheses) are as follows:29 March 2005 (63)26 May 2005 (67)25 August 2005 (87)27 October 2005 (74)29 November 2005 (44)
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | ¿All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.¿ (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a Fisher¿s Exact test with 7-day chronic-style toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected from November 2004 to November 2005.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
LOE ID: | 23081
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 15
Number of Exceedances: | 1
Data and Information Type: | TOXICITY TESTING
Data Used to Asses Water Quality: | One of 15 samples tested with Selenastrum capricornutum was toxic and violated the narrative toxicity objective. One sample collected at Santa Fe exhibited a statistically significant decrease in growth compared to the control. Sample date and percent of control (in parentheses) are indicated below.21 March 2005 (76)
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | ¿All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.¿ (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 4-day chronic-style toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from Merced River at Santa Fe.
Temporal Representation: | Samples were collected from July 2004 to September 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 23060
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 18
Number of Exceedances: | 3
Data and Information Type: | TOXICITY TESTING
Data Used to Asses Water Quality: | 3 of the 18 samples tested with Ceriodaphnia dubia were toxic and violated the narrative toxicity objective. Three samples collected at Santa Fe Drive exhibited a statistically significant decrease in survival compared to the control. The sample dates and percent of control (in parentheses) are as follows:31 July 2004 (79)31 August 2004 (42)16 March 2006 (35)
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.¿ (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 4-day acute-style toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from Merced River at Sante Fe Drive.
Temporal Representation: | Samples were collected from July 2004 to September 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 23064
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 17
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Asses Water Quality: | None of the 17 samples tested with Pimephales promelas were toxic and violated the narrative toxicity objective.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | ¿All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.¿ (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 4-day acute-style toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from Merced River at Santa Fe.
Temporal Representation: | Samples were collected from July 2004 to September 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 23061
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 11
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Asses Water Quality: | Zero of the 11 samples tested with Ceriodaphnia dubia were toxic and violated the narrative toxicity objective.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | ¿All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.¿ (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 48-hour acute-style toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected from October 2001 to November 2002.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
LOE ID: | 23065
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 12
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Asses Water Quality: | None of the 12 samples tested with Pimephales promelas were toxic and violated the narrative toxicity objective.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | ¿All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.¿ (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a Fisher¿s Exact test with 4-day acute-style toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from Merced River at River Road.
Temporal Representation: | Samples were collected from October 2000 to November 2002.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)

DECISION ID | 6938
Pollutant: | Exotic Species
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)(2006)
Revision Status | Original
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.10 of the Listing Policy. Under section 3.10 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. Three studies, two in 1969-1971 and one in 1986 were used for this assessment, which showed an overall increase of native and non-native species over time. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. Three studies were conducted, two in 1969-1971 and one in 1986. 2. Baseline data was taken from the 1969-1971 studies. All three studies sampled the same geographic area, with similar sampling sizes. 3. Rank abundance, Pearson product moment correlations, and principal components analysis were the statistical analyses employed during these studies. 4. The comparison showed a net increase of native and non-native species observed at all sampling sites. The data was based on the percentage of sites the species were collected at for each study. 5. Some native species were collected at more sites in 1986 than in 1969-71. Some non-native species were collected at more sites than in 1969-71. Eight native species increased in the watersheds they were observed from 1969-71 to 1986, while 5 native species decreased. Nine non-native species increased over time from 1969-71 to 1986, while 7 non-native species decreased. 6. It cannot be determined if the trend in water quality is expected to meet water standards by the next listing cycle. 7. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | No new data were assessed for 2008. The Regional Board will update this decision when new data and information become available and are assessed.
SWRCB Board Decision / Staff Recommendation: | This is a decision made by the State Water Resources Control Board and approved by the USEPA in 2006 . No new data were assessed by the Regional Board for 2008. The decision has not changed.
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 6938

LOE ID: | 2754
Pollutant: | Exotic Species
LOE Subgroup: | Population/Community Degradation
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Number of Samples: | 0
Number of Exceedances: | 0
Data and Information Type: | Fish surveys
Data Used to Asses Water Quality: | Two previous studies (conducted in 1969-71) (Moyle and Nichols, 1973; Moyle and Nichols, 1974) were used as baseline comparisons to a study conducted in 1986 (Brown and Moyle, 1993). Species percent collection data were the same for each baseline study at the sampling sites. The baseline studies and this study sampled the same geographic area, with similar sampling sizes. The baseline data was compared to the data collected in 1986. The comparison showed an overall net increase of native species observed at all sampling sites, as well as a net increase in non-native species. The data was based on the percentage of sites the species were collected at for each study. Overall, some native species were collected at more sites in 1986 (an increase in percent) than in the 1969-71 studies (Brown and Moyle, 1993). Some non-native species were collected at more sites (an increase in percent) than in the 1969-71 studies. Eight native species increased in the watersheds they were observed (collected at more sites over time) from 1969-71 to 1986, while 5 native species decreased (collected at less sites over time). Nine non-native species increased over time (collected at more sites over time) from 1969-71 to 1986, while 7 non-native species decreased (collected at less sites over time).
Data Reference: | Placeholder reference 2006 303(d)
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. Compliance with this objective will be determined by analyses of indicator organisms, species diversity, population density, growth anomalies, and biotoxicity tests of appropriate duration or other methods as specified by the Regional Water Board. Taken from Region 5 Basin Plan, Page III-8.00, Water Quality Objectives.
Objective/Criterion Reference: | Placeholder reference 2006 303(d)
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Stanislaus, Tuolumne, Merced, Chowchilla, Fresno, San Joaquin, Kings, Kaweah, and Tule Rivers, between 90 and 1100 meters elevation.
Temporal Representation: | Baseline studies: 37 samples taken during the summer and autumn of 1969, 1970 and 1971 and 130 samples were taken from 7/27-9/4/1970. Another survey was conducted from Sept. 1985 to Sept. 1986 at 186 sites. Only 156 sites were used from this study for statistical analyses, (Brown and Moyle, 1993).
Environmental Conditions: | Changes in relative diversity and abundance of native species may also be driven by habitat alteration, flow changes, or hydromodification.
QAPP Information: | Peer Reviewed Journal Articles.
QAPP Information Reference(s):

DECISION ID | 7423
Pollutant: | Group A Pesticides
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | List on 303(d) list (TMDL required list)(2006)
Revision Status | Original
Sources: | Agriculture
Expected TMDL Completion Date: | 2011
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | 303(d) listing decisions made prior to 2006 were not held in an assessment database. The Regional Boards will update this decision when new data and information become available and are assessed.
RWQCB Board Decision / Staff Recommendation: | No new data were assessed for 2008. The decision has not changed.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 7423

LOE ID: | 4478
Pollutant: | Group A Pesticides
LOE Subgroup: | Pollutant-Tissue
Matrix: | Tissue
Fraction: | Not Recorded
Beneficial Use: | Commercial or recreational collection of fish, shellfish, or organisms
Number of Samples: | 0
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Asses Water Quality: | Unspecified--This LOE is a placeholder to support a 303(d) listing decision made prior to 2006.
Data Reference: | Placeholder reference pre-2006 303(d)
Water Quality Objective/Criterion: | Unspecified
Objective/Criterion Reference: | Placeholder reference pre-2006 303(d)
Evaluation Guideline: | Unspecified
Guideline Reference: | Placeholder reference pre-2006 303(d)
Spatial Representation: | Unspecified
Temporal Representation: | Unspecified
Environmental Conditions: | Unspecified
QAPP Information: | Unspecified
QAPP Information Reference(s):

DECISION ID | 6818
Pollutant: | Mercury
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | List on 303(d) list (TMDL required list)(2006)
Revision Status | Original
Sources: | Resource Extraction
Expected TMDL Completion Date: | 2019
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.5 of the Listing Policy. One line of evidence is available in the administrative record to assess this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Two of the 2 samples exceeded the OEHHA Screening Value and this exceeds the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | No new data were assessed for 2008. The Regional Board will update this decision when new data and information become available and are assessed.
SWRCB Board Decision / Staff Recommendation: | This is a decision made by the State Water Resources Control Board and approved by the USEPA in 2006 . No new data were assessed by the Regional Board for 2008. The decision has not changed.
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 6818

LOE ID: | 2753
Pollutant: | Mercury
LOE Subgroup: | Pollutant-Tissue
Matrix: | Tissue
Fraction: | Total
Beneficial Use: | Commercial or recreational collection of fish, shellfish, or organisms
Number of Samples: | 2
Number of Exceedances: | 2
Data and Information Type: | Fish tissue analysis
Data Used to Asses Water Quality: | Two out of 2 samples exceeded. Two filet composite samples were collected in 1998. One sample each of largemouth bass and one of channel catfish. Both samples exceeded the guideline (TSMP, 2002).
Data Reference: | Placeholder reference 2006 303(d)
Water Quality Objective/Criterion: | Central Valley RWQCB Basin Plan: All waters shall be maintained free of toxic substances in concentrations that are toxic to, or produce detrimental physiological responses in human, plant, animal, or aquatic life.
Objective/Criterion Reference: | Placeholder reference 2006 303(d)
Evaluation Guideline: | OEHHA Screening Value of 0.3 ug/g for mercury (Brodberg & Pollock, 1999).
Guideline Reference: | Placeholder reference 2006 303(d)
Spatial Representation: | One station located at George J. Hatfield State Recreation Area.
Temporal Representation: | Samples were collected on 11/5/98.
Environmental Conditions: |
QAPP Information: | Environmental Chemistry Quality Assurance and Data Report for the Toxic Substances Monitoring Program, 1996-2000. Department of Fish and Game.
QAPP Information Reference(s):