# Draft 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 5 - Central Valley Region

Water Body Name: | Hangtown Creek (El Dorado County)
Water Body ID: | CAR5143102120081114001020
Water Body Type: | River & Stream

DECISION ID | 12594
Pollutant: | Specific Conductivity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 1 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.2 of the Listing Policy. Table 3.2 of the listing policy recommends listing if a minimum sample size of 5 has 5 or more samples that exceed the evaluation criteria.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12594

LOE ID: | 25404
Pollutant: | Specific Conductivity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 1 sample collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Specific Conductivity.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | The water quality objective used was the California Secondary MCL recommended level of 900 uS/cm. The Basin Plan includes chemical constituent water quality objectives that include (by reference) secondary maximum contaminant levels (MCLs) protective of
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | The sample was collected at Hangman Creek @ Main Street.
Temporal Representation: | The sample was collected on Sep 27 2006
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 12599
Pollutant: | pH
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that only 1 sample is available and a minimum of 5 is needed for evaluation under section 3.2.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12599

LOE ID: | 25403
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 1 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for pH.
Data Reference: | SWAMP data entered by SWRCB into BDAT database
Water Quality Objective/Criterion: | pH levels should not be lower than 6.5 or higher than 8.5 (Basin Plan Objective)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Hangman Creek @ Main Street.
Temporal Representation: | The samples were collected from Sep 27 2006 to Sep 27 2006
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):