# Draft 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 5 - Central Valley Region

Water Body Name: | Littlejohns Creek
Water Body ID: | CAR5314000020070511145114
Water Body Type: | River & Stream

DECISION ID | 9653
Pollutant: | Arsenic
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 9 available concentrations exceeded the USEPA Primary MCL and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is based on staff findings that 0 of 9 available concentrations exceeded the California Toxics Rule and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9653

LOE ID: | 21141
Pollutant: | Arsenic
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 9
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 9 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Arsenic.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Eastside Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Arsenic levels should not exceed 340 ug/L maximum concentration for 1-hour average (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Compilation of Water Quality Goals
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Littlejohns Creek at Austin Road. Samples were collected at Littlejohn's Creek at Sonora Road.
Temporal Representation: | The samples were collected from Mar 18 2003 to Jun 30 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 20951
Pollutant: | Arsenic
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 9
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 9 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Arsenic.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Eastside Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Arsenic levels should not exceed 10 ug/L (USEPA Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Littlejohns Creek at Austin Road. Samples were collected at Littlejohn's Creek at Sonora Road.
Temporal Representation: | The samples were collected from Mar 18 2003 to Jun 30 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 9654
Pollutant: | Boron
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 9 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. Table 3.1 of the listing policy recommends listing if a sample size of 9 has 2 or more samples that exceed the evaluation criteria. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9654

LOE ID: | 20952
Pollutant: | Boron
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 9
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 9 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Boron.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Eastside Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Boron levels should not exceed 1000 ug/L (Department of Health Services Health Advisory)
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Littlejohns Creek at Austin Road. Samples were collected at Littlejohn's Creek at Sonora Road.
Temporal Representation: | The samples were collected from Mar 18 2003 to Jun 30 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 9656
Pollutant: | Chloride
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 8 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. Table 3.1 of the listing policy recommends listing if a sample size of 8 has 2 or more samples that exceed the evaluation criteria. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9656

LOE ID: | 21132
Pollutant: | Chloride
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 8
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 8 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Chloride.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Eastside Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Chloride levels should not exceed 250 mg/L (USEPA Maximum Contaminant Level)
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Littlejohns Creek at Austin Road. Samples were collected at Littlejohn's Creek at Sonora Road.
Temporal Representation: | The samples were collected from Mar 18 2003 to Jun 30 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 14181
Pollutant: | Chlorpyrifos
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess this pollutant. One of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. One of 13 available 4-day average concentrations exceeded the 4-day average maximum concentration criterion and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. In addition, 1 of 13 available 1-hour average concentrations exceeded the 1-hour average concentration criterion and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. Three samples had concentrations less than quantitation limits and the quantitation limits are greater than the water quality criteria concentrations. Therefore the results for these samples were not used in this analysis in accordance with section 6.1.5.5 of the Listing Policy 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 14181

LOE ID: | 22133
Pollutant: | Chlorpyrifos
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Sixteen water samples were collected from Littlejohns Creek from August 2004 through September 2006, representing thirteen 4-day average concentrations and thirteen 1-hour average concentrations. One of the thirteen 4-day average concentrations exceeded the 4-day maximum concentration guideline of 0.015 ug/L. One of the thirteen 1-hour average concentrations exceeded the maximum 1-hour concentration of 0.025 ug/L. Two water samples had method detection limits (0.0254) higher than the CDFG Hazard Assessment Criteria (0.015 ug/L) and 1 sample had a 'not quantified' value. Therefore, the 3 samples were not included in this analysis.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007). All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
| Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | California Department of Fish and Game (CDFG) Hazard Assessment Criteria - 0.015 ug/L 4-day average and 0.025 ug/L 1-hour average (Siepmann and Finlayson, 2000, with minor corrections to significant figures as described in Beaulaurier et al., 2005).
Guideline Reference: | Water quality criteria for diazinon and chlorpyrifos. Administrative Report 00-3. Rancho Cordova, CA: Pesticide Investigations Unit, Office of Spills and Response. CA Department of Fish and Game
Spatial Representation: | Samples were collected from Littlejohns Creek at Jack Tone Road.
Temporal Representation: | Samples were collected at monthly interval from August 2004 through September 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):

DECISION ID | 9657
Pollutant: | Chromium (total)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 9 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. Table 3.1 of the listing policy recommends listing if a sample size of 9 has 2 or more samples that exceed the evaluation criteria. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9657

LOE ID: | 21143
Pollutant: | Chromium (total)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 9
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 9 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Chromium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Eastside Basin
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Chromium levels should not exceed 50 ug/L (Department of Public Health Primary MCL)
Guideline Reference: | Compilation of Water Quality Goals
Spatial Representation: | Samples were collected at Littlejohns Creek at Austin Road. Samples were collected at Littlejohn's Creek at Sonora Road.
Temporal Representation: | The samples were collected from Mar 18 2003 to Jun 30 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 14185
Pollutant: | Diuron
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. One of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. One of 7 samples exceeded the narrative toxicity objective and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 14185

LOE ID: | 22392
Pollutant: | Diuron
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 2
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Four water samples were collected at Littlejohns Creek during two storms. For samples that were collected within less than a 96-hour period of time, the mean was taken of the samples and compared to the maximum concentration (EC50) for diuron.1 of 2 concentrations exceeded the maximum concentration of 1.3 ug/L.
Data Reference: | Zipped file of Central Valley Waterways Pesticide TMDL monitoring data spreadsheets and reports
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007).All waters shall be maintained free of toxic substances that in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | The Board will use the best available technical information to evaluate compliance with the narrative objectives. Other available technical information on the pesticide (such as Lowest Observed Effect Concentrations and No Observed Effect Levels), the water bodies and organisms involved will be evaluated to determine if lower concentrations are required to meet the narrative objectives (CRWQCB, 2006). The 96 hour EC50 for the most sensitive species is 1.3 ug/L (ECOTOX, 2008).
Guideline Reference: | Ecotox database, http://cfpub.epa.gov/ecotox/
Spatial Representation: | Samples collected from Littlejohns Creek at Jack Tone Road.
Temporal Representation: | Samples were collected daily for two days during two storms on January 14 and15, 2006, and on February 28 and March 1, 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Calanchini, H. 2006. Quality Assurance Project Plan, Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. John Muir Institute of the Environment, U.C. Davis. Davis, CA.
QAPP Information Reference(s): | Quality Assurance Project Plan. Sacramento and San Joaquin River Basins and Sacramento-San Joaquin Delta TMDL Monitoring for Organophosphorus Pesticides and Other Pesticides Identified as Posing a High Risk to Surface Waters. Final. SWAMP Project ID 02TM5001 (Revision 0.0). John Muir Institute of the Environment, U.C. Davis. Davis, CA. January 26, 2006
LOE ID: | 22393
Pollutant: | Diuron
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 5
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Five water samples were collected monthly at Littlejohns Creek from May through September 2006. Zero of 5 concentrations exceeded the maximum concentration of 1.3 ug/L.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | No individual pesticide or combination of pesticides shall be present in concentrations that adversely affect beneficial uses (CVRWQCB, 2007). All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | The Board will use the best available technical information to evaluate compliance with the narrative objectives. Other available technical information on the pesticide (such as Lowest Observed Effect Concentrations and No Observed Effect Levels), the water bodies and organisms involved will be evaluated to determine if lower concentrations are required to meet the narrative objectives (CRWQCB, 2006). The 96-hour EC50 for the most sensitive species is 1.3 ug/L (ECOTOX, 2008).
Guideline Reference: | Ecotox database, http://cfpub.epa.gov/ecotox/
Spatial Representation: | Samples collected from Littlejohns Creek at Jack Tone Road.
Temporal Representation: | Samples were collected monthly from May through September 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):

DECISION ID | 14187
Pollutant: | Oxygen, Dissolved
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess this pollutant. One of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. One of 33 samples fell below the minimum criterion water quality objective listed in the Sacramento/San Joaquin River Basin Plan and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 14187

LOE ID: | 22124
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Fifteen samples were taken from Littlejohns Creek between 2003 and 2004. None of the fifteen samples fell below the Water Quality Objective for minimum dissolved oxygen content in surface water.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | From the Sacramento/San Joaquin River Basin Plan the (WARM) Warm Freshwater Habitat criterion is a Minimum Dissolved Oxygen content of 5mg/L.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Littlejohns Creek at Austin Road in San Joaquin County.
Temporal Representation: | Samples were collected between March 2003 and March 2004. Samples were collected at bi-monthly and monthly intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
LOE ID: | 22123
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 18
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Eighteen samples were taken from Littlejohns Creek between 2004 and 2006. One of the eighteen samples fell below the Water Quality Objective for minimum dissolved oxygen content in surface water.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | From the Sacramento/San Joaquin River Basin Plan the (WARM) Warm Freshwater Habitat is a Minimum Dissolved Oxygen content of 5mg/L.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Littlejohns Creek at Jack Tone Road in San Joaquin County.
Temporal Representation: | Samples were collected between August 2004 and September 2006. Samples were collected at bi-monthly and monthly intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):

DECISION ID | 14179
Pollutant: | Salinity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 65 samples exceeded the water quality objectives for electrical conductivity (salinity) and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 14179

LOE ID: | 22119
Pollutant: | Salinity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 25
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Twenty-five samples were taken from Littlejohns Creek between 2004 and 2006. None of the twenty-five samples exceed the California Secondary MCL for electrical conductivity in surface water.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | The water quality objective used was the California Secondary MCL recommended level of 900 uS/cm. The Basin Plan includes chemical constituent water quality objectives that include (by reference) secondary maximum contaminant levels (MCL's) protective of MUN (CVRWQCB, 2007a).The secondary MCL's for electrical conductivity provide a range of values including a recommended level (900 uS/cm), upper level (1600 uS/cm) and a short-term level (2200 uS/cm). The 'recommended' concentration was used as it is intended to be protective of all drinking water uses. Though individual listing evaluations did not look at the water supply source serving the given geographic area, there are certain areas that receive supply waters (such as the Delta Mendota Canal) that at times may be elevated above the recommended level of the secondary MCL. Where future information is made available to document this to be the case, these water bodies may be re-evaluated in future listing cycles.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Littlejohns Creek at Newcastle Road and at Jack Tone Road in San Joaquin County.
Temporal Representation: | Samples were collected between April 2003 and September 2006. Samples were collected at monthly intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 22120
Pollutant: | Salinity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 40
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Forty samples were taken from Littlejohns Creek between 2003 and 2004. None of the forty samples exceed the California Secondary MCL for electrical conductivity in surface water.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | The water quality objective used was the California Secondary MCL recommended level of 900 uS/cm. The Basin Plan includes chemical constituent water quality objectives that include (by reference) secondary maximum contaminant levels (MCLs) protective of MUN (CVRWQCB, 2007a).The secondary MCLs for electrical conductivity provide a range of values including a recommended level (900 uS/cm), upper level (1600 uS/cm) and a short-term level (2200 uS/cm). The recommended concentration was used as it is intended to be protective of all drinking water uses. Though individual listing evaluations did not look at the water supply source serving the given geographic area, there are certain areas that receive supply waters (such as the Delta Mendota Canal) that at times may be elevated above the recommended level of the secondary MCL. Where future information is made available to document this to be the case, these water bodies may be re-evaluated in future listing cycles.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Littlejohns Creek at Austin Road and at Sonora Road, in San Joaquin County.
Temporal Representation: | Samples were collected between February 2003 and March 2006. Samples were collected at monthly intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)

DECISION ID | 14189
Pollutant: | pH (high)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. Three of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Three of 65 samples had pH values higher than the pH objective and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 14189

LOE ID: | 22129
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 39
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | The Central Valley Regional Water Quality Control Board Surface Water Ambient Monitoring Program collected 39 samples from February 2003 to March 2004. Two of the 39 samples had a pH value over 8.5 and did not meet the evaluation objective.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | The pH of water shall not be depressed below 6.5,raised above 8.5, or changed at any time more than 0.5 units from normal ambient pH.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Measurement of pH within the range of 6.5 and 8.5. A high pH value is greater than 8.5.
Guideline Reference:
Spatial Representation: | Samples were collected from Littlejohns Creek at Austin Road and at Sonora Road.
Temporal Representation: | Sampling occurred from February 2003 to March 2004.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
LOE ID: | 22128
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 26
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | The San Joaquin Delta Water Quality Coalition collected 26 samples from April 2003 to September 2006. One sample had a pH higher than 8.5 and did not meet the evaluation objective.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | The pH of water shall not be depressed below 6.5,raised above 8.5, or changed at any time more than 0.5 units from normal ambient pH.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Measurement of pH within the range of 6.5 and 8.5. A high pH value is greater than 8.5.
Guideline Reference:
Spatial Representation: | Samples were collected from Littlejohns Creek at Newcastle Road and at Jack Tone Road.
Temporal Representation: | Sampling occurred from April 2003 to September 2006
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):

DECISION ID | 14190
Pollutant: | pH (low)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. One of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. One of 65 samples had pH values lower than the pH objective and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 14190

LOE ID: | 22131
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 39
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | The Central Valley Regional Water Quality Control Board Surface Water Ambient Monitoring Program collected 39 samples from February 2003 to March 2004. None of the 39 samples had a pH value lower than 6.5 and did not meet the evaluation objective.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | The pH of water shall not be depressed below 6.5,raised above 8.5, or changed at any time more than 0.5 units from normal ambient pH.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Measurement of pH within the range of 6.5 and 8.5. A low pH value is lower than 6.5.
Guideline Reference:
Spatial Representation: | Samples were collected from Littlejohns Creek at Austin Road and at Sonora Road.
Temporal Representation: | Sampling occurred from February 2003 to March 2004.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
LOE ID: | 22130
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 26
Number of Exceedances: | 1
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | The San Joaquin Delta Water Quality Coalition collected 26 samples from April 2003 to September 2006. One sample had a pH lower than 6.5 and did not meet the evaluation objective.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | The pH of water shall not be depressed below 6.5,raised above 8.5, or changed at any time more than 0.5 units from normal ambient pH.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Measurement of pH within the range of 6.5 and 8.5. A low pH value is lower than 6.5.
Guideline Reference:
Spatial Representation: | Samples were collected from Littlejohns Creek at Newcastle Road and at Jack Tone Road.
Temporal Representation: | Sampling occurred from April 2003 to September 2006
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):

DECISION ID | 12780
Pollutant: | Escherichia coli (E. Coli)
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. Twenty-two of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Twenty-two of 56 samples exceed the E. Coli objective and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12780

LOE ID: | 22125
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 16
Number of Exceedances: | 5
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | The San Joaquin Delta Water Quality Coalition collected 16 samples from August 2004 to September 2006. Five out of the 16 samples collected exceeded the evaluation objective.
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. The objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | The USEPA E. Coli objective of 235/100 mL in any single sample (USEPA 1986).
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Samples were collected at Littlejohns Creek at Jack Tone Road.
Temporal Representation: | Sampling occurred from August 2004 to September 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 22126
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 40
Number of Exceedances: | 17
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | The Central Valley Regional Water Quality Control Board Surface Water Ambient Monitoring Program collected 40 samples from March 2003 to March 2004. Seventeen out of 40 samples exceeded the evaluation objective.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. The objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | The USEPA E. Coli objective of 235/100 mL in any single sample (USEPA 1986).
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Samples were collected at two locations: Littlejohns Creek at Austin Road and at Sonora Road.
Temporal Representation: | Sampling occurred from March 2003 to March 2004.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Boards Quality Assurance Program Plan for the State of Californias Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)

DECISION ID | 12783
Pollutant: | Unknown Toxicity
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Three lines of evidence are available in the administrative record to assess this pollutant. Four of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Two of 15 samples tested with selenastrum exceed the narrative toxicity objective and this exceeds the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12783

LOE ID: | 22134
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 15
Number of Exceedances: | 2
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Two of 15 samples tested with Selenastrum capricornutum were toxic and violated the narrative toxicity objective. Two samples collected at Jack Tone Road exhibited a statistically significant decrease in growth compared to the control. The sample date and percent of control (in parentheses) are as follows:24 August 2004 (55)21 March 2005 (85)
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 4-day chronic-style toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from Littlejohns Creek at Jack Tone Road.
Temporal Representation: | Samples were collected from August 2004 to September 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 22121
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 21
Number of Exceedances: | 1
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | One of the 21 samples tested with Ceriodaphnia dubia was toxic and violated the narrative toxicity objective. One sample collected at Littlejohns Creek at Newcastle Road exhibited a statistically significant decrease in growth compared to the control. The sample date and percent of control (in parentheses) are as follows: 02 September 2003 (0).
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 4-day acute-style toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from two locations on Littlejohns Creek: at Jack Tone Road and at Newcastle Road.
Temporal Representation: | Samples were collected from April 2003 to September 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):
LOE ID: | 22132
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Water
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 23
Number of Exceedances: | 1
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | One of the 23 samples tested with Pimephales promelas was toxic and violated the narrative toxicity objective. One sample collected at Littlejohns Creek at Jack Tone Road exhibited a statistically significant decrease in growth compared to the control. The sample date and percent of control (in parentheses) are as follows: 16 February 2005 (70).
Data Reference: | Revised Draft of the 2007 Review of the Monitoring Data for the Irrigated Lands Regulatory Conditional Waiver Program
| Monitoring and Reporting Program, Order Nos. R5-2003-0826, R5-2005-0833, and R5-2008-0005 for Coalition Groups Under Resolution No. R5-2003-0105, Conditional Waiver of Waste Discharge Requirements for Discharges From Irrigated Lands Within the Central Valley Region
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances (CVRWQCB, 2007).
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 4-day acute-style toxicity tests.
Guideline Reference:
Spatial Representation: | Samples were collected from two locations: Littlejohns Creek at Newcastle Road and at Jack Tone Road.
Temporal Representation: | Samples were collected from April 2003 to September 2006.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Monitoring was conducted in accordance with Central Valley Water Board Monitoring and Reporting Program (order number R5-2003-0826) requirements (CVRWQCB, 2003)
QAPP Information Reference(s):