# Final 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 5 - Central Valley Region

Water Body Name: | Mountain House Creek (from Altamont Pass to Old River, Alameda and San Joaquin Counties; partly in Delta Waterways, southern portion)
Water Body ID: | CAR5440000020080702173527
Water Body Type: | River & Stream

DECISION ID | 10201
Pollutant: | Arsenic
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 7 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 9 available concentrations exceeded the USEPA Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10201

LOE ID: | 21081
Pollutant: | Arsenic
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 9
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 9 samples collected by the Surface Water Ambient Monitoring Program exceeded the USEPA Primary MCL of 10 ug/L for total arsenic
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | Total arsenic levels must not exceed the USEPA Primary MCL of 10 ug/L
Objective/Criterion Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Mountain House Creek at Mountain House Parkway
Temporal Representation: | The samples were collected between June 26, 2001 and May 27, 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 8500
Pollutant: | Arsenic
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 7
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | None of the 7 samples collected by the Surface Water Ambient Monitoring Program exceeded the CTR criterion of 340 ug/L for dissolved arsenic
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | Dissolved arsenic levels should not exceed the CTR 1-hour average maximum concentration of 340 ug/L
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Mountain House Creek at Mountain House Parkway
Temporal Representation: | The samples were collected between June 26, 2001 and October 29, 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10202
Pollutant: | Boron
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 15 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. Table 3.1 of the listing policy recommends listing if a sample size of 15 has 2 or more samples that exceed the evaluation criteria. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10202

LOE ID: | 20462
Pollutant: | Boron
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 15
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 15 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective of 1,000 ug/L for boron
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Boron levels should not exceed 1,000 ug/L (Department of Health Services Health Advisory)
Guideline Reference: | Drinking Water Notification and Response Levels: An Overview
Spatial Representation: | Samples were collected from Mountain House Creek at Mountain House Parkway
Temporal Representation: | The samples were collected between December 27, 2000 and May 27, 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10203
Pollutant: | Cadmium
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 6 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 9 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10203

LOE ID: | 21083
Pollutant: | Cadmium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 9
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | None of the 9 samples collected by the Surface Water Ambient Monitoring Program exceeded the California Primary MCL of 5 ug/L for total cadmium
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | Total cadmium levels should not exceed the California Department of Public Health Primary MCL of 5 ug/L
Objective/Criterion Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Mountain House Creek at Mountain House Parkway
Temporal Representation: | The samples were collected between June 26, 2001 and May 27, 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 8502
Pollutant: | Cadmium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 6
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | None of the 6 samples collected by the Surface Water Ambient Monitoring Program exceeded the calculated CTR criterion for dissolved cadmium
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | Dissolved cadmium levels should not exceed the calculated limit based on the formula: Criteria Maximum Concentration (1-hour Average dissolved)=(EXP(1.128*LN(hardness)-3.6867))*(1.136672-(LN(hardness)*0.041838))
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Mountain House Creek at Mountain House Parkway
Temporal Representation: | The samples were collected between August 28, 2001 and October 29, 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10205
Pollutant: | Chromium (total)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 16 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10205

LOE ID: | 20430
Pollutant: | Chromium (total)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 16
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Zero of the 16 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Chromium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Chromium levels should not exceed 50 ug/L (Department of Public Health Primary MCL).
Guideline Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Spatial Representation: | Samples were collected at Mountain House Creek at Mountain House Parkway.
Temporal Representation: | The samples were collected from December 27 2000 to May 27 2003.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10206
Pollutant: | Copper
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 12 samples exceed the California Toxics Rule 4-day average criteria for dissolved Copper and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10206

LOE ID: | 8504
Pollutant: | Copper
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 12
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Zero of the 12 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Copper.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | California Toxics Rule 4-day average criteria for dissolved Copper.
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Mountain House Creek at Mountain House Parkway.
Temporal Representation: | The samples were collected from December 2000 to October 2002.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10207
Pollutant: | Escherichia coli (E. Coli)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.3 of the Listing Policy. Under section 3.3 a single line of evidence is necessary to assess listing status. One line of evidence are available in the administrative record to assess this pollutant. Two of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Two of 2 samples exceeded the USEPA E. Coli guideline for water contact and non-contact recreation and this sample size is insufficient to determine with the power and confidence of the Listing Policy if standards are not met. A minimum of 5 samples is needed for application of table 3.2. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10207

LOE ID: | 23142
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 2
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | The Central Valley Regional Water Quality Control Board Surface Water Ambient Monitoring Program collected 2 samples from July 2002 to July 2003. Two out of 2 samples exceeded the evaluation objective.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. The objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
| Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Evaluation Guideline: | The USEPA E. Coli objective of 235/100 mL in any single sample (USEPA 1986).
Guideline Reference: | Quality Criteria for Water 1986. United States Environmental Protection Agency. Office of Water. Regulations and Standards. Washington D.C. EPA 440/5-86-001.
Spatial Representation: | Samples were collected at Mountain House Creek.
Temporal Representation: | Sampling occurred from July 2002 to July 2003.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)
LOE ID: | 7551
Pollutant: | Escherichia coli (E. Coli)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Non-Contact Recreation
Number of Samples: | 2
Number of Exceedances: | 2
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Two of the 2 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for E.Coli Bacteria. The exceeded results are as follows: 7/31/2002 - a sample taken at Mountain House Creek at Mountain House Parkway had a result of 1046MPN. 7/29/2003 - a sample taken at Mountain House Creek at Mountain House Parkway had a result of 1203MPN.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | E.Coli Bacteria levels should not exceed 409 MPN/100 mL in any single sample (USEPA E.Coli Guideline)
Guideline Reference: | Ambient Water Quality Criteria for Bacteria - 1986. EPA440/5-84-002
Spatial Representation: | Samples were collected at Mountain House Creek at Mountain House Parkway.
Temporal Representation: | The samples were collected from Jul 31 2002 to Jul 29 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10208
Pollutant: | Lead
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 13 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 16 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10208

LOE ID: | 20508
Pollutant: | Lead
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 16
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Zero of the 16 samples collected by the Surface Water Ambient Monitoring Program exceeded the Primary MCL of 15 ug/L for total lead
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | Total lead levels should not exceed 15 ug/L (Department of Public Health Primary MCL)
Objective/Criterion Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Mountain House Creek at Mountain House Parkway
Temporal Representation: | The samples were collected between December 27, 2000 and May 27, 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 8508
Pollutant: | Lead
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 13 samples collected by the Surface Water Ambient Monitoring Program exceeded the calculated CTR CMC for dissolved lead
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | Dissolved lead levels should not exceed the calculated CTR value based on the formula: Criteria Maximum Concentration (1-hour Average, dissolved)=(EXP(1.273*LN(hardness)-1.46))*(1.46203-(LN(hardness)*0.145712))
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Mountain House Creek at Mountain House Parkway
Temporal Representation: | The samples were collected between December 27, 2000 and October 29, 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10210
Pollutant: | Nickel
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 13 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 16 available concentrations exceeded the Department of Public Health Primary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10210

LOE ID: | 20510
Pollutant: | Nickel
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 16
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Zero of the 16 samples collected by the Surface Water Ambient Monitoring Program exceeded the Primary MCL of 100 ug/L for total nickel
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | Total nickel levels should not exceed 100 ug/L (Department of Public Health Primary MCL)
Objective/Criterion Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Mountain House Creek at Mountain House Parkway
Temporal Representation: | The samples were collected between December 27, 2000 and May 27, 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 8513
Pollutant: | Nickel
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 13 samples collected by the Surface Water Ambient Monitoring Program exceeded the calculated CTR CMC for dissolved nickel
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | Dissolved nickel levels should not exceed the calculated CTR limit based on the formula: Criteria Maximum Concentration (1-hour Average, dissolved)=(EXP(0.846*LN(hardness)+2.255))*(0.998)
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Mountain House Creek at Mountain House Parkway
Temporal Representation: | The samples were collected between December 27, 2000, and October 29, 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10211
Pollutant: | Nitrate as Nitrate (NO3)
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 10 available concentrations exceeded the USEPA Primary MCL and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is based on staff findings that 0 of 10 available concentrations exceeded the USEPA National Ambient Water Quality Objective and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10211

LOE ID: | 20392
Pollutant: | Nitrate as Nitrate (NO3)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 10
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 10 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Nitrate-N.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Nitrate-N levels should not exceed 45 mg/L (Department of Public Health Primary MCL)
Guideline Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Spatial Representation: | Samples were collected at Mountain House Creek at Mountain House Parkway.
Temporal Representation: | The samples were collected from Dec 27 2000 to Sep 25 2001
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 8516
Pollutant: | Nitrate as Nitrate (NO3)
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 10
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 10 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation guideline for Nitrate-N.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Nitrate-N levels should not to exceed 100 mg/L (USEPA National Ambient Water Quality Objective)
Guideline Reference: | National Recommended Water Quality Criteria. United States Environmental Protection Agency. Office of Water. Office of Science and Technology. 4304T The Blue Book
Spatial Representation: | Samples were collected at Mountain House Creek at Mountain House Parkway.
Temporal Representation: | The samples were collected from Dec 27 2000 to Sep 25 2001
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 9150
Pollutant: | Oxygen, Dissolved
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 1 of 12 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.2 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met. "
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9150

LOE ID: | 8505
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 12
Number of Exceedances: | 1
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | One of the 12 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Dissolved Oxygen. The exceeded results are as follows: 6/26/2001 - a sample taken at Mountain House Creek at Mountain House Parkway had a result of 2.9mg/L.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | The Basin Plan Objective sets the minimum Dissolved Oxygen content at 7 mg/L
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Mountain House Creek at Mountain House Parkway.
Temporal Representation: | The samples were collected from Jun 26 2001 to Jul 29 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 13714
Pollutant: | Sediment Toxicity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.6 of the Listing Policy. Under section 3.6 one line(s) of evidence are necessary to assess listing status. One lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 1 samples exceeded the narrative toxicity objective and this sample size is insufficient to determine with the power and confidence of the Listing Policy if standards are not met. A minimum of 2 samples is needed for application of table 3.1. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because it cannot be determined if applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 13714

LOE ID: | 23143
Pollutant: | Toxicity
LOE Subgroup: | Toxicity
Matrix: | Sediment
Fraction: | Total
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | TOXICITY TESTING
Data Used to Assess Water Quality: | Only one sample tested with Hyalella azteca survival.
Data Reference: | Monitoring Data from the Surface Water Ambient Monitoring Program (SWAMP), San Joaquin River Basin - 2007 Data Review
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CVRWQCB, 2007)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Statistically significant difference from control using a t-test with 10-day Hyalella azteca sediment toxicity tests.
Guideline Reference: | Methods for Measuring the Toxicity and Bioaccumulation of Sediment-associated Contaminants with Freshwater Invertebrates, Second Edition. U.S. Environmental Protection Agency Office of Research and Development, Duluth, MI , U.S. Environmental Protection Agency Office of Water, Washington, DC EPA-600/R-99/064
Spatial Representation: | Sample was collected from Mountain House Creek at Byron Road.
Temporal Representation: | Sample was collected on September 24, 2002.
Environmental Conditions: |
QAPP Information: | Data quality: Fair. Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s): | Quality Assurance Management Plan for the State of California's Surface Water Ambient Monitoring Program. Sacramento, CA. State Water Resources Control Board. SWAMP. December 2002 (1st version)

DECISION ID | 10212
Pollutant: | Selenium
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that only 1 sample is available and a minimum of 2 samples is needed for evaluation under section 3.1 for the Municipal Beneficial Use and for the Cold Water Habitat. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because it cannot be determined if applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10212

LOE ID: | 8519
Pollutant: | Selenium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 1 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Selenium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006) Selenium levels should not to exceed 5 ug/L (CTR)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Mountain House Creek at Mountain House Parkway.
Temporal Representation: | The samples were collected from Oct 29 2002 to Oct 29 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 20284
Pollutant: | Selenium
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 0 of the 1 sample collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Selenium.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Selenium levels should not exceed 50 ug/L (Department of Public Health Primary MCL)
Guideline Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Spatial Representation: | The sample was collected at Mountain House Creek at Mountain House Parkway.
Temporal Representation: | The sample was collected on Oct 29 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10215
Pollutant: | Zinc
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | "This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 2 lines of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 0 of 13 available concentrations exceeded the California Toxics Rule for Cold Freshwater Habitat and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The recommendation is also based on staff findings that 0 of 16 available concentrations exceeded the Department of Public Health Secondary MCL for Municipal & Domestic Supply and this does not exceed the allowable frequency using Table 3.1 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met."
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10215

LOE ID: | 20459
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 14
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Zero of the 14 samples collected by the Surface Water Ambient Monitoring Program exceeded the Secondary MCL for total zinc
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | Total zinc levels should not exceed 5,000 ug/L (Department of Public Health Secondary MCL)
Objective/Criterion Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Mountain House Creek at Mountain House Parkway
Temporal Representation: | The samples were collected between December 27, 2000 and May 27, 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 8521
Pollutant: | Zinc
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 13
Number of Exceedances: | 0
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | Zero of the 13 samples collected by the Surface Water Ambient Monitoring Program exceeded the calculated CTR CMC for dissolved zinc
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | Dissolved zinc levels should not exceed the calculated CTR limit based on the formula: Criteria Maximum Concentration=EXP((0.8473*LN(hardness))+0.884)*(0.978)
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Mountain House Creek at Mountain House Parkway
Temporal Representation: | The samples were collected between December 27, 2000 and October 29, 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 9147
Pollutant: | pH
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is not sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 1 of 21 available concentrations exceeded the water quality objective and this does not exceed the allowable frequency using Table 3.2 of the Listing Policy. Table 3.2 of the listing policy recommends listing if a sample size of 21 has 5 or more samples that exceed the evaluation criteria. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 9147

LOE ID: | 8523
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 21
Number of Exceedances: | 1
Data and Information Type: | Not Specified
Data Used to Assess Water Quality: | One of the 21 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for pH. The exceeded results are as follows: 7/31/2002 - a sample taken at Mountain House Creek at Mountain House Parkway had a result of 8.8none.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | pH levels should not be lower than 6.5 or higher than 8.5 (Basin Plan Objective)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected at Mountain House Creek at Mountain House Parkway.
Temporal Representation: | The samples were collected from Dec 27 2000 to Jul 29 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 15957
Pollutant: | Chloride
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that 5 of 15 available concentrations exceeded the water quality objective and this does exceed the allowable frequency using Table 3.1 of the Listing Policy. Table 3.1 of the listing policy recommends listing if a sample size of 15 has 2 or more samples that exceed the evaluation criteria. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 15957

LOE ID: | 21092
Pollutant: | Chloride
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 15
Number of Exceedances: | 5
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Five of the 15 samples collected by the Surface Water Ambient Monitoring Program exceeded the evaluation objective for Chloride.
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | All waters shall be maintained free of toxic substances in concentrations that produce detrimental physiological responses in human, plant, animal, or aquatic life. This objective applies regardless of whether the toxicity is caused by a single substance or the interactive effect of multiple substances. (CRWQCB, 2006)
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: | Chloride levels should not exceed 250 mg/L (Department of Public Health Secondary MCL).
Guideline Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Spatial Representation: | Samples were collected at Mountain House Creek at Mountain House Parkway.
Temporal Representation: | The samples were collected from December 27 2000 to May 27 2003.
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):

DECISION ID | 10214
Pollutant: | Salinity
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for listing under sections 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Data is available from 1 line of evidence for this pollutant. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification for placing this water segment-pollution combination on the section 303(d) list. The recommendation is based on staff findings that: 5 of 21 available specific conductivity measurments exceeded the water quality objective and this does exceed the allowable frequency using Table 3.2 of the Listing Policy. Five of 9 available total dissolved solids concentrations exceeded the water quality objective and this does exceed the allowable frequency using Table 3.2 of the Listing Policy. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 10214

LOE ID: | 21103
Pollutant: | Specific Conductivity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 21
Number of Exceedances: | 5
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Eight of the 21 samples collected by the Surface Water Ambient Monitoring Program exceeded the "recommended" Secondary MCL of 900 uS/cm for electrical conductivity
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | The secondary MCLs for electrical conductivity provide a range of values including a "recommended" level (900 uS/cm), upper level (1600 uS/cm) and a short-term level (2200 uS/cm). The recommended concentration was used as it is intended to be protective of all drinking water uses
Objective/Criterion Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Mountain House Creek at Mountain House Parkway
Temporal Representation: | The samples were collected between December 27, 2000 and July 29, 2003
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):
LOE ID: | 20961
Pollutant: | Total Dissolved Solids
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 9
Number of Exceedances: | 5
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | Five of the 9 samples collected by the Surface Water Ambient Monitoring Program exceeded the "recommended" Secondary MCL of 500 mg/L for Total Dissolved Solids
Data Reference: | San Joaquin River SWAMP Monitoring Data - Drainage Basin Inflows
Water Quality Objective/Criterion: | The secondary MCLs for Total Dissolved Solids provide a range of values including a recommended level (500 mg/L), upper level (1000 mg/L) and a short-term level (1500 mg/L). The recommended concentration was used as it is intended to be protective of all drinking water uses
Objective/Criterion Reference: | California Code of Regulations, Title 22, Division 4, Chapter 15. Domestic Water Quality and Monitoring. http://www.cdph.ca.gov/certlic/drinkingwater/Pages/Lawbook.aspx
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Mountain House Creek at Mountain House Parkway
Temporal Representation: | The samples were collected between December 27, 2000 and October 29, 2002
Environmental Conditions: |
QAPP Information: | Monitoring was conducted in accordance with the State Water Resources Control Board's Quality Assurance Program Plan for the State of California's Surface Water Ambient Monitoring Program.
QAPP Information Reference(s):