# Final 2008 California 303(d)/305(b) Integrated Report

# Supporting Information

## Regional Board 5 - Central Valley Region

Water Body Name: | Honcut Creek (Butte and Yuba Counties)
Water Body ID: | CAR5154000020080707105944
Water Body Type: | River & Stream

DECISION ID | 12893
Pollutant: | Copper
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. Two of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Two of 29 samples exceed the 4-day maximum criterion for dissolved copper and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12893

LOE ID: | 22281
Pollutant: | Copper
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 29
Number of Exceedances: | 2
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 29 samples were taken from Honcut Creek between March 2002 and April 2004. Two of the 29 samples exceed guidelines for dissolved copper.
Data Reference: | Project effects on water quality designated beneficial uses for surface waters, and results for bacterial monitoring of swimming areas in 2003. FERC Project No. 2100. Sacramento, CA: State of CA Department of Water Resources
Water Quality Objective/Criterion: | California Toxics Rule Criteria (USEPA) - Freshwater Aquatic Life ProtectionContinuous Concentration (4-day Average) calculated based on the fallowing formula (e{.8545xLN[hardness]}-1.702) x(0.960) which incorporates hardnessU.S. Environmental Protection Agency, Federal Register, Volume 65, No. 97 (Thursday, 18 May 2000), pp. 31682-31719 [California Toxics Rule]; and Federal Register, Volume 66, No. 30 (Tuesday, 13 February 2001), pp. 9960-9962 [California Toxics Rule Correction] http://www.gpoaccess.gov/fr/browse.html.
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
| Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Honcut Creek above Pacific Ranch Near Palermo.
Temporal Representation: | Samples were collected between March 2002 and April 2004.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Quality Control for all of the elements described in section 6.1.4 of the Policy was conducted in accordance with the Laboratory QAPP developed by the State of California Resources Agency Department of Water Resources (DWR, 2005). Quality Assurance Project Plan for Oroville Facilities Relicensing FERC Project No. 2100 SP-W1. Department of Water Resources (DWR). Oroville Facilities Relicensing FERC Project No. 2100. January 2005.
QAPP Information Reference(s):

DECISION ID | 14504
Pollutant: | Fecal Coliform
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 23 calculated geometric means exceeded the fecal coliform objective and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. According to table 3.2, a minimum sample size of 26 is required to designate a fully supporting use rating. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 14504

LOE ID: | 22279
Pollutant: | Fecal Coliform
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Water Contact Recreation
Number of Samples: | 23
Number of Exceedances: | 0
Data and Information Type: | PATHOGEN MONITORING
Data Used to Assess Water Quality: | The Department of Water Resources collected 26 samples from March 2002 to April 2004. The geometric mean per month per site was calculated from the samples and 0 out of the 23 calculated geometric means exceeded the evaluation objective.
Data Reference: | Project effects on water quality designated beneficial uses for surface waters, and results for bacterial monitoring of swimming areas in 2003. FERC Project No. 2100. Sacramento, CA: State of CA Department of Water Resources
Water Quality Objective/Criterion: | In waters designated for contact recreation (REC-1), the fecal coliform concentration based on a minimum of not less than five samples for any 30-day period shall not exceed a geometric mean of 200/100 ml, nor shall more than ten percent of the total number of samples taken during any 30-day period exceed 400/100 ml.
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Honcut Creek at Pacific Ranch near Palermo.
Temporal Representation: | Sampling occurred from March 2002 to April 2004.
Environmental Conditions: |
QAPP Information: | Data quality: Good. Quality Control for all of the elements described in section 6.1.4 of the Policy was conducted in accordance with the Laboratory QAPP developed by the State of California Resources Agency Department of Water Resources (DWR, 2005). Quality Assurance Project Plan for Oroville Facilities Relicensing FERC Project No. 2100 SP-W1. Department of Water Resources (DWR). Oroville Facilities Relicensing FERC Project No. 2100. January 2005.
QAPP Information Reference(s):

DECISION ID | 14503
Pollutant: | Lead
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess this pollutant. None of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. None of 29 samples exceeded the Basin Plan criteria and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should not be placed on the section 303(d) list because applicable water quality standards are not being exceeded.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 14503

LOE ID: | 22260
Pollutant: | Lead
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Warm Freshwater Habitat
Aquatic Life Use: | Warm Freshwater Habitat
Number of Samples: | 29
Number of Exceedances: | 0
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 29 samples were taken from Honcut Creek between 2002 and 2004. 0 of the 29 samples exceed guidelines for dissolved lead.
Data Reference: | Project effects on water quality designated beneficial uses for surface waters, and results for bacterial monitoring of swimming areas in 2003. FERC Project No. 2100. Sacramento, CA: State of CA Department of Water Resources
Water Quality Objective/Criterion: | California Toxics Rule Criteria (USEPA) - Freshwater Aquatic Life ProtectionContinuous Concentration (4-day Average) calculated based on the following formula: (e(1.273xLN(hardness))-4.705)x((1.46203-LN(hardness))x0.145712)U.S. Environmental Protection Agency, Federal Register, Volume 65, No. 97 (Thursday, 18 May 2000), pp. 31682-31719 [California Toxics Rule]; and Federal Register, Volume 66, No. 30 (Tuesday, 13 February 2001), pp. 9960-9962 [California Toxics Rule Correction] http://www.gpoaccess.gov/fr/browse.html.
Objective/Criterion Reference: | Water Quality Standards 2000. Establishment of numeric criteria for priority toxic pollutants for the State of California: Rules and regulations. Federal Register Vol. 65, No. 97. Washington, D.C.: Environmental Protection Agency
| Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Honcut Creek at Pacific Ranch near Palermo.
Temporal Representation: | Samples were collected from March 2002 through April 2004. Samples were collected at monthly intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Excellent. Quality Control for all of the elements described in section 6.1.4 of the Policy was conducted in accordance with the Laboratory QAPP developed by the State of California Resources Agency Department of Water Resources (DWR, 2005). Quality Assurance Project Plan for Oroville Facilities Relicensing FERC Project No. 2100 SP-W1. Department of Water Resources (DWR). Oroville Facilities Relicensing FERC Project No. 2100. January 2005.
QAPP Information Reference(s):

DECISION ID | 12892
Pollutant: | Oxygen, Dissolved
Final Listing Decision: | List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | New Decision
Revision Status | Revised
Sources: | Source Unknown
Expected TMDL Completion Date: | 2021
Impairment from Pollutant or Pollution: | Pollutant
Weight of Evidence: | This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. One lines of evidence are available in the administrative record to assess this pollutant. Ten of the samples exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification in favor of placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used satisfies the data quality requirements of section 6.1.4 of the Policy. 2. The data used satisfies the data quantity requirements of section 6.1.5 of the Policy. 3. Ten of 28 samples exceed the minimum criterion for COLD (7 mg/L) and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. In addition, 4 of 28 samples exceed the minimum criterion for WARM (5 mg/L) and this exceeds the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
RWQCB Board Decision / Staff Recommendation: | After review of the available data and information, RWQCB staff concludes that the water body-pollutant combination should be placed on the section 303(d) list because applicable water quality standards are exceeded and a pollutant contributes to or causes the problem.
SWRCB Board Decision / Staff Recommendation: |
USEPA Decision: |

Lines of Evidence (LOEs) for Decision ID 12892

LOE ID: | 22262
Pollutant: | Oxygen, Dissolved
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Total
Beneficial Use: | Cold Freshwater Habitat
Aquatic Life Use: | Cold Freshwater Habitat
Number of Samples: | 28
Number of Exceedances: | 10
Data and Information Type: | PHYSICAL/CHEMICAL MONITORING
Data Used to Assess Water Quality: | 28 samples were taken from Honcut Creek between March 2002 and April 2004. 10 samples exceed the minimum dissolved oxygen concentration (7 mg/L), and 4 samples exceeds 5 mg/L.
Data Reference: | Oroville Facilities Relicensing-FERC Project No. 2100. Contaminant accumulation in fish, sediments, and the aquatic food chain. Sacramento, CA: State of CA Department of Water Resources
Water Quality Objective/Criterion: | Sacramento/San Joaquin River Basin Plan (CVRWQCB, 2007a)(COLD), Minimum Dissolved Oxygen concentration of 7mg/L(SPWN), Minimum Dissolved Oxygen concentration of 7mg/L(WARM), Minimum Dissolved Oxygen concentration of 5mg/L
Objective/Criterion Reference: | Central Valley Regional Water Quality Control Board. Water Quality Control Plan (Basin Plan) for the California Regional Water Quality Control Board - Central Valley Region
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | Samples were collected from Honcut Creek at Pacific Ranch near Palermo.
Temporal Representation: | Samples were collected between March 2002 and April 2004 at weekly or monthly intervals.
Environmental Conditions: |
QAPP Information: | Data quality: Good?. Quality Control for all of the elements described in section 6.1.4 of the Policy was conducted in accordance with the Laboratory QAPP developed by the State of California Resources Agency Department of Water Resources (DWR, 2005). Quality Assurance Project Plan for Oroville Facilities Relicensing FERC Project No. 2100 SP-W1. Department of Water Resources (DWR). Oroville Facilities Relicensing FERC Project No. 2100. January 2005.
QAPP Information Reference(s):