# Draft California 2012 Integrated Report( 303(d) List/305(b) Report)

# Supporting Information

## Regional Board 6 - Lahontan Region

Water Body Name: | Red Rock Creek
Water Body ID: | CAR6380007020080811103007
Water Body Type: | River & Stream

DECISION ID | 26061 | Region 6
Red Rock Creek

Pollutant: | Nitrate
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)(2010)
Revision Status | Original
Impairment from Pollutant or Pollution: | Pollutant
Regional Board Staff Conclusion: | Regional Board Conclusion: This pollutant was considered for placement on the section 303(d) list in a previous assessment cycle. No new information was reviewed for this current assessment cycle. Therefore, the previous conclusion remains unchanged, and is as follows: This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. The single sample did not exceed the California Maximum Contaminant Level. No biological data are available to assess whether it exceeded the water quality objective for biostimulatory substances. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used do not satisfy the data quality requirements of section 6.1.4 of the Policy. 2. The data used do not satisfy the data quantity requirements of section 6.1.5 or Table 3.1 of the Policy. 3. The single sample did not exceed the Maximum Contaminant Level and this does not exceed the allowable frequency listed in Table 3.1 of the Listing Policy. No biological data are available to assess compliance with the objective for biostimulatory substances. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
Regional Board Staff Decision Recommendation: | No new data were assessed for this assessment cycle. The conclusion reached in the previous cycle remains in same. The Regional Board will update this decision when new data and information become available in a future assessment cycle.

Line of Evidence (LOE) for Decision ID 26061, Nitrate | Region 6
Red Rock Creek
LOE ID: | 25873
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | Fixed station physical/chemical (conventional plus toxic pollutants)
Data Used to Assess Water Quality: | The U.S. Bureau of Land Management sampled this station on August 5, 2002. The concentration of NO3-N in one sample was 0.31 mg/L.
Data Reference: | Water quality data for surface waters on U.S Bureau of Land Management lands in Lassen and Modoc Counties
SWAMP Data: | Non-SWAMP
Water Quality Objective/Criterion: | The Lahontan Basin Plan does not include site specific objectives for this water body. The regionwide narrative objective for biostimulatory substances states: "Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect the water for beneficial uses."
Objective/Criterion Reference: | Water Quality Control Plan for the Lahontan Region (as amended)
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | One station, Red Rock Creek below spillway, was sampled.
Temporal Representation: | One sample was collected on August 5, 2002.
Environmental Conditions: | Red Rock Creek is located in the Madeline Plains Hydrologic Unit (HU No. 638.00) in Lassen County. No site-specific water quality objectives have been established for the waters of this watershed. The sampling station was below the spillway from Dodge Reservoir (called Doge in the USBLM database).
QAPP Information: | No quality assurance information was submitted with the data.
QAPP Information Reference(s):
Line of Evidence (LOE) for Decision ID 26061, Nitrate | Region 6
Red Rock Creek
LOE ID: | 25875
Pollutant: | Nitrate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | Fixed station physical/chemical (conventional plus toxic pollutants)
Data Used to Assess Water Quality: | The U.S. Bureau of Land Management sampled this station on August 5, 2002. The concentration of NO3-N in one sample was 0.31 mg/L. The MCL was not exceeded.
Data Reference: | Water quality data for surface waters on U.S Bureau of Land Management lands in Lassen and Modoc Counties
SWAMP Data: | Non-SWAMP
Water Quality Objective/Criterion: | California Maximum Contaminant Levels (MCLs) apply to ambient waters under the Lahontan Basin Plan's "Chemical Constituents" objective. The MCL for nitrate is 45 mg/L expressed "as nitrate," equivalent to 10 mg/L expressed "as N."
Objective/Criterion Reference: | Water Quality Control Plan for the Lahontan Region (as amended)
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | One station, Red Rock Creek below spillway, was sampled.
Temporal Representation: | One sample was collected on August 5, 2002.
Environmental Conditions: | Red Rock Creek is located in the Madeline Plains Hydrologic Unit (HU No. 638.00) in Lassen County. No site-specific water quality objectives have been established for the waters of this watershed. The sampling station was below the spillway from Dodge Reservoir (called Doge in the USBLM database).
QAPP Information: | No quality assurance information was submitted with the data.
QAPP Information Reference(s):

DECISION ID | 25946 | Region 6
Red Rock Creek

Pollutant: | Phosphate
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)(2010)
Revision Status | Original
Impairment from Pollutant or Pollution: | Pollutant
Regional Board Staff Conclusion: | Regional Board Conclusion: This pollutant was considered for placement on the section 303(d) list in a previous assessment cycle. No new information was reviewed for this current assessment cycle. Therefore, the previous conclusion remains unchanged, and is as follows: This pollutant is being considered for placement on the section 303(d) list under section 3.1 of the Listing Policy. Under section 3.1 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. No biological data are available to assess whether the single sample exceeded the water quality objective for biostimulatory substances. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used do not satisfy the data quality requirements of section 6.1.4 of the Policy. 2. The data used do not satisfy the data quantity requirements of section 6.1.5 or Table 3.1 of the Policy. 3. No biological data are available to assess compliance with the water quality objective for biostimulatory substances. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
Regional Board Staff Decision Recommendation: | No new data were assessed for this assessment cycle. The conclusion reached in the previous cycle remains in same. The Regional Board will update this decision when new data and information become available in a future assessment cycle.

Line of Evidence (LOE) for Decision ID 25946, Phosphate | Region 6
Red Rock Creek
LOE ID: | 25874
Pollutant: | Phosphate
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | Dissolved
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | Fixed station physical/chemical (conventional plus toxic pollutants)
Data Used to Assess Water Quality: | The U.S. Bureau of Land Management sampled this station on August 5, 2002. The concentration of PO4-P in one sample was 1.04 mg/L..
Data Reference: | Water quality data for surface waters on U.S Bureau of Land Management lands in Lassen and Modoc Counties
SWAMP Data: | Non-SWAMP
Water Quality Objective/Criterion: | The Lahontan Basin Plan does not include site specific objectives for this water body. The regionwide narrative objective for biostimulatory substances states: "Waters shall not contain biostimulatory substances in concentrations that promote aquatic growths to the extent that such growths cause nuisance or adversely affect the water for beneficial uses."
Objective/Criterion Reference: | Water Quality Control Plan for the Lahontan Region (as amended)
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | One station, Red Rock Creek below spillway, was sampled.
Temporal Representation: | One sample was collected on August 5, 2002.
Environmental Conditions: | Red Rock Creek is located in the Madeline Plains Hydrologic Unit (HU No. 638.00) in Lassen County. No site-specific water quality objectives have been established for the waters of this watershed. The sampling station was below the spillway from Dodge Reservoir (called Doge in the USBLM database).
QAPP Information: | No quality assurance information was submitted with the data.
QAPP Information Reference(s):

DECISION ID | 25875 | Region 6
Red Rock Creek

Pollutant: | Sediment
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)(2010)
Revision Status | Original
Impairment from Pollutant or Pollution: | Pollutant
Regional Board Staff Conclusion: | Regional Board Conclusion: This pollutant was considered for placement on the section 303(d) list in a previous assessment cycle. No new information was reviewed for this current assessment cycle. Therefore, the previous conclusion remains unchanged, and is as follows: One line of evidence is available in the administrative record to assess this pollutant. The Lahontan Basin Plan's objective for sediment is antidegradation-based and the available data are insufficient to document baseline and trend conditions as required by section 3.10 of the Listing Policy. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used do not satisfy the data quality requirements of section 6.1.4 of the Policy. 2. The data used do not satisfy the data quantity requirements of section 6.1.5 of the Policy. 3. The single sample is insufficient to determine compliance with the objective under section 3.10 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
Regional Board Staff Decision Recommendation: | No new data were assessed for this assessment cycle. The conclusion reached in the previous cycle remains in same. The Regional Board will update this decision when new data and information become available in a future assessment cycle.

Line of Evidence (LOE) for Decision ID 25875, Sediment | Region 6
Red Rock Creek
LOE ID: | 25878
Pollutant: | Sediment
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | Fixed station physical/chemical (conventional plus toxic pollutants)
Data Used to Assess Water Quality: | The U.S. Bureau of Land Management sampled this station on August 5, 2002. The concentration of suspended sediment in one sample was 7.2 mg/L.
Data Reference: | Water quality data for surface waters on U.S Bureau of Land Management lands in Lassen and Modoc Counties
SWAMP Data: | Non-SWAMP
Water Quality Objective/Criterion: | The Lahontan Basin Plan's narrative objective states: "The suspended sediment load and suspended sediment discharge rate of surface waters shall not be altered in such a manner as to cause nuisance or adversely affect the water for beneficial uses."
Objective/Criterion Reference: | Water Quality Control Plan for the Lahontan Region (as amended)
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | One station, Red Rock Creek below spillway, was sampled.
Temporal Representation: | One sample was collected on August 5, 2002.
Environmental Conditions: | Red Rock Creek is located in the Madeline Plains Hydrologic Unit (HU No. 638.00) in Lassen County. No site-specific water quality objectives have been established for the waters of this watershed. The sampling station was below the spillway from Dodge Reservoir (called Doge in the USBLM database).
QAPP Information: | No quality assurance information was submitted with the data.
QAPP Information Reference(s):

DECISION ID | 25888 | Region 6
Red Rock Creek

Pollutant: | Specific Conductance
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)(2010)
Revision Status | Original
Impairment from Pollutant or Pollution: | Pollutant
Regional Board Staff Conclusion: | Regional Board Conclusion: This pollutant was considered for placement on the section 303(d) list in a previous assessment cycle. No new information was reviewed for this current assessment cycle. Therefore, the previous conclusion remains unchanged, and is as follows: This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. One line of evidence is available in the administrative record to assess this pollutant. The single sample does not exceed the water quality objective. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used do not satisfy the data quality requirements of section 6.1.4 of the Policy. 2. The data used do not satisfy the data quantity requirements of section 6.1.5 or Table 3.2 of the Policy. 3. The single sample did not exceed the water quality objective and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
Regional Board Staff Decision Recommendation: | No new data were assessed for this assessment cycle. The conclusion reached in the previous cycle remains in same. The Regional Board will update this decision when new data and information become available in a future assessment cycle.

Line of Evidence (LOE) for Decision ID 25888, Specific Conductance | Region 6
Red Rock Creek
LOE ID: | 25871
Pollutant: | Specific Conductance
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | Fixed station physical/chemical (conventional plus toxic pollutants)
Data Used to Assess Water Quality: | The U.S. Bureau of Land Management sampled this station on August 5, 2002. One specific conductance measurement was 205 uS/cm. The MCL was not exceeded.
Data Reference: | Water quality data for surface waters on U.S Bureau of Land Management lands in Lassen and Modoc Counties
SWAMP Data: | Non-SWAMP
Water Quality Objective/Criterion: | California Maximum Contaminant Levels (MCLs) apply to ambient waters under the Lahontan Basin Plan's "Chemical Constituents" objective. The MCL for specific conductance is 900 microsiemens per centimeter (uS/cm).
Objective/Criterion Reference: | Water Quality Control Plan for the Lahontan Region (as amended)
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | One station, Red Rock Creek below spillway, was sampled.
Temporal Representation: | One sample was collected on August 5, 2002.
Environmental Conditions: | Red Rock Creek is located in the Madeline Plains Hydrologic Unit (HU No. 638.00) in Lassen County. No site-specific water quality objectives have been established for the waters of this watershed. The sampling station was below the spillway from Dodge Reservoir (called Doge in the USBLM database).
QAPP Information: | No quality assurance information was submitted with the data.
QAPP Information Reference(s):

DECISION ID | 25889 | Region 6
Red Rock Creek

Pollutant: | Turbidity
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)(2010)
Revision Status | Original
Impairment from Pollutant or Pollution: | Pollutant
Regional Board Staff Conclusion: | Regional Board Conclusion: This pollutant was considered for placement on the section 303(d) list in a previous assessment cycle. No new information was reviewed for this current assessment cycle. Therefore, the previous conclusion remains unchanged, and is as follows: This pollutant is being considered for placement on the section 303(d) list under section 3.2 of the Listing Policy. Under section 3.2 a single line of evidence is necessary to assess listing status. Two lines of evidence are available in the administrative record to assess this pollutant. The single sample does not exceed the California Maximum Contaminant Level. The narrative turbidity objective is antidegradation-based and the single sample is insufficient to assess compliance with it under Section 3.10 of the Listing Policy. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used do not satisfy the data quality requirements of section 6.1.4 of the Policy. 2. The data used do not satisfy the data quantity requirements of section 6.1.5 or Table 3.2 of the Policy. 3. The single sample did not exceed the Maximum Contaminant Level and this does not exceed the allowable frequency listed in Table 3.2 of the Listing Policy. The single sample is insufficient to meet the requirements of section 3.10 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
Regional Board Staff Decision Recommendation: | No new data were assessed for this assessment cycle. The conclusion reached in the previous cycle remains the same. The Regional Board will update this decision when new data and information become available in a future assessment cycle.

Line of Evidence (LOE) for Decision ID 25889, Turbidity | Region 6
Red Rock Creek
LOE ID: | 25876
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | Fixed station physical/chemical (conventional plus toxic pollutants)
Data Used to Assess Water Quality: | The U.S. Bureau of Land Management sampled this station on August 5, 2002. The turbidity in one sample was 17.2 NTU.
Data Reference: | Water quality data for surface waters on U.S Bureau of Land Management lands in Lassen and Modoc Counties
SWAMP Data: | Non-SWAMP
Water Quality Objective/Criterion: | The Lahontan Basin Plan's regionwide turbidity objective states: "Waters shall be free of changes in turbidity that cause nuisance or adversely affect the water for beneficial uses. Increases in turbidity shall not exceed natural levels by more than 10 percent."
Objective/Criterion Reference: | Water Quality Control Plan for the Lahontan Region (as amended)
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | One station, Red Rock Creek below spillway, was sampled.
Temporal Representation: | One sample was collected on August 5, 2002.
Environmental Conditions: | Red Rock Creek is located in the Madeline Plains Hydrologic Unit (HU No. 638.00) in Lassen County. No site-specific water quality objectives have been established for the waters of this watershed. The sampling station was below the spillway from Dodge Reservoir (called Doge in the USBLM database).
QAPP Information: | No quality assurance information was submitted with the data.
QAPP Information Reference(s):
Line of Evidence (LOE) for Decision ID 25889, Turbidity | Region 6
Red Rock Creek
LOE ID: | 25877
Pollutant: | Turbidity
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Municipal & Domestic Supply
Number of Samples: | 1
Number of Exceedances: | 1
Data and Information Type: | Fixed station physical/chemical (conventional plus toxic pollutants)
Data Used to Assess Water Quality: | The U.S. Bureau of Land Management sampled this station on August 5, 2002. The turbidity in one sample was 17.2 NTU, exceeding the MCL.
Data Reference: | Water quality data for surface waters on U.S Bureau of Land Management lands in Lassen and Modoc Counties
SWAMP Data: | Non-SWAMP
Water Quality Objective/Criterion: | California Maximum Contaminant Levels (MCLs) apply to ambient waters under the Lahontan Basin Plan's "Chemical Constituents" objective. The MCL for turbidity is 5 NTU.
Objective/Criterion Reference: | Water Quality Control Plan for the Lahontan Region (as amended)
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | One station, Red Rock Creek below spillway, was sampled.
Temporal Representation: | One sample was collected on August 5, 2002.
Environmental Conditions: | Red Rock Creek is located in the Madeline Plains Hydrologic Unit (HU No. 638.00) in Lassen County. No site-specific water quality objectives have been established for the waters of this watershed. The sampling station was below the spillway from Dodge Reservoir (called Doge in the USBLM database).
QAPP Information: | No quality assurance information was submitted with the data.
QAPP Information Reference(s):

DECISION ID | 25887 | Region 6
Red Rock Creek

Pollutant: | pH
Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)
Last Listing Cycle's Final Listing Decision: | Do Not List on 303(d) list (TMDL required list)(2010)
Revision Status | Original
Impairment from Pollutant or Pollution: | Pollutant
Regional Board Staff Conclusion: | Regional Board Conclusion: This pollutant was considered for placement on the section 303(d) list in a previous assessment cycle. No new information was reviewed for this current assessment cycle. Therefore, the previous conclusion remains unchanged, and is as follows: One line of evidence is available in the administrative record to assess this pollutant. The Lahontan Basin Plan's objective for pH is antidegradation-based and the available data are insufficient to document baseline and trend conditions as required by section 3.10 of the Listing Policy. Based on the readily available data and information, the weight of evidence indicates that there is sufficient justification against placing this water segment-pollutant combination on the section 303(d) list in the Water Quality Limited Segments category. This conclusion is based on the staff findings that: 1. The data used do not satisfy the data quality requirements of section 6.1.4 of the Policy. 2. The data used do not satisfy the data quantity requirements of section 6.1.5 of the Policy. 3. The single sample is insufficient to determine compliance with the objective under section 3.10 of the Listing Policy. 4. Pursuant to section 3.11 of the Listing Policy, no additional data and information are available indicating that standards are not met.
Regional Board Staff Decision Recommendation: | No new data were assessed for this assessment cycle. The conclusion reached in the previous cycle remains in same. The Regional Board will update this decision when new data and information become available in a future assessment cycle.

Line of Evidence (LOE) for Decision ID 25887, pH | Region 6
Red Rock Creek
LOE ID: | 25872
Pollutant: | pH
LOE Subgroup: | Pollutant-Water
Matrix: | Water
Fraction: | None
Beneficial Use: | Cold Freshwater Habitat
Number of Samples: | 1
Number of Exceedances: | 0
Data and Information Type: | Fixed station physical/chemical (conventional plus toxic pollutants)
Data Used to Assess Water Quality: | The U.S. Bureau of Land Management sampled this station on August 5, 2002. One pH measurement was 8.8 units.
Data Reference: | Water quality data for surface waters on U.S Bureau of Land Management lands in Lassen and Modoc Counties
SWAMP Data: | Non-SWAMP
Water Quality Objective/Criterion: | The Lahontan Basin Plan's objective for pH states: "In fresh waters with designated beneficial uses of COLD or WARM, changes in normal ambient pH levels shall not exceed 0.5 pH units. For all other waters of the region, the pH shall not be depressed below 6.5 nor raised above 8.5 units. The Regional Board recognizes that some waters of the Region may have natural pH levels outside of the 6.5 to 8.5 range. Compliance with the pH objective for these waters will be determined on a case-by-case basis."
Objective/Criterion Reference: | Water Quality Control Plan for the Lahontan Region (as amended)
Evaluation Guideline: |
Guideline Reference:
Spatial Representation: | One station, Red Rock Creek below spillway, was sampled.
Temporal Representation: | One sample was collected on August 5, 2002.
Environmental Conditions: | Red Rock Creek is located in the Madeline Plains Hydrologic Unit (HU No. 638.00) in Lassen County. No site-specific water quality objectives have been established for the waters of this watershed. The sampling station was below the spillway from Dodge Reservoir (called Doge in the USBLM database).
QAPP Information: | No quality assurance information was submitted with the data.
QAPP Information Reference(s):